{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":23,"n_cols":76,"rows_kept":23,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["81","4.15.30.1","UPS1_25_InputVolA","1号UPSA相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["82","4.15.30.1","UPS1_25_InputVolB","1号UPSB相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["83","4.15.30.1","UPS1_25_InputVolC","1号UPSC相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["84","4.15.30.1","UPS1_25_OutputVolA","1号UPSA相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["85","4.15.30.1","UPS1_25_OutputVolB","1号UPSB相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["86","4.15.30.1","UPS1_25_OutputVolC","1号UPSC相输出电压","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["87","4.15.30.1","UPS1_25_OutputCurrA","1号UPSA相输出电流","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"10","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["88","4.15.30.1","UPS1_25_OutputCurrB","1号UPSB相输出电流","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"10","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["89","4.15.30.1","UPS1_25_OutputCurrC","1号UPSC相输出电流","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"10","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["90","4.15.30.1","UPS1_25_Freq","1号UPS输入频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"50","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["91","4.15.30.1","UPS1_25_BatteryVol","1号UPS电池电压","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["92","4.15.30.1","UPS1_25_Temp","1号UPS环境温度","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"25","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["93","4.15.30.1","UPS1_25_InputVolAbnormal","1号UPS市电电压异常","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["94","4.15.30.1","UPS1_25_BattertLow","1号UPS电池低电压","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["95","4.15.30.1","UPS1_25_Bypass","1号UPS旁路","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["96","4.15.30.1","UPS1_25_Fail","1号UPSUPS故障","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["97","4.15.30.1","UPS1_25_ShutDown","1号UPS蜂鸣器开","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","关,"]
["98","4.15.30.1","UPS1_25_RemainTime","1号UPS电池剩余时间","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","M","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","3","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["99","4.15.30.1","UPS1_25_OutputpowerA","1号UPSA相输出功率","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","KW","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["100","4.15.30.1","UPS1_25_OutputpowerB","1号UPSB相输出功率","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","KW","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["101","4.15.30.1","UPS1_25_OutputpowerC","1号UPSC相输出功率","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","KW","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["102","4.15.30.1","UPS1_25_Load","1号UPS负载量","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":23,"n_cols":76,"rows_kept":23,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["81","4.15.30.1","UPS1_25_InputVolA","二号五楼A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["82","4.15.30.1","UPS1_25_InputVolB","二号五楼B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["83","4.15.30.1","UPS1_25_InputVolC","二号五楼C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["84","4.15.30.1","UPS1_25_OutputVolA","二号五楼A相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["85","4.15.30.1","UPS1_25_OutputVolB","二号五楼B相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["86","4.15.30.1","UPS1_25_OutputVolC","二号五楼C相输出电压","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["87","4.15.30.1","UPS1_25_OutputCurrA","二号五楼A相输出电流","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"10","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["88","4.15.30.1","UPS1_25_OutputCurrB","二号五楼B相输出电流","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"10","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["89","4.15.30.1","UPS1_25_OutputCurrC","二号五楼C相输出电流","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"10","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["90","4.15.30.1","UPS1_25_Freq","二号五楼输入频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"50","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["91","4.15.30.1","UPS1_25_BatteryVol","二号五楼电池电压","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"220","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["92","4.15.30.1","UPS1_25_Temp","二号五楼环境温度","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"25","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["93","4.15.30.1","UPS1_25_InputVolAbnormal","二号五楼市电电压异常","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["94","4.15.30.1","UPS1_25_BattertLow","二号五楼电池低电压","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["95","4.15.30.1","UPS1_25_Bypass","二号五楼旁路","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["96","4.15.30.1","UPS1_25_Fail","二号五楼UPS故障","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["97","4.15.30.1","UPS1_25_ShutDown","二号五楼蜂鸣器开","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","关,"]
["98","4.15.30.1","UPS1_25_RemainTime","二号五楼电池剩余时间","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","M","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","3","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["99","4.15.30.1","UPS1_25_OutputpowerA","二号五楼A相输出功率","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","KW","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["100","4.15.30.1","UPS1_25_OutputpowerB","二号五楼B相输出功率","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","KW","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["101","4.15.30.1","UPS1_25_OutputpowerC","二号五楼C相输出功率","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","KW","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["102","4.15.30.1","UPS1_25_Load","二号五楼负载量","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]