{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":146,"n_cols":76,"rows_kept":146,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.36.1","HipulseU_1_ACInputvoltageAB","1号UPS 交流输入电压AB","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.36.1","HipulseU_1_ACInputvoltageBC","1号UPS 交流输入电压BC","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.36.1","HipulseU_1_ACInputvoltageCA","1号UPS 交流输入电压CA","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.36.1","HipulseU_1_ACoutputvoltageA","1号UPS 交流输出电压A","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.36.1","HipulseU_1_ACoutputvoltageB","1号UPS 交流输出电压B","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.36.1","HipulseU_1_ACoutputvoltageC","1号UPS 交流输出电压C","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.36.1","HipulseU_1_ACoutputCurrentA","1号UPS 交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.36.1","HipulseU_1_ACoutputCurrentB","1号UPS 交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.36.1","HipulseU_1_ACoutputCurrentC","1号UPS 交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.36.1","HipulseU_1_DCInputVoltage","1号UPS 直流输入电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.36.1","HipulseU_1_OutputFrequency","1号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.36.1","HipulseU_1_ACInputLineVoltageAB","1号UPS 交流输入线电压AB","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.36.1","HipulseU_1_ACInputLineVoltageBC","1号UPS 交流输入线电压BC","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.36.1","HipulseU_1_ACInputLineVoltageCA","1号UPS 交流输入线电压CA","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.36.1","HipulseU_1_InputCurrentA","1号UPS A相输入电流","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.36.1","HipulseU_1_InputCurrentB","1号UPS B相输入电流","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.36.1","HipulseU_1_InputCurrentC","1号UPS C相输入电流","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.36.1","HipulseU_1_InputFrequency","1号UPS 输入频率","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.36.1","HipulseU_1_AphaseBypassVoltage","1号UPS A相旁路电压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.36.1","HipulseU_1_BphaseBypassVoltage","1号UPS B相旁路电压","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.36.1","HipulseU_1_CphaseBypassVoltage","1号UPS C相旁路电压","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.36.1","HipulseU_1_BypassFrequency","1号UPS 旁路频率","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.36.1","HipulseU_1_BatteryCurrent","1号UPS 电池电流","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.36.1","HipulseU_1_AphaseOutputActivePower","1号UPS A相输出有功功率","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.36.1","HipulseU_1_BphaseOutputActivePower","1号UPS B相输出有功功率","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.36.1","HipulseU_1_CphaseOutputActivePower","1号UPS C相输出有功功率","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.36.1","HipulseU_1_AphaseOutputApparentPower","1号UPS A相输出视在功率","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.36.1","HipulseU_1_BphaseOutputApparentPower","1号UPS B相输出视在功率","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.36.1","HipulseU_1_CphaseOutputApparentPower","1号UPS C相输出视在功率","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.36.1","HipulseU_1_AphaseOutputpercentage","1号UPS A相输出负载百分比","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","4.19.36.1","HipulseU_1_BphaseOutputpercentage","1号UPS B相输出负载百分比","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","4.19.36.1","HipulseU_1_CphaseOutputpercentage","1号UPS C相输出负载百分比","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.19.36.1","HipulseU_1_RemainingBatteryBackupTime","1号UPS 电池后备时间","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","8888","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","4.19.36.1","HipulseU_1_BatteryTemperature","1号UPS 电池温度","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["35","4.19.36.1","HipulseU_1_Temperature","1号UPS 环境温度","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","4.19.36.1","HipulseU_1_PowerSupply","1号UPS 供电方式","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["37","4.19.36.1","HipulseU_1_batteryTest","1号UPS 电池自检中","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["38","4.19.36.1","HipulseU_1_onoffstatus","1号UPS 开机/关机状态","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224,","UPS关机,"]
["39","4.19.36.1","HipulseU_1_upssupply","1号UPS UPS供电","1","0","0","1","0","cmd-67","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","3","225,226,227,","电池逆变供电,联合逆变供电,整流电池均不供电,"]
["40","4.19.36.1","HipulseU_1_InputSwitchStatus","1号UPS 输入开关状态","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开,"]
["41","4.19.36.1","HipulseU_1_MaintenanceBypassSwitchState","1号UPS 维修旁路开关状态","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开,"]
["42","4.19.36.1","HipulseU_1_BypassSwitchCondition","1号UPS 旁路开关状态","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开,"]
["43","4.19.36.1","HipulseU_1_OutputSwitchState","1号UPS 输出开关状态","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开,"]
["45","4.19.36.1","HipulseU_1_InverterSynorAsynchronous","1号UPS 逆变器同步/不同步","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","3，","不同步,"]
["46","4.19.36.1","HipulseU_1_MainRoadVoltageExceptionally","1号UPS 主路电压异常","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常，"]
["47","4.19.36.1","HipulseU_1_InverterOutputVoltageAbnormal","1号UPS 逆变输出电压异常","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常，"]
["48","4.19.36.1","HipulseU_1_BypassCases","1号UPS 旁路情况","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常，"]
["49","4.19.36.1","HipulseU_1_TotalBatteryVoltageStatus","1号UPS 蓄电池总电压状态","1","0","0","1","0","cmd-80","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","4","1,2,240,225,226,","低于下限,高于上限,电池无,电池接反,"]
["50","4.19.36.1","HipulseU_1_MainRoadFrequencyException","1号UPS 主路频率异常","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","超限,"]
["51","4.19.36.1","HipulseU_1_MainRoadPhaseFailure","1号UPS 主路缺相故障","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障,"]
["52","4.19.36.1","HipulseU_1_AuxiliaryPowerSupply1Down","1号UPS 辅助电源1掉电","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障,"]
["53","4.19.36.1","HipulseU_1_AuxiliaryPowerSupp2y1Down","1号UPS 辅助电源2掉电","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["54","4.19.36.1","HipulseU_1_RectifierExcessivelyWarm ","1号UPS 整流器过温","1","0","0","1","0","cmd-91","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过温，"]
["55","4.19.36.1","HipulseU_1_RectifierCommunicationFailure","1号UPS 整流通讯故障","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["56","4.19.36.1","HipulseU_1_InverterOverTemperature","1号UPS 逆变器过温","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过温，"]
["57","4.19.36.1","HipulseU_1_Fanfailure","1号UPS 风扇故障","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["58","4.19.36.1","HipulseU_1_SingleOutputOverload","1号UPS 单机输出过载","1","0","0","1","0","cmd-102","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过载，"]
["59","4.19.36.1","HipulseU_1_AbnormalShutdownBypass","1号UPS 旁路异常关机","1","0","0","1","0","cmd-105","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常关机，"]
["60","4.19.36.1","HipulseU_1_ACoutputovervoltage","1号UPS 交流输出过压","1","0","0","1","0","cmd-106","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["61","4.19.36.1","HipulseU_1_Inverterovercurrent","1号UPS 逆变器过流","1","0","0","1","0","cmd-107","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过流，"]
["62","4.19.36.1","HipulseU_1_Bypassforewordinstead","1号UPS 旁路相序反","1","0","0","1","0","cmd-108","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["63","4.19.36.1","HipulseU_1_Switchbypasstheloadimpact","1号UPS 负载冲击转旁路","1","0","0","1","0","cmd-109","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["64","4.19.36.1","HipulseU_1_Bypassovercurrentfault","1号UPS 旁路过流故障","1","0","0","1","0","cmd-117","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["65","4.19.36.1","HipulseU_1_Bypassinductanceovertemperature","1号UPS 旁路电感过温","1","0","0","1","0","cmd-119","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过高，"]
["66","4.19.36.1","HipulseU_1_Contravariantcommunication","1号UPS 逆变通讯故障","1","0","0","1","0","cmd-123","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["67","4.19.36.1","HipulseU_1_Environmenthyperpyrexia","1号UPS 环境温度过高","1","0","0","1","0","cmd-126","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过高，"]
["68","4.19.36.1","HipulseU_1_Batteryhyperpyrexia","1号UPS 电池温度过高","1","0","0","1","0","cmd-128","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过高，"]
["69","4.19.36.1","HipulseU_1_Batteryfusebroken","1号UPS 电池熔丝断","1","0","0","1","0","cmd-130","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","断，"]
["70","4.19.36.1","HipulseU_1_outputfusebreaks","1号UPS 输出熔丝断","1","0","0","1","0","cmd-132","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","断，"]
["71","4.19.36.1","HipulseU_1_Busbarelectriccapacity","1号UPS 母线电容过压","1","0","0","1","0","cmd-133","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["72","4.19.36.1","HipulseU_1_Busovervoltage","1号UPS 母线过压","1","0","0","1","0","cmd-134","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["1","4.19.36.1","HipulseU_1_Communications","1号UPS通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","137",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]
[]
["1","4.19.36.2","HipulseU_2_ACInputvoltageAB","2号UPS 交流输入电压AB","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.36.2","HipulseU_2_ACInputvoltageBC","2号UPS 交流输入电压BC","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.36.2","HipulseU_2_ACInputvoltageCA","2号UPS 交流输入电压CA","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.36.2","HipulseU_2_ACoutputvoltageA","2号UPS 交流输出电压A","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.36.2","HipulseU_2_ACoutputvoltageB","2号UPS 交流输出电压B","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.36.2","HipulseU_2_ACoutputvoltageC","2号UPS 交流输出电压C","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.36.2","HipulseU_2_ACoutputCurrentA","2号UPS 交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.36.2","HipulseU_2_ACoutputCurrentB","2号UPS 交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.36.2","HipulseU_2_ACoutputCurrentC","2号UPS 交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.36.2","HipulseU_2_DCInputVoltage","2号UPS 直流输入电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.36.2","HipulseU_2_OutputFrequency","2号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.36.2","HipulseU_2_ACInputLineVoltageAB","2号UPS 交流输入线电压AB","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.36.2","HipulseU_2_ACInputLineVoltageBC","2号UPS 交流输入线电压BC","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.36.2","HipulseU_2_ACInputLineVoltageCA","2号UPS 交流输入线电压CA","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.36.2","HipulseU_2_InputCurrentA","2号UPS A相输入电流","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.36.2","HipulseU_2_InputCurrentB","2号UPS B相输入电流","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.36.2","HipulseU_2_InputCurrentC","2号UPS C相输入电流","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.36.2","HipulseU_2_InputFrequency","2号UPS 输入频率","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.36.2","HipulseU_2_AphaseBypassVoltage","2号UPS A相旁路电压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.36.2","HipulseU_2_BphaseBypassVoltage","2号UPS B相旁路电压","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.36.2","HipulseU_2_CphaseBypassVoltage","2号UPS C相旁路电压","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.36.2","HipulseU_2_BypassFrequency","2号UPS 旁路频率","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.36.2","HipulseU_2_BatteryCurrent","2号UPS 电池电流","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.36.2","HipulseU_2_AphaseOutputActivePower","2号UPS A相输出有功功率","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.36.2","HipulseU_2_BphaseOutputActivePower","2号UPS B相输出有功功率","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.36.2","HipulseU_2_CphaseOutputActivePower","2号UPS C相输出有功功率","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.36.2","HipulseU_2_AphaseOutputApparentPower","2号UPS A相输出视在功率","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.36.2","HipulseU_2_BphaseOutputApparentPower","2号UPS B相输出视在功率","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.36.2","HipulseU_2_CphaseOutputApparentPower","2号UPS C相输出视在功率","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.36.2","HipulseU_2_AphaseOutputpercentage","2号UPS A相输出负载百分比","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","4.19.36.2","HipulseU_2_BphaseOutputpercentage","2号UPS B相输出负载百分比","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","4.19.36.2","HipulseU_2_CphaseOutputpercentage","2号UPS C相输出负载百分比","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.19.36.2","HipulseU_2_RemainingBatteryBackupTime","2号UPS 电池后备时间","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","8888","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","4.19.36.2","HipulseU_2_BatteryTemperature","2号UPS 电池温度","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["35","4.19.36.2","HipulseU_2_Temperature","2号UPS 环境温度","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","4.19.36.2","HipulseU_2_PowerSupply","2号UPS 供电方式","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["37","4.19.36.2","HipulseU_2_batteryTest","2号UPS 电池自检中","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["38","4.19.36.2","HipulseU_2_onoffstatus","2号UPS 开机/关机状态","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224,","UPS关机,"]
["39","4.19.36.2","HipulseU_2_upssupply","2号UPS UPS供电","1","0","0","1","0","cmd-67","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","3","225,226,227,","电池逆变供电,联合逆变供电,整流电池均不供电,"]
["40","4.19.36.2","HipulseU_2_InputSwitchStatus","2号UPS 输入开关状态","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开，"]
["41","4.19.36.2","HipulseU_2_MaintenanceBypassSwitchState","2号UPS 维修旁路开关状态","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开，"]
["42","4.19.36.2","HipulseU_2_BypassSwitchCondition","2号UPS 旁路开关状态","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开，"]
["43","4.19.36.2","HipulseU_2_OutputSwitchState","2号UPS 输出开关状态","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","断开，"]
["45","4.19.36.2","HipulseU_2_InverterSynorAsynchronous","2号UPS 逆变器同步/不同步","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","3，","不同步，"]
["46","4.19.36.2","HipulseU_2_MainRoadVoltageExceptionally","2号UPS 主路电压异常","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常，"]
["47","4.19.36.2","HipulseU_2_InverterOutputVoltageAbnormal","2号UPS 逆变输出电压异常","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常，"]
["48","4.19.36.2","HipulseU_2_BypassCases","2号UPS 旁路情况","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常，"]
["49","4.19.36.2","HipulseU_2_TotalBatteryVoltageStatus","2号UPS 蓄电池总电压状态","1","0","0","1","0","cmd-80","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","4","1,2,240,225,226,","低于下限，高于上限，电池无，电池接反，"]
["50","4.19.36.2","HipulseU_2_MainRoadFrequencyException","2号UPS 主路频率异常","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","224，","超限,"]
["51","4.19.36.2","HipulseU_2_MainRoadPhaseFailure","2号UPS 主路缺相故障","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["52","4.19.36.2","HipulseU_2_AuxiliaryPowerSupply1Down","2号UPS 辅助电源1掉电","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["53","4.19.36.2","HipulseU_2_AuxiliaryPowerSupp2y1Down","2号UPS 辅助电源2掉电","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["54","4.19.36.2","HipulseU_2_RectifierExcessivelyWarm ","2号UPS 整流器过温","1","0","0","1","0","cmd-91","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过温，"]
["55","4.19.36.2","HipulseU_2_RectifierCommunicationFailure","2号UPS 整流通讯故障","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["56","4.19.36.2","HipulseU_2_InverterOverTemperature","2号UPS 逆变器过温","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过温，"]
["57","4.19.36.2","HipulseU_2_Fanfailure","2号UPS 风扇故障","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["58","4.19.36.2","HipulseU_2_SingleOutputOverload","2号UPS 单机输出过载","1","0","0","1","0","cmd-102","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过载，"]
["59","4.19.36.2","HipulseU_2_AbnormalShutdownBypass","2号UPS 旁路异常关机","1","0","0","1","0","cmd-105","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","异常关机，"]
["60","4.19.36.2","HipulseU_2_ACoutputovervoltage","2号UPS 交流输出过压","1","0","0","1","0","cmd-106","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["61","4.19.36.2","HipulseU_2_Inverterovercurrent","2号UPS 逆变器过流","1","0","0","1","0","cmd-107","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过流，"]
["62","4.19.36.2","HipulseU_2_Bypassforewordinstead","2号UPS 旁路相序反","1","0","0","1","0","cmd-108","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["63","4.19.36.2","HipulseU_2_Switchbypasstheloadimpact","2号UPS 负载冲击转旁路","1","0","0","1","0","cmd-109","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["64","4.19.36.2","HipulseU_2_Bypassovercurrentfault","2号UPS 旁路过流故障","1","0","0","1","0","cmd-117","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["65","4.19.36.2","HipulseU_2_Bypassinductanceovertemperature","2号UPS 旁路电感过温","1","0","0","1","0","cmd-119","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过高，"]
["66","4.19.36.2","HipulseU_2_Contravariantcommunication","2号UPS 逆变通讯故障","1","0","0","1","0","cmd-123","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["67","4.19.36.2","HipulseU_2_Environmenthyperpyrexia","2号UPS 环境温度过高","1","0","0","1","0","cmd-126","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过高，"]
["68","4.19.36.2","HipulseU_2_Batteryhyperpyrexia","2号UPS 电池温度过高","1","0","0","1","0","cmd-128","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","过高，"]
["69","4.19.36.2","HipulseU_2_Batteryfusebroken","2号UPS 电池熔丝断","1","0","0","1","0","cmd-130","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","断，"]
["70","4.19.36.2","HipulseU_2_outputfusebreaks","2号UPS 输出熔丝断","1","0","0","1","0","cmd-132","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","断，"]
["71","4.19.36.2","HipulseU_2_Busbarelectriccapacity","2号UPS 母线电容过压","1","0","0","1","0","cmd-133","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["72","4.19.36.2","HipulseU_2_Busovervoltage","2号UPS 母线过压","1","0","0","1","0","cmd-134","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","36",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240，","故障，"]
["1","4.19.36.2","HipulseU_2_Communications","2号UPS通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","137",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]