{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":344,"n_cols":76,"rows_kept":344,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.38.1","nxr_1_Aphaseinputvoltage","1号UPS A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.38.1","nxr_1_Bphaseinputvoltage","1号UPS B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.38.1","nxr_1_PhaseCinputvoltage","1号UPS C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.38.1","nxr_1_Aphaseoutputvoltage","1号UPS A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.38.1","nxr_1_Bphaseoutputvoltage","1号UPS B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.38.1","nxr_1_Cphaseoutputvoltage","1号UPS C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.38.1","nxr_1_Aphaseoutputcurrent","1号UPS A相输出电流","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.38.1","nxr_1_Bphaseoutputcurrent","1号UPS B相输出电流","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.38.1","nxr_1_PhaseCoutputcurrent","1号UPS C相输出电流","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.38.1","nxr_1_BatteryPack1voltage","1号UPS 电池组1电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.38.1","nxr_1_Outputfrequency","1号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.38.1","nxr_1_BatteryPack2voltage","1号UPS 电池组2电压","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.38.1","nxr_1_Thisrackispowersupplymode","1号UPS 本机架供电方式","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","1,2,233,","01:UPS供电,02:旁路供电,E9:均不供电,"]
["18","4.19.38.1","nxr_1_BatPack1Selftest","1号UPS 电池组1电池自检","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["19","4.19.38.1","nxr_1_BatPack1Charge","1号UPS 电池组1均充/浮充状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["20","4.19.38.1","nxr_1_Themachineturnsonoffthephone","1号UPS 整机开机/关机","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","224,","E0:关机,"]
["21","4.19.38.1","nxr_1_Rectifierpowersupplycondition","1号UPS 整流器供电状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","4","224,225,226,227,","E0:主路逆变供电,E1:电池逆变供电,E2:联合逆变供电,E3:整流电池均不供电,"]
["22","4.19.38.1","nxr_1_Thegeneratorswitchonevents","1号UPS 整机发电机接入事件","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:发电机接入,E1:发电机没接入,"]
["23","4.19.38.1","nxr_1_Theinputemptyopenposition","1号UPS 整机输入空开状态","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["24","4.19.38.1","nxr_1_Themachinemaintenancebypassemptyopenposition","1号UPS 整机维修旁路空开状态","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["25","4.19.38.1","nxr_1_Thebypassemptyopenposition","1号UPS 整机旁路空开状态","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["26","4.19.38.1","nxr_1_Theoutputemptyopenposition","1号UPS 整机输出空开状态","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["27","4.19.38.1","nxr_1_Therotatingemptyopenposition","1号UPS 整机旋转空开状态","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["28","4.19.38.1","nxr_1_Framesystemcurrentsupplystateweaver","1号UPS 机架并机系统供电状态","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","6","224,225,226,227,228,229,","E0:均不供电,E1:旁路供电,E2:市电供电,E3:电池逆变供电,E4:联合供电,E5:输出禁止,"]
["29","4.19.38.1","nxr_1_BatPack2Selftest","1号UPS 电池组2电池自检","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["30","4.19.38.1","nxr_1_BatPack2Charge","1号UPS 电池组2浮充/均充状态","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["31","4.19.38.1","nxr_1_Module1onlinestatus","1号UPS 模块1在线状态","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["32","4.19.38.1","nxr_1_Module2onlinestatus","1号UPS 模块2在线状态","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["33","4.19.38.1","nxr_1_Module3onlinestatus","1号UPS 模块3在线状态","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["34","4.19.38.1","nxr_1_Module4onlinestatus","1号UPS 模块4在线状态","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["35","4.19.38.1","nxr_1_Module5onlinestatus","1号UPS 模块5在线状态","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["36","4.19.38.1","nxr_1_Module6onlinestatus","1号UPS 模块6在线状态","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["37","4.19.38.1","nxr_1_Module7onlinestatus","1号UPS 模块7在线状态","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["38","4.19.38.1","nxr_1_Module8onlinestatus","1号UPS 模块8在线状态","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["39","4.19.38.1","nxr_1_Module9onlinestatus","1号UPS 模块9在线状态","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["40","4.19.38.1","nxr_1_Module10onlinestatus","1号UPS 模块10在线状态","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["41","4.19.38.1","nxr_1_Invertersynchronousnosynchronization","1号UPS 逆变器同步/不同步","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","3,","03:不同步,"]
["42","4.19.38.1","nxr_1_Massiveabnormalvoltage","1号UPS 主路电压异常","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["43","4.19.38.1","nxr_1_rectifier","1号UPS 整流器","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["44","4.19.38.1","nxr_1_inverter","1号UPS 逆变器","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["45","4.19.38.1","nxr_1_Bypassstate","1号UPS 旁路状态","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["46","4.19.38.1","nxr_1_Batterystate1","1号UPS 电池组1状态","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","5","240,241,242,243,244,","F0:低于下限(关机点),F1:高于上限(电压过高),F2:电池无,F3:预告警,F4:电池接反,"]
["49","4.19.38.1","nxr_1_Powermodule1fault","1号UPS 功率模块1故障","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["50","4.19.38.1","nxr_1_Powermodule2fault","1号UPS 功率模块2故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["51","4.19.38.1","nxr_1_Powermodule3fault","1号UPS 功率模块3故障","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["52","4.19.38.1","nxr_1_Powermodule4fault","1号UPS 功率模块4故障","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["53","4.19.38.1","nxr_1_Powermodule5fault","1号UPS 功率模块5故障","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["54","4.19.38.1","nxr_1_Powermodule6fault","1号UPS 功率模块6故障","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["55","4.19.38.1","nxr_1_Powermodule7fault","1号UPS 功率模块7故障","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["56","4.19.38.1","nxr_1_Powermodule8fault","1号UPS 功率模块8故障","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["57","4.19.38.1","nxr_1_Powermodule9fault","1号UPS 功率模块9故障","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["58","4.19.38.1","nxr_1_Powermodule10fault","1号UPS 功率模块10故障","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["59","4.19.38.1","nxr_1_AbnormalLBS","1号UPS LBS异常","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["60","4.19.38.1","nxr_1_Thekeyboardboardfailureormachinecapacityisinvalid","1号UPS 键盘板故障或机型容量无效","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:键盘板故障,F1:机型容量无效,"]
["61","4.19.38.1","nxr_1_Fanfault","1号UPS 风扇故障","1","0","0","1","0","cmd-61","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["62","4.19.38.1","nxr_1_Environmentaltemperatureistoohigh","1号UPS 环境温度过高","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["63","4.19.38.1","nxr_1_Emergencyshutdown","1号UPS 紧急关机","1","0","0","1","0","cmd-63","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:紧急关机,"]
["64","4.19.38.1","nxr_1_Bypassthyristorfault","1号UPS 旁路晶闸管故障","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["65","4.19.38.1","nxr_1_Bypassthesequence","1号UPS 旁路相序反","1","0","0","1","0","cmd-65","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["66","4.19.38.1","nxr_1_Bypasstheflowfault","1号UPS 旁路过流故障","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["67","4.19.38.1","nxr_1_Bypassabnormalshutdown","1号UPS 旁路异常关机","1","0","0","1","0","cmd-67","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["68","4.19.38.1","nxr_1_Bypassswitchingtimesrestrictions","1号UPS 旁路切换次数限制","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["69","4.19.38.1","nxr_1_Theweavermoduleboardfailure","1号UPS 模块并机板故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["70","4.19.38.1","nxr_1_Modulelinefaultweaver","1号UPS 模块并机线连接故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["71","4.19.38.1","nxr_1_Theweavermodulecommunicationfault","1号UPS 模块并机通信故障","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["72","4.19.38.1","nxr_1_Auxiliarypower2offelectricity","1号UPS 辅助电源2掉电","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["73","4.19.38.1","nxr_1_Contactpowerboard1fault","1号UPS 接触电源板1故障","1","0","0","1","0","cmd-73","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["74","4.19.38.1","nxr_1_Contactpowerboard2fault","1号UPS 接触电源板2故障","1","0","0","1","0","cmd-74","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["75","4.19.38.1","nxr_1_Redundancyfanpowerfailure","1号UPS 冗余风扇电源故障","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["76","4.19.38.1","nxr_1_BCBaccess","1号UPS BCB接入情况","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","00:BCB未接入,F0:BCB闭合,"]
["77","4.19.38.1","nxr_1_Batterypacks1contactorfault","1号UPS 电池组1接触器故障","1","0","0","1","0","cmd-77","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["78","4.19.38.1","nxr_1_Batterypacks2contactorfault","1号UPS 电池组2接触器故障","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["79","4.19.38.1","nxr_1_Batterypacks1switchfault","1号UPS 电池组1交换器故障","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["80","4.19.38.1","nxr_1_Batterypacks2switchfault","1号UPS 电池组2交换器故障","1","0","0","1","0","cmd-80","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["81","4.19.38.1","nxr_1_Batterypacks1switchtheflow","1号UPS 电池组1交换器过流","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["82","4.19.38.1","nxr_1_Batterypacks2switchtheflow","1号UPS 电池组2交换器过流","1","0","0","1","0","cmd-82","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["83","4.19.38.1","nxr_1_Batterypacks1switchthermal","1号UPS 电池组1交换器过温","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["84","4.19.38.1","nxr_1_Batterypacks2switchthermal","1号UPS 电池组2交换器过温","1","0","0","1","0","cmd-84","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["85","4.19.38.1","nxr_1_1thebatterychargerfault","1号UPS 电池组1充电器故障","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["86","4.19.38.1","nxr_1_2thebatterychargerfault","1号UPS 电池组2充电器故障","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["87","4.19.38.1","nxr_1_Batterylife1","1号UPS 电池组1寿命情况","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["88","4.19.38.1","nxr_1_Batterylife2","1号UPS 电池组2寿命情况","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["89","4.19.38.1","nxr_1_Batterypacks1temperaturewastoohigh","1号UPS 电池组1温度过高","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["90","4.19.38.1","nxr_1_Batterypacks2temperaturewastoohigh","1号UPS 电池组2温度过高","1","0","0","1","0","cmd-90","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["91","4.19.38.1","nxr_1_Batterypacks1groundfault","1号UPS 电池组1接地故障","1","0","0","1","0","cmd-91","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["92","4.19.38.1","nxr_1_Batterypacks2groundfault","1号UPS 电池组2接地故障","1","0","0","1","0","cmd-92","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["93","4.19.38.1","nxr_1_Massiveunusualfrequency","1号UPS 主路频率异常","1","0","0","1","0","cmd-93","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["94","4.19.38.1","nxr_1_Balanceinductancethermal","1号UPS 平衡电感过温","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["95","4.19.38.1","nxr_1_Inputinductancethermal","1号UPS 输入电感过温","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["96","4.19.38.1","nxr_1_Rectifierthermal","1号UPS 整流器过温","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["97","4.19.38.1","nxr_1_Balancecircuitfault","1号UPS 平衡电路故障","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["98","4.19.38.1","nxr_1_Balanceelectricitypassbyflow","1号UPS 平衡电路过流","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["99","4.19.38.1","nxr_1_Meltbrokenwirerunning","1号UPS 主路熔丝断","1","0","0","1","0","cmd-99","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["100","4.19.38.1","nxr_1_1theauxiliarypoweroff","1号UPS 辅助电源1掉电","1","0","0","1","0","cmd-100","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["101","4.19.38.1","nxr_1_Sequencerunningagainst","1号UPS 主路相序反","1","0","0","1","0","cmd-101","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["102","4.19.38.1","nxr_1_Rectifierflow","1号UPS 整流器过流","1","0","0","1","0","cmd-102","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["103","4.19.38.1","nxr_1_Softstartupfailure","1号UPS 软启动失败","1","0","0","1","0","cmd-103","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["104","4.19.38.1","nxr_1_Inverterinductancethermal","1号UPS 逆变电感过温","1","0","0","1","0","cmd-104","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["105","4.19.38.1","nxr_1_Inverterthermal","1号UPS 逆变器过温","1","0","0","1","0","cmd-105","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["106","4.19.38.1","nxr_1_Thethyristorinverterfault","1号UPS 逆变器晶闸管故障","1","0","0","1","0","cmd-106","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["107","4.19.38.1","nxr_1_Theuseroperationerror","1号UPS 用户操作错误","1","0","0","1","0","cmd-107","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:错误,"]
["108","4.19.38.1","nxr_1_Outputmeltsilkbroken","1号UPS 输出熔丝断","1","0","0","1","0","cmd-108","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["109","4.19.38.1","nxr_1_Monolithicoutputoverload","1号UPS 单片输出过载","1","0","0","1","0","cmd-109","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["110","4.19.38.1","nxr_1_Expertsystemoverload","1号UPS 并机系统过载","1","0","0","1","0","cmd-110","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["111","4.19.38.1","nxr_1_Singleoverloadovertime","1号UPS 单机过载超时","1","0","0","1","0","cmd-111","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载超时,"]
["112","4.19.38.1","nxr_1_Acoutputpressure","1号UPS 交流输出过压","1","0","0","1","0","cmd-112","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过压,"]
["113","4.19.38.1","nxr_1_Inverterflow","1号UPS 逆变器过流","1","0","0","1","0","cmd-113","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["114","4.19.38.1","nxr_1_Impactloadtobypass","1号UPS 负载冲击转旁路","1","0","0","1","0","cmd-114","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["115","4.19.38.1","nxr_1_Allflowweaverfault","1号UPS 并机均流故障","1","0","0","1","0","cmd-115","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["116","4.19.38.1","nxr_1_Busabnormalshutdown","1号UPS 母线异常关机","1","0","0","1","0","cmd-116","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["117","4.19.38.1","nxr_1_Adjacenttobypassmachinerequest","1号UPS 邻机请求转旁路","1","0","0","1","0","cmd-117","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["118","4.19.38.1","nxr_1_Dcbusovervoltagefault","1号UPS 直流母线过压故障","1","0","0","1","0","cmd-118","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["119","4.19.38.1","nxr_1_Rectifiercommunicationfault","1号UPS 整流通信故障","1","0","0","1","0","cmd-119","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["120","4.19.38.1","nxr_1_Invertercommunicationfailures","1号UPS 逆变通讯故障","1","0","0","1","0","cmd-120","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["121","4.19.38.1","nxr_1_Outputdccomponentfaulttoo","1号UPS 输出直流分量过大故障","1","0","0","1","0","cmd-121","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["122","4.19.38.1","nxr_1_Expertsystembatteryforecastpfault","1号UPS 并机系统电池预告警故障","1","0","0","1","0","cmd-122","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["123","4.19.38.1","nxr_1_Inputlackofzerofault","1号UPS 输入缺零故障","1","0","0","1","0","cmd-123","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["124","4.19.38.1","nxr_1_Invertercontactorfault","1号UPS 逆变接触器故障","1","0","0","1","0","cmd-124","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["125","4.19.38.1","nxr_1_Inputcontactorfault","1号UPS 输入接触器故障","1","0","0","1","0","cmd-125","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["126","4.19.38.1","nxr_1_Inputcurrentabnormal","1号UPS 输入电流异常","1","0","0","1","0","cmd-126","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["127","4.19.38.1","nxr_1_Outputabnormalvoltage","1号UPS 输出电压异常","1","0","0","1","0","cmd-127","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["130","4.19.38.1","nxr_1_AcinputlinevoltageAB","1号UPS 交流输入线电压AB","1","0","0","1","0","cmd-130","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["131","4.19.38.1","nxr_1_AcinputlinevoltageBC","1号UPS 交流输入线电压BC","1","0","0","1","0","cmd-131","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["132","4.19.38.1","nxr_1_AcinputlinevoltageCA","1号UPS 交流输入线电压CA","1","0","0","1","0","cmd-132","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["133","4.19.38.1","nxr_1_Aphaseinputcurrent","1号UPS A相输入电流","1","0","0","1","0","cmd-133","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["134","4.19.38.1","nxr_1_Bphaseinputcurrent","1号UPS B相输入电流","1","0","0","1","0","cmd-134","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["135","4.19.38.1","nxr_1_CPhaseinputcurrent","1号UPS C相输入电流","1","0","0","1","0","cmd-135","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["136","4.19.38.1","nxr_1_Inputfrequency","1号UPS 输入频率","1","0","0","1","0","cmd-136","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["137","4.19.38.1","nxr_1_Aphaseinputpowerfactor","1号UPS A相输入功率因数","1","0","0","1","0","cmd-137","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["138","4.19.38.1","nxr_1_Bphaseinputpowerfactor","1号UPS B相输入功率因数","1","0","0","1","0","cmd-138","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["139","4.19.38.1","nxr_1_Cphaseinputpowerfactor","1号UPS C相输入功率因数","1","0","0","1","0","cmd-139","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["140","4.19.38.1","nxr_1_Aphasebypassvoltage","1号UPS A相旁路电压","1","0","0","1","0","cmd-140","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["141","4.19.38.1","nxr_1_Bphasebypassvoltage","1号UPS B相旁路电压","1","0","0","1","0","cmd-141","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["142","4.19.38.1","nxr_1_CPhasebypassvoltage","1号UPS C相旁路电压","1","0","0","1","0","cmd-142","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["143","4.19.38.1","nxr_1_Bypassfrequency","1号UPS 旁路频率","1","0","0","1","0","cmd-143","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["146","4.19.38.1","nxr_1_Aphaseoutputpowerfactor","1号UPS A相输出功率因数","1","0","0","1","0","cmd-146","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["147","4.19.38.1","nxr_1_Bphaseoutputpowerfactor","1号UPS B相输出功率因数","1","0","0","1","0","cmd-147","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["148","4.19.38.1","nxr_1_Cphaseoutputpowerfactor","1号UPS C相输出功率因数","1","0","0","1","0","cmd-148","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["149","4.19.38.1","nxr_1_Aphaseoutputthanpeak","1号UPS A相输出峰值比","1","0","0","1","0","cmd-149","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["150","4.19.38.1","nxr_1_Bphaseoutputthanpeak","1号UPS B相输出峰值比","1","0","0","1","0","cmd-150","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["151","4.19.38.1","nxr_1_Cphaseoutputthanpeak","1号UPS C相输出峰值比","1","0","0","1","0","cmd-151","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["152","4.19.38.1","nxr_1_Aphaseoutputactivepower","1号UPS A相输出有功功率","1","0","0","1","0","cmd-152","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["153","4.19.38.1","nxr_1_Bphaseoutputactivepower","1号UPS B相输出有功功率","1","0","0","1","0","cmd-153","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["154","4.19.38.1","nxr_1_Cphaseoutputactivepower","1号UPS C相输出有功功率","1","0","0","1","0","cmd-154","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["155","4.19.38.1","nxr_1_Aphaseoutputreactivepower","1号UPS A相输出无功功率","1","0","0","1","0","cmd-155","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["156","4.19.38.1","nxr_1_Bphaseoutputreactivepower","1号UPS B相输出无功功率","1","0","0","1","0","cmd-156","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["157","4.19.38.1","nxr_1_Cphaseoutputreactivepower","1号UPS C相输出无功功率","1","0","0","1","0","cmd-157","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["158","4.19.38.1","nxr_1_Aphaseoutputpowerinstalled","1号UPS A相输出视在功率","1","0","0","1","0","cmd-158","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["159","4.19.38.1","nxr_1_Bphaseoutputpowerinstalled","1号UPS B相输出视在功率","1","0","0","1","0","cmd-159","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["160","4.19.38.1","nxr_1_Cphaseoutputpowerinstalled","1号UPS C相输出视在功率","1","0","0","1","0","cmd-160","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["161","4.19.38.1","nxr_1_Aphaseoutputloadpercentage","1号UPS A相输出负载百分比","1","0","0","1","0","cmd-161","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["162","4.19.38.1","nxr_1_Bphaseoutputloadpercentage","1号UPS B相输出负载百分比","1","0","0","1","0","cmd-162","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["163","4.19.38.1","nxr_1_Cphaseoutputloadpercentage","1号UPS C相输出负载百分比","1","0","0","1","0","cmd-163","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["165","4.19.38.1","nxr_1_SystemAphaseoutputactivepower","1号UPS 系统A相输出有功功率","1","0","0","1","0","cmd-165","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["166","4.19.38.1","nxr_1_SystemBphaseoutputactivepower","1号UPS 系统B相输出有功功率","1","0","0","1","0","cmd-166","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["167","4.19.38.1","nxr_1_SystemCphaseoutputactivepower","1号UPS 系统C相输出有功功率","1","0","0","1","0","cmd-167","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["168","4.19.38.1","nxr_1_SysteminstalledAphaseoutputpower","1号UPS 系统A相输出视在功率","1","0","0","1","0","cmd-168","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["169","4.19.38.1","nxr_1_SysteminstalledBphaseoutputpower","1号UPS 系统B相输出视在功率","1","0","0","1","0","cmd-169","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["170","4.19.38.1","nxr_1_SysteminstalledCphaseoutputpower","1号UPS 系统C相输出视在功率","1","0","0","1","0","cmd-170","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["171","4.19.38.1","nxr_1_SystemAphaseoutputreactivepower","1号UPS 系统A相输出无功功率","1","0","0","1","0","cmd-171","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["172","4.19.38.1","nxr_1_SystemBphaseoutputreactivepower","1号UPS 系统B相输出无功功率","1","0","0","1","0","cmd-172","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["173","4.19.38.1","nxr_1_SystemCphaseoutputreactivepower","1号UPS 系统C相输出无功功率","1","0","0","1","0","cmd-173","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["176","4.19.38.1","nxr_1_Batterybackuptime","1号UPS 电池后备时间","1","0","0","1","0","cmd-176","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["177","4.19.38.1","nxr_1_Arebatteryvoltage","1号UPS 正电池电压","1","0","0","1","0","cmd-177","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["178","4.19.38.1","nxr_1_Arebatteryelectriccurrent","1号UPS 正电池电流","1","0","0","1","0","cmd-178","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["179","4.19.38.1","nxr_1_Negativebatteryvoltage","1号UPS 负电池电压","1","0","0","1","0","cmd-179","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["180","4.19.38.1","nxr_1_Negativebatteryelectriccurrent","1号UPS 负电池电流","1","0","0","1","0","cmd-180","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["181","4.19.38.1","nxr_1_Batteryagingcoefficient","1号UPS 电池老化系数","1","0","0","1","0","cmd-181","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["182","4.19.38.1","nxr_1_Batterytemperature","1号UPS 电池温度","1","0","0","1","0","cmd-182","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["183","4.19.38.1","nxr_1_Environmenttemperature","1号UPS 环境温度","1","0","0","1","0","cmd-183","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","4.19.38.1","nxr_1_Communications","1号UPS通信状态","1000","0","0","1","0",null,null,"0","60","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","26",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
[]
["1","4.19.38.2","nxr_2_Aphaseinputvoltage","2号UPS A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.38.2","nxr_2_Bphaseinputvoltage","2号UPS B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.38.2","nxr_2_PhaseCinputvoltage","2号UPS C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.38.2","nxr_2_Aphaseoutputvoltage","2号UPS A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.38.2","nxr_2_Bphaseoutputvoltage","2号UPS B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.38.2","nxr_2_Cphaseoutputvoltage","2号UPS C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.38.2","nxr_2_Aphaseoutputcurrent","2号UPS A相输出电流","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.38.2","nxr_2_Bphaseoutputcurrent","2号UPS B相输出电流","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.38.2","nxr_2_PhaseCoutputcurrent","2号UPS C相输出电流","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.38.2","nxr_2_BatteryPack1voltage","2号UPS 电池组1电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.38.2","nxr_2_Outputfrequency","2号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.38.2","nxr_2_BatteryPack2voltage","2号UPS 电池组2电压","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.38.2","nxr_2_Thisrackispowersupplymode","2号UPS 本机架供电方式","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","1,2,233,","01:UPS供电,02:旁路供电,E9:均不供电,"]
["18","4.19.38.2","nxr_2_BatPack1Selftest","2号UPS 电池组1电池自检","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["19","4.19.38.2","nxr_2_BatPack1Charge","2号UPS 电池组1均充/浮充状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["20","4.19.38.2","nxr_2_Themachineturnsonoffthephone","2号UPS 整机开机/关机","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:关机,E1:开机,"]
["21","4.19.38.2","nxr_2_Rectifierpowersupplycondition","2号UPS 整流器供电状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","4","224,225,226,227,","E0:主路逆变供电,E1:电池逆变供电,E2:联合逆变供电,E3:整流电池均不供电,"]
["22","4.19.38.2","nxr_2_Thegeneratorswitchonevents","2号UPS 整机发电机接入事件","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:发电机接入,E1:发电机没接入,"]
["23","4.19.38.2","nxr_2_Theinputemptyopenposition","2号UPS 整机输入空开状态","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["24","4.19.38.2","nxr_2_Themachinemaintenancebypassemptyopenposition","2号UPS 整机维修旁路空开状态","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["25","4.19.38.2","nxr_2_Thebypassemptyopenposition","2号UPS 整机旁路空开状态","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["26","4.19.38.2","nxr_2_Theoutputemptyopenposition","2号UPS 整机输出空开状态","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["27","4.19.38.2","nxr_2_Therotatingemptyopenposition","2号UPS 整机旋转空开状态","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["28","4.19.38.2","nxr_2_Framesystemcurrentsupplystateweaver","2号UPS 机架并机系统供电状态","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","6","224,225,226,227,228,229,","E0:均不供电,E1:旁路供电,E2:市电供电,E3:电池逆变供电,E4:联合供电,E5:输出禁止,"]
["29","4.19.38.2","nxr_2_BatPack2Selftest","2号UPS 电池组2电池自检","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["30","4.19.38.2","nxr_2_BatPack2Charge","2号UPS 电池组2浮充/均充状态","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["31","4.19.38.2","nxr_2_Module1onlinestatus","2号UPS 模块1在线状态","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["32","4.19.38.2","nxr_2_Module2onlinestatus","2号UPS 模块2在线状态","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["33","4.19.38.2","nxr_2_Module3onlinestatus","2号UPS 模块3在线状态","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["34","4.19.38.2","nxr_2_Module4onlinestatus","2号UPS 模块4在线状态","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["35","4.19.38.2","nxr_2_Module5onlinestatus","2号UPS 模块5在线状态","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["36","4.19.38.2","nxr_2_Module6onlinestatus","2号UPS 模块6在线状态","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["37","4.19.38.2","nxr_2_Module7onlinestatus","2号UPS 模块7在线状态","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["38","4.19.38.2","nxr_2_Module8onlinestatus","2号UPS 模块8在线状态","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["39","4.19.38.2","nxr_2_Module9onlinestatus","2号UPS 模块9在线状态","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["40","4.19.38.2","nxr_2_Module10onlinestatus","2号UPS 模块10在线状态","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["41","4.19.38.2","nxr_2_Invertersynchronousnosynchronization","2号UPS 逆变器同步/不同步","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","3,","03:不同步,"]
["42","4.19.38.2","nxr_2_Massiveabnormalvoltage","2号UPS 主路电压异常","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["43","4.19.38.2","nxr_2_rectifier","2号UPS 整流器","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["44","4.19.38.2","nxr_2_inverter","2号UPS 逆变器","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["45","4.19.38.2","nxr_2_Bypassstate","2号UPS 旁路状态","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["46","4.19.38.2","nxr_2_Batterystate1","2号UPS 电池组1状态","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","5","240,241,242,243,244,","F0:低于下限(关机点),F1:高于上限(电压过高),F2:电池无,F3:预告警,F4:电池接反,"]
["49","4.19.38.2","nxr_2_Powermodule1fault","2号UPS 功率模块1故障","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["50","4.19.38.2","nxr_2_Powermodule2fault","2号UPS 功率模块2故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["51","4.19.38.2","nxr_2_Powermodule3fault","2号UPS 功率模块3故障","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["52","4.19.38.2","nxr_2_Powermodule4fault","2号UPS 功率模块4故障","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["53","4.19.38.2","nxr_2_Powermodule5fault","2号UPS 功率模块5故障","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["54","4.19.38.2","nxr_2_Powermodule6fault","2号UPS 功率模块6故障","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["55","4.19.38.2","nxr_2_Powermodule7fault","2号UPS 功率模块7故障","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["56","4.19.38.2","nxr_2_Powermodule8fault","2号UPS 功率模块8故障","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["57","4.19.38.2","nxr_2_Powermodule9fault","2号UPS 功率模块9故障","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["58","4.19.38.2","nxr_2_Powermodule10fault","2号UPS 功率模块10故障","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["59","4.19.38.2","nxr_2_AbnormalLBS","2号UPS LBS异常","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["60","4.19.38.2","nxr_2_Thekeyboardboardfailureormachinecapacityisinvalid","2号UPS 键盘板故障或机型容量无效","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:键盘板故障,F1:机型容量无效,"]
["61","4.19.38.2","nxr_2_Fanfault","2号UPS 风扇故障","1","0","0","1","0","cmd-61","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["62","4.19.38.2","nxr_2_Environmentaltemperatureistoohigh","2号UPS 环境温度过高","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["63","4.19.38.2","nxr_2_Emergencyshutdown","2号UPS 紧急关机","1","0","0","1","0","cmd-63","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:紧急关机,"]
["64","4.19.38.2","nxr_2_Bypassthyristorfault","2号UPS 旁路晶闸管故障","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["65","4.19.38.2","nxr_2_Bypassthesequence","2号UPS 旁路相序反","1","0","0","1","0","cmd-65","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["66","4.19.38.2","nxr_2_Bypasstheflowfault","2号UPS 旁路过流故障","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["67","4.19.38.2","nxr_2_Bypassabnormalshutdown","2号UPS 旁路异常关机","1","0","0","1","0","cmd-67","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["68","4.19.38.2","nxr_2_Bypassswitchingtimesrestrictions","2号UPS 旁路切换次数限制","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["69","4.19.38.2","nxr_2_Theweavermoduleboardfailure","2号UPS 模块并机板故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["70","4.19.38.2","nxr_2_Modulelinefaultweaver","2号UPS 模块并机线连接故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["71","4.19.38.2","nxr_2_Theweavermodulecommunicationfault","2号UPS 模块并机通信故障","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["72","4.19.38.2","nxr_2_Auxiliarypower2offelectricity","2号UPS 辅助电源2掉电","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["73","4.19.38.2","nxr_2_Contactpowerboard1fault","2号UPS 接触电源板1故障","1","0","0","1","0","cmd-73","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["74","4.19.38.2","nxr_2_Contactpowerboard2fault","2号UPS 接触电源板2故障","1","0","0","1","0","cmd-74","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["75","4.19.38.2","nxr_2_Redundancyfanpowerfailure","2号UPS 冗余风扇电源故障","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["76","4.19.38.2","nxr_2_BCBaccess","2号UPS BCB接入情况","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","00:BCB未接入,F0:BCB闭合,"]
["77","4.19.38.2","nxr_2_Batterypacks1contactorfault","2号UPS 电池组1接触器故障","1","0","0","1","0","cmd-77","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["78","4.19.38.2","nxr_2_Batterypacks2contactorfault","2号UPS 电池组2接触器故障","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["79","4.19.38.2","nxr_2_Batterypacks1switchfault","2号UPS 电池组1交换器故障","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["80","4.19.38.2","nxr_2_Batterypacks2switchfault","2号UPS 电池组2交换器故障","1","0","0","1","0","cmd-80","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["81","4.19.38.2","nxr_2_Batterypacks1switchtheflow","2号UPS 电池组1交换器过流","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["82","4.19.38.2","nxr_2_Batterypacks2switchtheflow","2号UPS 电池组2交换器过流","1","0","0","1","0","cmd-82","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["83","4.19.38.2","nxr_2_Batterypacks1switchthermal","2号UPS 电池组1交换器过温","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["84","4.19.38.2","nxr_2_Batterypacks2switchthermal","2号UPS 电池组2交换器过温","1","0","0","1","0","cmd-84","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["85","4.19.38.2","nxr_2_1thebatterychargerfault","2号UPS 电池组1充电器故障","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["86","4.19.38.2","nxr_2_2thebatterychargerfault","2号UPS 电池组2充电器故障","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["87","4.19.38.2","nxr_2_Batterylife1","2号UPS 电池组1寿命情况","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["88","4.19.38.2","nxr_2_Batterylife2","2号UPS 电池组2寿命情况","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["89","4.19.38.2","nxr_2_Batterypacks1temperaturewastoohigh","2号UPS 电池组1温度过高","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["90","4.19.38.2","nxr_2_Batterypacks2temperaturewastoohigh","2号UPS 电池组2温度过高","1","0","0","1","0","cmd-90","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["91","4.19.38.2","nxr_2_Batterypacks1groundfault","2号UPS 电池组1接地故障","1","0","0","1","0","cmd-91","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["92","4.19.38.2","nxr_2_Batterypacks2groundfault","2号UPS 电池组2接地故障","1","0","0","1","0","cmd-92","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["93","4.19.38.2","nxr_2_Massiveunusualfrequency","2号UPS 主路频率异常","1","0","0","1","0","cmd-93","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["94","4.19.38.2","nxr_2_Balanceinductancethermal","2号UPS 平衡电感过温","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["95","4.19.38.2","nxr_2_Inputinductancethermal","2号UPS 输入电感过温","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["96","4.19.38.2","nxr_2_Rectifierthermal","2号UPS 整流器过温","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["97","4.19.38.2","nxr_2_Balancecircuitfault","2号UPS 平衡电路故障","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["98","4.19.38.2","nxr_2_Balanceelectricitypassbyflow","2号UPS 平衡电路过流","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["99","4.19.38.2","nxr_2_Meltbrokenwirerunning","2号UPS 主路熔丝断","1","0","0","1","0","cmd-99","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["100","4.19.38.2","nxr_2_1theauxiliarypoweroff","2号UPS 辅助电源1掉电","1","0","0","1","0","cmd-100","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["101","4.19.38.2","nxr_2_Sequencerunningagainst","2号UPS 主路相序反","1","0","0","1","0","cmd-101","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["102","4.19.38.2","nxr_2_Rectifierflow","2号UPS 整流器过流","1","0","0","1","0","cmd-102","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["103","4.19.38.2","nxr_2_Softstartupfailure","2号UPS 软启动失败","1","0","0","1","0","cmd-103","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["104","4.19.38.2","nxr_2_Inverterinductancethermal","2号UPS 逆变电感过温","1","0","0","1","0","cmd-104","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["105","4.19.38.2","nxr_2_Inverterthermal","2号UPS 逆变器过温","1","0","0","1","0","cmd-105","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["106","4.19.38.2","nxr_2_Thethyristorinverterfault","2号UPS 逆变器晶闸管故障","1","0","0","1","0","cmd-106","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["107","4.19.38.2","nxr_2_Theuseroperationerror","2号UPS 用户操作错误","1","0","0","1","0","cmd-107","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:错误,"]
["108","4.19.38.2","nxr_2_Outputmeltsilkbroken","2号UPS 输出熔丝断","1","0","0","1","0","cmd-108","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["109","4.19.38.2","nxr_2_Monolithicoutputoverload","2号UPS 单片输出过载","1","0","0","1","0","cmd-109","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["110","4.19.38.2","nxr_2_Expertsystemoverload","2号UPS 并机系统过载","1","0","0","1","0","cmd-110","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["111","4.19.38.2","nxr_2_Singleoverloadovertime","2号UPS 单机过载超时","1","0","0","1","0","cmd-111","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载超时,"]
["112","4.19.38.2","nxr_2_Acoutputpressure","2号UPS 交流输出过压","1","0","0","1","0","cmd-112","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过压,"]
["113","4.19.38.2","nxr_2_Inverterflow","2号UPS 逆变器过流","1","0","0","1","0","cmd-113","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["114","4.19.38.2","nxr_2_Impactloadtobypass","2号UPS 负载冲击转旁路","1","0","0","1","0","cmd-114","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["115","4.19.38.2","nxr_2_Allflowweaverfault","2号UPS 并机均流故障","1","0","0","1","0","cmd-115","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["116","4.19.38.2","nxr_2_Busabnormalshutdown","2号UPS 母线异常关机","1","0","0","1","0","cmd-116","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["117","4.19.38.2","nxr_2_Adjacenttobypassmachinerequest","2号UPS 邻机请求转旁路","1","0","0","1","0","cmd-117","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["118","4.19.38.2","nxr_2_Dcbusovervoltagefault","2号UPS 直流母线过压故障","1","0","0","1","0","cmd-118","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["119","4.19.38.2","nxr_2_Rectifiercommunicationfault","2号UPS 整流通信故障","1","0","0","1","0","cmd-119","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["120","4.19.38.2","nxr_2_Invertercommunicationfailures","2号UPS 逆变通讯故障","1","0","0","1","0","cmd-120","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["121","4.19.38.2","nxr_2_Outputdccomponentfaulttoo","2号UPS 输出直流分量过大故障","1","0","0","1","0","cmd-121","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["122","4.19.38.2","nxr_2_Expertsystembatteryforecastpfault","2号UPS 并机系统电池预告警故障","1","0","0","1","0","cmd-122","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["123","4.19.38.2","nxr_2_Inputlackofzerofault","2号UPS 输入缺零故障","1","0","0","1","0","cmd-123","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["124","4.19.38.2","nxr_2_Invertercontactorfault","2号UPS 逆变接触器故障","1","0","0","1","0","cmd-124","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["125","4.19.38.2","nxr_2_Inputcontactorfault","2号UPS 输入接触器故障","1","0","0","1","0","cmd-125","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["126","4.19.38.2","nxr_2_Inputcurrentabnormal","2号UPS 输入电流异常","1","0","0","1","0","cmd-126","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["127","4.19.38.2","nxr_2_Outputabnormalvoltage","2号UPS 输出电压异常","1","0","0","1","0","cmd-127","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["130","4.19.38.2","nxr_2_AcinputlinevoltageAB","2号UPS 交流输入线电压AB","1","0","0","1","0","cmd-130","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["131","4.19.38.2","nxr_2_AcinputlinevoltageBC","2号UPS 交流输入线电压BC","1","0","0","1","0","cmd-131","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["132","4.19.38.2","nxr_2_AcinputlinevoltageCA","2号UPS 交流输入线电压CA","1","0","0","1","0","cmd-132","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["133","4.19.38.2","nxr_2_Aphaseinputcurrent","2号UPS A相输入电流","1","0","0","1","0","cmd-133","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["134","4.19.38.2","nxr_2_Bphaseinputcurrent","2号UPS B相输入电流","1","0","0","1","0","cmd-134","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["135","4.19.38.2","nxr_2_CPhaseinputcurrent","2号UPS C相输入电流","1","0","0","1","0","cmd-135","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["136","4.19.38.2","nxr_2_Inputfrequency","2号UPS 输入频率","1","0","0","1","0","cmd-136","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["137","4.19.38.2","nxr_2_Aphaseinputpowerfactor","2号UPS A相输入功率因数","1","0","0","1","0","cmd-137","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["138","4.19.38.2","nxr_2_Bphaseinputpowerfactor","2号UPS B相输入功率因数","1","0","0","1","0","cmd-138","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["139","4.19.38.2","nxr_2_Cphaseinputpowerfactor","2号UPS C相输入功率因数","1","0","0","1","0","cmd-139","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["140","4.19.38.2","nxr_2_Aphasebypassvoltage","2号UPS A相旁路电压","1","0","0","1","0","cmd-140","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["141","4.19.38.2","nxr_2_Bphasebypassvoltage","2号UPS B相旁路电压","1","0","0","1","0","cmd-141","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["142","4.19.38.2","nxr_2_CPhasebypassvoltage","2号UPS C相旁路电压","1","0","0","1","0","cmd-142","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["143","4.19.38.2","nxr_2_Bypassfrequency","2号UPS 旁路频率","1","0","0","1","0","cmd-143","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["146","4.19.38.2","nxr_2_Aphaseoutputpowerfactor","2号UPS A相输出功率因数","1","0","0","1","0","cmd-146","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["147","4.19.38.2","nxr_2_Bphaseoutputpowerfactor","2号UPS B相输出功率因数","1","0","0","1","0","cmd-147","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["148","4.19.38.2","nxr_2_Cphaseoutputpowerfactor","2号UPS C相输出功率因数","1","0","0","1","0","cmd-148","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["149","4.19.38.2","nxr_2_Aphaseoutputthanpeak","2号UPS A相输出峰值比","1","0","0","1","0","cmd-149","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["150","4.19.38.2","nxr_2_Bphaseoutputthanpeak","2号UPS B相输出峰值比","1","0","0","1","0","cmd-150","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["151","4.19.38.2","nxr_2_Cphaseoutputthanpeak","2号UPS C相输出峰值比","1","0","0","1","0","cmd-151","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["152","4.19.38.2","nxr_2_Aphaseoutputactivepower","2号UPS A相输出有功功率","1","0","0","1","0","cmd-152","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["153","4.19.38.2","nxr_2_Bphaseoutputactivepower","2号UPS B相输出有功功率","1","0","0","1","0","cmd-153","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["154","4.19.38.2","nxr_2_Cphaseoutputactivepower","2号UPS C相输出有功功率","1","0","0","1","0","cmd-154","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["155","4.19.38.2","nxr_2_Aphaseoutputreactivepower","2号UPS A相输出无功功率","1","0","0","1","0","cmd-155","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["156","4.19.38.2","nxr_2_Bphaseoutputreactivepower","2号UPS B相输出无功功率","1","0","0","1","0","cmd-156","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["157","4.19.38.2","nxr_2_Cphaseoutputreactivepower","2号UPS C相输出无功功率","1","0","0","1","0","cmd-157","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["158","4.19.38.2","nxr_2_Aphaseoutputpowerinstalled","2号UPS A相输出视在功率","1","0","0","1","0","cmd-158","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["159","4.19.38.2","nxr_2_Bphaseoutputpowerinstalled","2号UPS B相输出视在功率","1","0","0","1","0","cmd-159","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["160","4.19.38.2","nxr_2_Cphaseoutputpowerinstalled","2号UPS C相输出视在功率","1","0","0","1","0","cmd-160","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["161","4.19.38.2","nxr_2_Aphaseoutputloadpercentage","2号UPS A相输出负载百分比","1","0","0","1","0","cmd-161","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["162","4.19.38.2","nxr_2_Bphaseoutputloadpercentage","2号UPS B相输出负载百分比","1","0","0","1","0","cmd-162","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["163","4.19.38.2","nxr_2_Cphaseoutputloadpercentage","2号UPS C相输出负载百分比","1","0","0","1","0","cmd-163","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["165","4.19.38.2","nxr_2_SystemAphaseoutputactivepower","2号UPS 系统A相输出有功功率","1","0","0","1","0","cmd-165","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["166","4.19.38.2","nxr_2_SystemBphaseoutputactivepower","2号UPS 系统B相输出有功功率","1","0","0","1","0","cmd-166","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["167","4.19.38.2","nxr_2_SystemCphaseoutputactivepower","2号UPS 系统C相输出有功功率","1","0","0","1","0","cmd-167","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["168","4.19.38.2","nxr_2_SysteminstalledAphaseoutputpower","2号UPS 系统A相输出视在功率","1","0","0","1","0","cmd-168","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["169","4.19.38.2","nxr_2_SysteminstalledBphaseoutputpower","2号UPS 系统B相输出视在功率","1","0","0","1","0","cmd-169","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["170","4.19.38.2","nxr_2_SysteminstalledCphaseoutputpower","2号UPS 系统C相输出视在功率","1","0","0","1","0","cmd-170","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["171","4.19.38.2","nxr_2_SystemAphaseoutputreactivepower","2号UPS 系统A相输出无功功率","1","0","0","1","0","cmd-171","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["172","4.19.38.2","nxr_2_SystemBphaseoutputreactivepower","2号UPS 系统B相输出无功功率","1","0","0","1","0","cmd-172","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["173","4.19.38.2","nxr_2_SystemCphaseoutputreactivepower","2号UPS 系统C相输出无功功率","1","0","0","1","0","cmd-173","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["176","4.19.38.2","nxr_2_Batterybackuptime","2号UPS 电池后备时间","1","0","0","1","0","cmd-176","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["177","4.19.38.2","nxr_2_Arebatteryvoltage","2号UPS 正电池电压","1","0","0","1","0","cmd-177","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["178","4.19.38.2","nxr_2_Arebatteryelectriccurrent","2号UPS 正电池电流","1","0","0","1","0","cmd-178","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["179","4.19.38.2","nxr_2_Negativebatteryvoltage","2号UPS 负电池电压","1","0","0","1","0","cmd-179","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["180","4.19.38.2","nxr_2_Negativebatteryelectriccurrent","2号UPS 负电池电流","1","0","0","1","0","cmd-180","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["181","4.19.38.2","nxr_2_Batteryagingcoefficient","2号UPS 电池老化系数","1","0","0","1","0","cmd-181","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["182","4.19.38.2","nxr_2_Batterytemperature","2号UPS 电池温度","1","0","0","1","0","cmd-182","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["183","4.19.38.2","nxr_2_Environmenttemperature","2号UPS 环境温度","1","0","0","1","0","cmd-183","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","4.19.38.2","nxr_2_Communications","2号UPS通信状态","1000","0","0","1","0",null,null,"0","60","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","26",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":343,"n_cols":76,"rows_kept":343,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.38.1","nxr_1_Aphaseinputvoltage","1号UPS A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.38.1","nxr_1_Bphaseinputvoltage","1号UPS B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.38.1","nxr_1_PhaseCinputvoltage","1号UPS C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.38.1","nxr_1_Aphaseoutputvoltage","1号UPS A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.38.1","nxr_1_Bphaseoutputvoltage","1号UPS B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.38.1","nxr_1_Cphaseoutputvoltage","1号UPS C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.38.1","nxr_1_Aphaseoutputcurrent","1号UPS A相输出电流","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.38.1","nxr_1_Bphaseoutputcurrent","1号UPS B相输出电流","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.38.1","nxr_1_PhaseCoutputcurrent","1号UPS C相输出电流","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.38.1","nxr_1_BatteryPack1voltage","1号UPS 电池组1电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.38.1","nxr_1_Outputfrequency","1号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.38.1","nxr_1_BatteryPack2voltage","1号UPS 电池组2电压","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.38.1","nxr_1_Thisrackispowersupplymode","1号UPS 本机架供电方式","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","1,2,233,","01:UPS供电,02:旁路供电,E9:均不供电,"]
["18","4.19.38.1","nxr_1_BatPack1Selftest","1号UPS 电池组1电池自检","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["19","4.19.38.1","nxr_1_BatPack1Charge","1号UPS 电池组1均充/浮充状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["20","4.19.38.1","nxr_1_Themachineturnsonoffthephone","1号UPS 整机开机/关机","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","224,","E0:关机,"]
["21","4.19.38.1","nxr_1_Rectifierpowersupplycondition","1号UPS 整流器供电状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","4","224,225,226,227,","E0:主路逆变供电,E1:电池逆变供电,E2:联合逆变供电,E3:整流电池均不供电,"]
["22","4.19.38.1","nxr_1_Thegeneratorswitchonevents","1号UPS 整机发电机接入事件","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:发电机接入,E1:发电机没接入,"]
["23","4.19.38.1","nxr_1_Theinputemptyopenposition","1号UPS 整机输入空开状态","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["24","4.19.38.1","nxr_1_Themachinemaintenancebypassemptyopenposition","1号UPS 整机维修旁路空开状态","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["25","4.19.38.1","nxr_1_Thebypassemptyopenposition","1号UPS 整机旁路空开状态","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["26","4.19.38.1","nxr_1_Theoutputemptyopenposition","1号UPS 整机输出空开状态","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["27","4.19.38.1","nxr_1_Therotatingemptyopenposition","1号UPS 整机旋转空开状态","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["28","4.19.38.1","nxr_1_Framesystemcurrentsupplystateweaver","1号UPS 机架并机系统供电状态","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","6","224,225,226,227,228,229,","E0:均不供电,E1:旁路供电,E2:市电供电,E3:电池逆变供电,E4:联合供电,E5:输出禁止,"]
["29","4.19.38.1","nxr_1_BatPack2Selftest","1号UPS 电池组2电池自检","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["30","4.19.38.1","nxr_1_BatPack2Charge","1号UPS 电池组2浮充/均充状态","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["31","4.19.38.1","nxr_1_Module1onlinestatus","1号UPS 模块1在线状态","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["32","4.19.38.1","nxr_1_Module2onlinestatus","1号UPS 模块2在线状态","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["33","4.19.38.1","nxr_1_Module3onlinestatus","1号UPS 模块3在线状态","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["34","4.19.38.1","nxr_1_Module4onlinestatus","1号UPS 模块4在线状态","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["35","4.19.38.1","nxr_1_Module5onlinestatus","1号UPS 模块5在线状态","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["36","4.19.38.1","nxr_1_Module6onlinestatus","1号UPS 模块6在线状态","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["37","4.19.38.1","nxr_1_Module7onlinestatus","1号UPS 模块7在线状态","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["38","4.19.38.1","nxr_1_Module8onlinestatus","1号UPS 模块8在线状态","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["39","4.19.38.1","nxr_1_Module9onlinestatus","1号UPS 模块9在线状态","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["40","4.19.38.1","nxr_1_Module10onlinestatus","1号UPS 模块10在线状态","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["41","4.19.38.1","nxr_1_Invertersynchronousnosynchronization","1号UPS 逆变器同步/不同步","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","3,","03:不同步,"]
["42","4.19.38.1","nxr_1_Massiveabnormalvoltage","1号UPS 主路电压异常","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["43","4.19.38.1","nxr_1_rectifier","1号UPS 整流器","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["44","4.19.38.1","nxr_1_inverter","1号UPS 逆变器","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["45","4.19.38.1","nxr_1_Bypassstate","1号UPS 旁路状态","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["46","4.19.38.1","nxr_1_Batterystate1","1号UPS 电池组1状态","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","5","240,241,242,243,244,","F0:低于下限(关机点),F1:高于上限(电压过高),F2:电池无,F3:预告警,F4:电池接反,"]
["49","4.19.38.1","nxr_1_Powermodule1fault","1号UPS 功率模块1故障","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["50","4.19.38.1","nxr_1_Powermodule2fault","1号UPS 功率模块2故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["51","4.19.38.1","nxr_1_Powermodule3fault","1号UPS 功率模块3故障","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["52","4.19.38.1","nxr_1_Powermodule4fault","1号UPS 功率模块4故障","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["53","4.19.38.1","nxr_1_Powermodule5fault","1号UPS 功率模块5故障","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["54","4.19.38.1","nxr_1_Powermodule6fault","1号UPS 功率模块6故障","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["55","4.19.38.1","nxr_1_Powermodule7fault","1号UPS 功率模块7故障","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["56","4.19.38.1","nxr_1_Powermodule8fault","1号UPS 功率模块8故障","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["57","4.19.38.1","nxr_1_Powermodule9fault","1号UPS 功率模块9故障","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["58","4.19.38.1","nxr_1_Powermodule10fault","1号UPS 功率模块10故障","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["59","4.19.38.1","nxr_1_AbnormalLBS","1号UPS LBS异常","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["60","4.19.38.1","nxr_1_Thekeyboardboardfailureormachinecapacityisinvalid","1号UPS 键盘板故障或机型容量无效","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:键盘板故障,F1:机型容量无效,"]
["61","4.19.38.1","nxr_1_Fanfault","1号UPS 风扇故障","1","0","0","1","0","cmd-61","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["62","4.19.38.1","nxr_1_Environmentaltemperatureistoohigh","1号UPS 环境温度过高","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["63","4.19.38.1","nxr_1_Emergencyshutdown","1号UPS 紧急关机","1","0","0","1","0","cmd-63","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:紧急关机,"]
["64","4.19.38.1","nxr_1_Bypassthyristorfault","1号UPS 旁路晶闸管故障","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["65","4.19.38.1","nxr_1_Bypassthesequence","1号UPS 旁路相序反","1","0","0","1","0","cmd-65","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["66","4.19.38.1","nxr_1_Bypasstheflowfault","1号UPS 旁路过流故障","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["67","4.19.38.1","nxr_1_Bypassabnormalshutdown","1号UPS 旁路异常关机","1","0","0","1","0","cmd-67","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["68","4.19.38.1","nxr_1_Bypassswitchingtimesrestrictions","1号UPS 旁路切换次数限制","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["69","4.19.38.1","nxr_1_Theweavermoduleboardfailure","1号UPS 模块并机板故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["70","4.19.38.1","nxr_1_Modulelinefaultweaver","1号UPS 模块并机线连接故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["71","4.19.38.1","nxr_1_Theweavermodulecommunicationfault","1号UPS 模块并机通信故障","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["72","4.19.38.1","nxr_1_Auxiliarypower2offelectricity","1号UPS 辅助电源2掉电","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["73","4.19.38.1","nxr_1_Contactpowerboard1fault","1号UPS 接触电源板1故障","1","0","0","1","0","cmd-73","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["74","4.19.38.1","nxr_1_Contactpowerboard2fault","1号UPS 接触电源板2故障","1","0","0","1","0","cmd-74","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["75","4.19.38.1","nxr_1_Redundancyfanpowerfailure","1号UPS 冗余风扇电源故障","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["76","4.19.38.1","nxr_1_BCBaccess","1号UPS BCB接入情况","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","00:BCB未接入,F0:BCB闭合,"]
["77","4.19.38.1","nxr_1_Batterypacks1contactorfault","1号UPS 电池组1接触器故障","1","0","0","1","0","cmd-77","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["78","4.19.38.1","nxr_1_Batterypacks2contactorfault","1号UPS 电池组2接触器故障","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["79","4.19.38.1","nxr_1_Batterypacks1switchfault","1号UPS 电池组1交换器故障","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["80","4.19.38.1","nxr_1_Batterypacks2switchfault","1号UPS 电池组2交换器故障","1","0","0","1","0","cmd-80","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["81","4.19.38.1","nxr_1_Batterypacks1switchtheflow","1号UPS 电池组1交换器过流","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["82","4.19.38.1","nxr_1_Batterypacks2switchtheflow","1号UPS 电池组2交换器过流","1","0","0","1","0","cmd-82","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["83","4.19.38.1","nxr_1_Batterypacks1switchthermal","1号UPS 电池组1交换器过温","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["84","4.19.38.1","nxr_1_Batterypacks2switchthermal","1号UPS 电池组2交换器过温","1","0","0","1","0","cmd-84","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["85","4.19.38.1","nxr_1_1thebatterychargerfault","1号UPS 电池组1充电器故障","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["86","4.19.38.1","nxr_1_2thebatterychargerfault","1号UPS 电池组2充电器故障","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["87","4.19.38.1","nxr_1_Batterylife1","1号UPS 电池组1寿命情况","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["88","4.19.38.1","nxr_1_Batterylife2","1号UPS 电池组2寿命情况","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["89","4.19.38.1","nxr_1_Batterypacks1temperaturewastoohigh","1号UPS 电池组1温度过高","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["90","4.19.38.1","nxr_1_Batterypacks2temperaturewastoohigh","1号UPS 电池组2温度过高","1","0","0","1","0","cmd-90","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["91","4.19.38.1","nxr_1_Batterypacks1groundfault","1号UPS 电池组1接地故障","1","0","0","1","0","cmd-91","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["92","4.19.38.1","nxr_1_Batterypacks2groundfault","1号UPS 电池组2接地故障","1","0","0","1","0","cmd-92","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["93","4.19.38.1","nxr_1_Massiveunusualfrequency","1号UPS 主路频率异常","1","0","0","1","0","cmd-93","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["94","4.19.38.1","nxr_1_Balanceinductancethermal","1号UPS 平衡电感过温","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["95","4.19.38.1","nxr_1_Inputinductancethermal","1号UPS 输入电感过温","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["96","4.19.38.1","nxr_1_Rectifierthermal","1号UPS 整流器过温","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["97","4.19.38.1","nxr_1_Balancecircuitfault","1号UPS 平衡电路故障","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["98","4.19.38.1","nxr_1_Balanceelectricitypassbyflow","1号UPS 平衡电路过流","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["99","4.19.38.1","nxr_1_Meltbrokenwirerunning","1号UPS 主路熔丝断","1","0","0","1","0","cmd-99","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["100","4.19.38.1","nxr_1_1theauxiliarypoweroff","1号UPS 辅助电源1掉电","1","0","0","1","0","cmd-100","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["101","4.19.38.1","nxr_1_Sequencerunningagainst","1号UPS 主路相序反","1","0","0","1","0","cmd-101","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["102","4.19.38.1","nxr_1_Rectifierflow","1号UPS 整流器过流","1","0","0","1","0","cmd-102","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["103","4.19.38.1","nxr_1_Softstartupfailure","1号UPS 软启动失败","1","0","0","1","0","cmd-103","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["104","4.19.38.1","nxr_1_Inverterinductancethermal","1号UPS 逆变电感过温","1","0","0","1","0","cmd-104","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["105","4.19.38.1","nxr_1_Inverterthermal","1号UPS 逆变器过温","1","0","0","1","0","cmd-105","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["106","4.19.38.1","nxr_1_Thethyristorinverterfault","1号UPS 逆变器晶闸管故障","1","0","0","1","0","cmd-106","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["107","4.19.38.1","nxr_1_Theuseroperationerror","1号UPS 用户操作错误","1","0","0","1","0","cmd-107","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:错误,"]
["108","4.19.38.1","nxr_1_Outputmeltsilkbroken","1号UPS 输出熔丝断","1","0","0","1","0","cmd-108","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["109","4.19.38.1","nxr_1_Monolithicoutputoverload","1号UPS 单片输出过载","1","0","0","1","0","cmd-109","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["110","4.19.38.1","nxr_1_Expertsystemoverload","1号UPS 并机系统过载","1","0","0","1","0","cmd-110","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["111","4.19.38.1","nxr_1_Singleoverloadovertime","1号UPS 单机过载超时","1","0","0","1","0","cmd-111","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载超时,"]
["112","4.19.38.1","nxr_1_Acoutputpressure","1号UPS 交流输出过压","1","0","0","1","0","cmd-112","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过压,"]
["113","4.19.38.1","nxr_1_Inverterflow","1号UPS 逆变器过流","1","0","0","1","0","cmd-113","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["114","4.19.38.1","nxr_1_Impactloadtobypass","1号UPS 负载冲击转旁路","1","0","0","1","0","cmd-114","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["115","4.19.38.1","nxr_1_Allflowweaverfault","1号UPS 并机均流故障","1","0","0","1","0","cmd-115","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["116","4.19.38.1","nxr_1_Busabnormalshutdown","1号UPS 母线异常关机","1","0","0","1","0","cmd-116","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["117","4.19.38.1","nxr_1_Adjacenttobypassmachinerequest","1号UPS 邻机请求转旁路","1","0","0","1","0","cmd-117","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["118","4.19.38.1","nxr_1_Dcbusovervoltagefault","1号UPS 直流母线过压故障","1","0","0","1","0","cmd-118","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["119","4.19.38.1","nxr_1_Rectifiercommunicationfault","1号UPS 整流通信故障","1","0","0","1","0","cmd-119","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["120","4.19.38.1","nxr_1_Invertercommunicationfailures","1号UPS 逆变通讯故障","1","0","0","1","0","cmd-120","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["121","4.19.38.1","nxr_1_Outputdccomponentfaulttoo","1号UPS 输出直流分量过大故障","1","0","0","1","0","cmd-121","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["122","4.19.38.1","nxr_1_Expertsystembatteryforecastpfault","1号UPS 并机系统电池预告警故障","1","0","0","1","0","cmd-122","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["123","4.19.38.1","nxr_1_Inputlackofzerofault","1号UPS 输入缺零故障","1","0","0","1","0","cmd-123","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["124","4.19.38.1","nxr_1_Invertercontactorfault","1号UPS 逆变接触器故障","1","0","0","1","0","cmd-124","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["125","4.19.38.1","nxr_1_Inputcontactorfault","1号UPS 输入接触器故障","1","0","0","1","0","cmd-125","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["126","4.19.38.1","nxr_1_Inputcurrentabnormal","1号UPS 输入电流异常","1","0","0","1","0","cmd-126","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["127","4.19.38.1","nxr_1_Outputabnormalvoltage","1号UPS 输出电压异常","1","0","0","1","0","cmd-127","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["130","4.19.38.1","nxr_1_AcinputlinevoltageAB","1号UPS 交流输入线电压AB","1","0","0","1","0","cmd-130","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["131","4.19.38.1","nxr_1_AcinputlinevoltageBC","1号UPS 交流输入线电压BC","1","0","0","1","0","cmd-131","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["132","4.19.38.1","nxr_1_AcinputlinevoltageCA","1号UPS 交流输入线电压CA","1","0","0","1","0","cmd-132","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["133","4.19.38.1","nxr_1_Aphaseinputcurrent","1号UPS A相输入电流","1","0","0","1","0","cmd-133","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["134","4.19.38.1","nxr_1_Bphaseinputcurrent","1号UPS B相输入电流","1","0","0","1","0","cmd-134","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["135","4.19.38.1","nxr_1_CPhaseinputcurrent","1号UPS C相输入电流","1","0","0","1","0","cmd-135","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["136","4.19.38.1","nxr_1_Inputfrequency","1号UPS 输入频率","1","0","0","1","0","cmd-136","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["137","4.19.38.1","nxr_1_Aphaseinputpowerfactor","1号UPS A相输入功率因数","1","0","0","1","0","cmd-137","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["138","4.19.38.1","nxr_1_Bphaseinputpowerfactor","1号UPS B相输入功率因数","1","0","0","1","0","cmd-138","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["139","4.19.38.1","nxr_1_Cphaseinputpowerfactor","1号UPS C相输入功率因数","1","0","0","1","0","cmd-139","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["140","4.19.38.1","nxr_1_Aphasebypassvoltage","1号UPS A相旁路电压","1","0","0","1","0","cmd-140","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["141","4.19.38.1","nxr_1_Bphasebypassvoltage","1号UPS B相旁路电压","1","0","0","1","0","cmd-141","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["142","4.19.38.1","nxr_1_CPhasebypassvoltage","1号UPS C相旁路电压","1","0","0","1","0","cmd-142","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["143","4.19.38.1","nxr_1_Bypassfrequency","1号UPS 旁路频率","1","0","0","1","0","cmd-143","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["146","4.19.38.1","nxr_1_Aphaseoutputpowerfactor","1号UPS A相输出功率因数","1","0","0","1","0","cmd-146","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["147","4.19.38.1","nxr_1_Bphaseoutputpowerfactor","1号UPS B相输出功率因数","1","0","0","1","0","cmd-147","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["148","4.19.38.1","nxr_1_Cphaseoutputpowerfactor","1号UPS C相输出功率因数","1","0","0","1","0","cmd-148","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["149","4.19.38.1","nxr_1_Aphaseoutputthanpeak","1号UPS A相输出峰值比","1","0","0","1","0","cmd-149","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["150","4.19.38.1","nxr_1_Bphaseoutputthanpeak","1号UPS B相输出峰值比","1","0","0","1","0","cmd-150","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["151","4.19.38.1","nxr_1_Cphaseoutputthanpeak","1号UPS C相输出峰值比","1","0","0","1","0","cmd-151","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["152","4.19.38.1","nxr_1_Aphaseoutputactivepower","1号UPS A相输出有功功率","1","0","0","1","0","cmd-152","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["153","4.19.38.1","nxr_1_Bphaseoutputactivepower","1号UPS B相输出有功功率","1","0","0","1","0","cmd-153","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["154","4.19.38.1","nxr_1_Cphaseoutputactivepower","1号UPS C相输出有功功率","1","0","0","1","0","cmd-154","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["155","4.19.38.1","nxr_1_Aphaseoutputreactivepower","1号UPS A相输出无功功率","1","0","0","1","0","cmd-155","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["156","4.19.38.1","nxr_1_Bphaseoutputreactivepower","1号UPS B相输出无功功率","1","0","0","1","0","cmd-156","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["157","4.19.38.1","nxr_1_Cphaseoutputreactivepower","1号UPS C相输出无功功率","1","0","0","1","0","cmd-157","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["158","4.19.38.1","nxr_1_Aphaseoutputpowerinstalled","1号UPS A相输出视在功率","1","0","0","1","0","cmd-158","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["159","4.19.38.1","nxr_1_Bphaseoutputpowerinstalled","1号UPS B相输出视在功率","1","0","0","1","0","cmd-159","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["160","4.19.38.1","nxr_1_Cphaseoutputpowerinstalled","1号UPS C相输出视在功率","1","0","0","1","0","cmd-160","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["161","4.19.38.1","nxr_1_Aphaseoutputloadpercentage","1号UPS A相输出负载百分比","1","0","0","1","0","cmd-161","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["162","4.19.38.1","nxr_1_Bphaseoutputloadpercentage","1号UPS B相输出负载百分比","1","0","0","1","0","cmd-162","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["163","4.19.38.1","nxr_1_Cphaseoutputloadpercentage","1号UPS C相输出负载百分比","1","0","0","1","0","cmd-163","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["165","4.19.38.1","nxr_1_SystemAphaseoutputactivepower","1号UPS 系统A相输出有功功率","1","0","0","1","0","cmd-165","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["166","4.19.38.1","nxr_1_SystemBphaseoutputactivepower","1号UPS 系统B相输出有功功率","1","0","0","1","0","cmd-166","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["167","4.19.38.1","nxr_1_SystemCphaseoutputactivepower","1号UPS 系统C相输出有功功率","1","0","0","1","0","cmd-167","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["168","4.19.38.1","nxr_1_SysteminstalledAphaseoutputpower","1号UPS 系统A相输出视在功率","1","0","0","1","0","cmd-168","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["169","4.19.38.1","nxr_1_SysteminstalledBphaseoutputpower","1号UPS 系统B相输出视在功率","1","0","0","1","0","cmd-169","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["170","4.19.38.1","nxr_1_SysteminstalledCphaseoutputpower","1号UPS 系统C相输出视在功率","1","0","0","1","0","cmd-170","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["171","4.19.38.1","nxr_1_SystemAphaseoutputreactivepower","1号UPS 系统A相输出无功功率","1","0","0","1","0","cmd-171","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["172","4.19.38.1","nxr_1_SystemBphaseoutputreactivepower","1号UPS 系统B相输出无功功率","1","0","0","1","0","cmd-172","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["173","4.19.38.1","nxr_1_SystemCphaseoutputreactivepower","1号UPS 系统C相输出无功功率","1","0","0","1","0","cmd-173","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["176","4.19.38.1","nxr_1_Batterybackuptime","1号UPS 电池后备时间","1","0","0","1","0","cmd-176","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["177","4.19.38.1","nxr_1_Arebatteryvoltage","1号UPS 正电池电压","1","0","0","1","0","cmd-177","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["178","4.19.38.1","nxr_1_Arebatteryelectriccurrent","1号UPS 正电池电流","1","0","0","1","0","cmd-178","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["179","4.19.38.1","nxr_1_Negativebatteryvoltage","1号UPS 负电池电压","1","0","0","1","0","cmd-179","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["180","4.19.38.1","nxr_1_Negativebatteryelectriccurrent","1号UPS 负电池电流","1","0","0","1","0","cmd-180","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["181","4.19.38.1","nxr_1_Batteryagingcoefficient","1号UPS 电池老化系数","1","0","0","1","0","cmd-181","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["182","4.19.38.1","nxr_1_Batterytemperature","1号UPS 电池温度","1","0","0","1","0","cmd-182","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["183","4.19.38.1","nxr_1_Environmenttemperature","1号UPS 环境温度","1","0","0","1","0","cmd-183","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","4.19.38.1","nxr_1_Communications","1号UPS通信状态","1000","0","0","1","0",null,null,"0","60","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","26",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["1","4.19.38.2","nxr_2_Aphaseinputvoltage","2号UPS A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.38.2","nxr_2_Bphaseinputvoltage","2号UPS B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.38.2","nxr_2_PhaseCinputvoltage","2号UPS C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.38.2","nxr_2_Aphaseoutputvoltage","2号UPS A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.38.2","nxr_2_Bphaseoutputvoltage","2号UPS B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.38.2","nxr_2_Cphaseoutputvoltage","2号UPS C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.38.2","nxr_2_Aphaseoutputcurrent","2号UPS A相输出电流","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.38.2","nxr_2_Bphaseoutputcurrent","2号UPS B相输出电流","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.38.2","nxr_2_PhaseCoutputcurrent","2号UPS C相输出电流","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.38.2","nxr_2_BatteryPack1voltage","2号UPS 电池组1电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.38.2","nxr_2_Outputfrequency","2号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.38.2","nxr_2_BatteryPack2voltage","2号UPS 电池组2电压","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.38.2","nxr_2_Thisrackispowersupplymode","2号UPS 本机架供电方式","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","1,2,233,","01:UPS供电,02:旁路供电,E9:均不供电,"]
["18","4.19.38.2","nxr_2_BatPack1Selftest","2号UPS 电池组1电池自检","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["19","4.19.38.2","nxr_2_BatPack1Charge","2号UPS 电池组1均充/浮充状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["20","4.19.38.2","nxr_2_Themachineturnsonoffthephone","2号UPS 整机开机/关机","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:关机,E1:开机,"]
["21","4.19.38.2","nxr_2_Rectifierpowersupplycondition","2号UPS 整流器供电状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","4","224,225,226,227,","E0:主路逆变供电,E1:电池逆变供电,E2:联合逆变供电,E3:整流电池均不供电,"]
["22","4.19.38.2","nxr_2_Thegeneratorswitchonevents","2号UPS 整机发电机接入事件","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:发电机接入,E1:发电机没接入,"]
["23","4.19.38.2","nxr_2_Theinputemptyopenposition","2号UPS 整机输入空开状态","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["24","4.19.38.2","nxr_2_Themachinemaintenancebypassemptyopenposition","2号UPS 整机维修旁路空开状态","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["25","4.19.38.2","nxr_2_Thebypassemptyopenposition","2号UPS 整机旁路空开状态","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["26","4.19.38.2","nxr_2_Theoutputemptyopenposition","2号UPS 整机输出空开状态","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["27","4.19.38.2","nxr_2_Therotatingemptyopenposition","2号UPS 整机旋转空开状态","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:断开状态,E1:闭合状态,"]
["28","4.19.38.2","nxr_2_Framesystemcurrentsupplystateweaver","2号UPS 机架并机系统供电状态","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","6","224,225,226,227,228,229,","E0:均不供电,E1:旁路供电,E2:市电供电,E3:电池逆变供电,E4:联合供电,E5:输出禁止,"]
["29","4.19.38.2","nxr_2_BatPack2Selftest","2号UPS 电池组2电池自检","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:自检中,E1:没在自检,"]
["30","4.19.38.2","nxr_2_BatPack2Charge","2号UPS 电池组2浮充/均充状态","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","3","224,225,226,","E0:浮充,E1:均充,E2:非充电状态,"]
["31","4.19.38.2","nxr_2_Module1onlinestatus","2号UPS 模块1在线状态","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["32","4.19.38.2","nxr_2_Module2onlinestatus","2号UPS 模块2在线状态","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["33","4.19.38.2","nxr_2_Module3onlinestatus","2号UPS 模块3在线状态","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["34","4.19.38.2","nxr_2_Module4onlinestatus","2号UPS 模块4在线状态","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["35","4.19.38.2","nxr_2_Module5onlinestatus","2号UPS 模块5在线状态","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["36","4.19.38.2","nxr_2_Module6onlinestatus","2号UPS 模块6在线状态","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["37","4.19.38.2","nxr_2_Module7onlinestatus","2号UPS 模块7在线状态","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["38","4.19.38.2","nxr_2_Module8onlinestatus","2号UPS 模块8在线状态","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["39","4.19.38.2","nxr_2_Module9onlinestatus","2号UPS 模块9在线状态","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["40","4.19.38.2","nxr_2_Module10onlinestatus","2号UPS 模块10在线状态","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","224,225,","E0:在线,E1:不在线,"]
["41","4.19.38.2","nxr_2_Invertersynchronousnosynchronization","2号UPS 逆变器同步/不同步","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","3,","03:不同步,"]
["42","4.19.38.2","nxr_2_Massiveabnormalvoltage","2号UPS 主路电压异常","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["43","4.19.38.2","nxr_2_rectifier","2号UPS 整流器","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["44","4.19.38.2","nxr_2_inverter","2号UPS 逆变器","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["45","4.19.38.2","nxr_2_Bypassstate","2号UPS 旁路状态","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["46","4.19.38.2","nxr_2_Batterystate1","2号UPS 电池组1状态","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","5","240,241,242,243,244,","F0:低于下限(关机点),F1:高于上限(电压过高),F2:电池无,F3:预告警,F4:电池接反,"]
["49","4.19.38.2","nxr_2_Powermodule1fault","2号UPS 功率模块1故障","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["50","4.19.38.2","nxr_2_Powermodule2fault","2号UPS 功率模块2故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["51","4.19.38.2","nxr_2_Powermodule3fault","2号UPS 功率模块3故障","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["52","4.19.38.2","nxr_2_Powermodule4fault","2号UPS 功率模块4故障","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["53","4.19.38.2","nxr_2_Powermodule5fault","2号UPS 功率模块5故障","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["54","4.19.38.2","nxr_2_Powermodule6fault","2号UPS 功率模块6故障","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["55","4.19.38.2","nxr_2_Powermodule7fault","2号UPS 功率模块7故障","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["56","4.19.38.2","nxr_2_Powermodule8fault","2号UPS 功率模块8故障","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["57","4.19.38.2","nxr_2_Powermodule9fault","2号UPS 功率模块9故障","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["58","4.19.38.2","nxr_2_Powermodule10fault","2号UPS 功率模块10故障","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["59","4.19.38.2","nxr_2_AbnormalLBS","2号UPS LBS异常","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["60","4.19.38.2","nxr_2_Thekeyboardboardfailureormachinecapacityisinvalid","2号UPS 键盘板故障或机型容量无效","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:键盘板故障,F1:机型容量无效,"]
["61","4.19.38.2","nxr_2_Fanfault","2号UPS 风扇故障","1","0","0","1","0","cmd-61","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["62","4.19.38.2","nxr_2_Environmentaltemperatureistoohigh","2号UPS 环境温度过高","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["63","4.19.38.2","nxr_2_Emergencyshutdown","2号UPS 紧急关机","1","0","0","1","0","cmd-63","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:紧急关机,"]
["64","4.19.38.2","nxr_2_Bypassthyristorfault","2号UPS 旁路晶闸管故障","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["65","4.19.38.2","nxr_2_Bypassthesequence","2号UPS 旁路相序反","1","0","0","1","0","cmd-65","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["66","4.19.38.2","nxr_2_Bypasstheflowfault","2号UPS 旁路过流故障","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["67","4.19.38.2","nxr_2_Bypassabnormalshutdown","2号UPS 旁路异常关机","1","0","0","1","0","cmd-67","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:异常,"]
["68","4.19.38.2","nxr_2_Bypassswitchingtimesrestrictions","2号UPS 旁路切换次数限制","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["69","4.19.38.2","nxr_2_Theweavermoduleboardfailure","2号UPS 模块并机板故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["70","4.19.38.2","nxr_2_Modulelinefaultweaver","2号UPS 模块并机线连接故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["71","4.19.38.2","nxr_2_Theweavermodulecommunicationfault","2号UPS 模块并机通信故障","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["72","4.19.38.2","nxr_2_Auxiliarypower2offelectricity","2号UPS 辅助电源2掉电","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["73","4.19.38.2","nxr_2_Contactpowerboard1fault","2号UPS 接触电源板1故障","1","0","0","1","0","cmd-73","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["74","4.19.38.2","nxr_2_Contactpowerboard2fault","2号UPS 接触电源板2故障","1","0","0","1","0","cmd-74","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["75","4.19.38.2","nxr_2_Redundancyfanpowerfailure","2号UPS 冗余风扇电源故障","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["76","4.19.38.2","nxr_2_BCBaccess","2号UPS BCB接入情况","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","00:BCB未接入,F0:BCB闭合,"]
["77","4.19.38.2","nxr_2_Batterypacks1contactorfault","2号UPS 电池组1接触器故障","1","0","0","1","0","cmd-77","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["78","4.19.38.2","nxr_2_Batterypacks2contactorfault","2号UPS 电池组2接触器故障","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["79","4.19.38.2","nxr_2_Batterypacks1switchfault","2号UPS 电池组1交换器故障","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["80","4.19.38.2","nxr_2_Batterypacks2switchfault","2号UPS 电池组2交换器故障","1","0","0","1","0","cmd-80","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["81","4.19.38.2","nxr_2_Batterypacks1switchtheflow","2号UPS 电池组1交换器过流","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["82","4.19.38.2","nxr_2_Batterypacks2switchtheflow","2号UPS 电池组2交换器过流","1","0","0","1","0","cmd-82","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["83","4.19.38.2","nxr_2_Batterypacks1switchthermal","2号UPS 电池组1交换器过温","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["84","4.19.38.2","nxr_2_Batterypacks2switchthermal","2号UPS 电池组2交换器过温","1","0","0","1","0","cmd-84","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["85","4.19.38.2","nxr_2_1thebatterychargerfault","2号UPS 电池组1充电器故障","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["86","4.19.38.2","nxr_2_2thebatterychargerfault","2号UPS 电池组2充电器故障","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["87","4.19.38.2","nxr_2_Batterylife1","2号UPS 电池组1寿命情况","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["88","4.19.38.2","nxr_2_Batterylife2","2号UPS 电池组2寿命情况","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","240,241,","F0:电池需更换,F1:电池寿命终结,"]
["89","4.19.38.2","nxr_2_Batterypacks1temperaturewastoohigh","2号UPS 电池组1温度过高","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["90","4.19.38.2","nxr_2_Batterypacks2temperaturewastoohigh","2号UPS 电池组2温度过高","1","0","0","1","0","cmd-90","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过高,"]
["91","4.19.38.2","nxr_2_Batterypacks1groundfault","2号UPS 电池组1接地故障","1","0","0","1","0","cmd-91","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["92","4.19.38.2","nxr_2_Batterypacks2groundfault","2号UPS 电池组2接地故障","1","0","0","1","0","cmd-92","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["93","4.19.38.2","nxr_2_Massiveunusualfrequency","2号UPS 主路频率异常","1","0","0","1","0","cmd-93","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:超限,"]
["94","4.19.38.2","nxr_2_Balanceinductancethermal","2号UPS 平衡电感过温","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["95","4.19.38.2","nxr_2_Inputinductancethermal","2号UPS 输入电感过温","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["96","4.19.38.2","nxr_2_Rectifierthermal","2号UPS 整流器过温","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["97","4.19.38.2","nxr_2_Balancecircuitfault","2号UPS 平衡电路故障","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["98","4.19.38.2","nxr_2_Balanceelectricitypassbyflow","2号UPS 平衡电路过流","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["99","4.19.38.2","nxr_2_Meltbrokenwirerunning","2号UPS 主路熔丝断","1","0","0","1","0","cmd-99","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["100","4.19.38.2","nxr_2_1theauxiliarypoweroff","2号UPS 辅助电源1掉电","1","0","0","1","0","cmd-100","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["101","4.19.38.2","nxr_2_Sequencerunningagainst","2号UPS 主路相序反","1","0","0","1","0","cmd-101","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["102","4.19.38.2","nxr_2_Rectifierflow","2号UPS 整流器过流","1","0","0","1","0","cmd-102","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["103","4.19.38.2","nxr_2_Softstartupfailure","2号UPS 软启动失败","1","0","0","1","0","cmd-103","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["104","4.19.38.2","nxr_2_Inverterinductancethermal","2号UPS 逆变电感过温","1","0","0","1","0","cmd-104","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["105","4.19.38.2","nxr_2_Inverterthermal","2号UPS 逆变器过温","1","0","0","1","0","cmd-105","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过温,"]
["106","4.19.38.2","nxr_2_Thethyristorinverterfault","2号UPS 逆变器晶闸管故障","1","0","0","1","0","cmd-106","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["107","4.19.38.2","nxr_2_Theuseroperationerror","2号UPS 用户操作错误","1","0","0","1","0","cmd-107","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:错误,"]
["108","4.19.38.2","nxr_2_Outputmeltsilkbroken","2号UPS 输出熔丝断","1","0","0","1","0","cmd-108","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:断,"]
["109","4.19.38.2","nxr_2_Monolithicoutputoverload","2号UPS 单片输出过载","1","0","0","1","0","cmd-109","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["110","4.19.38.2","nxr_2_Expertsystemoverload","2号UPS 并机系统过载","1","0","0","1","0","cmd-110","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载,"]
["111","4.19.38.2","nxr_2_Singleoverloadovertime","2号UPS 单机过载超时","1","0","0","1","0","cmd-111","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过载超时,"]
["112","4.19.38.2","nxr_2_Acoutputpressure","2号UPS 交流输出过压","1","0","0","1","0","cmd-112","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过压,"]
["113","4.19.38.2","nxr_2_Inverterflow","2号UPS 逆变器过流","1","0","0","1","0","cmd-113","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:过流,"]
["114","4.19.38.2","nxr_2_Impactloadtobypass","2号UPS 负载冲击转旁路","1","0","0","1","0","cmd-114","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["115","4.19.38.2","nxr_2_Allflowweaverfault","2号UPS 并机均流故障","1","0","0","1","0","cmd-115","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["116","4.19.38.2","nxr_2_Busabnormalshutdown","2号UPS 母线异常关机","1","0","0","1","0","cmd-116","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["117","4.19.38.2","nxr_2_Adjacenttobypassmachinerequest","2号UPS 邻机请求转旁路","1","0","0","1","0","cmd-117","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["118","4.19.38.2","nxr_2_Dcbusovervoltagefault","2号UPS 直流母线过压故障","1","0","0","1","0","cmd-118","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["119","4.19.38.2","nxr_2_Rectifiercommunicationfault","2号UPS 整流通信故障","1","0","0","1","0","cmd-119","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["120","4.19.38.2","nxr_2_Invertercommunicationfailures","2号UPS 逆变通讯故障","1","0","0","1","0","cmd-120","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["121","4.19.38.2","nxr_2_Outputdccomponentfaulttoo","2号UPS 输出直流分量过大故障","1","0","0","1","0","cmd-121","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["122","4.19.38.2","nxr_2_Expertsystembatteryforecastpfault","2号UPS 并机系统电池预告警故障","1","0","0","1","0","cmd-122","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["123","4.19.38.2","nxr_2_Inputlackofzerofault","2号UPS 输入缺零故障","1","0","0","1","0","cmd-123","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["124","4.19.38.2","nxr_2_Invertercontactorfault","2号UPS 逆变接触器故障","1","0","0","1","0","cmd-124","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["125","4.19.38.2","nxr_2_Inputcontactorfault","2号UPS 输入接触器故障","1","0","0","1","0","cmd-125","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["126","4.19.38.2","nxr_2_Inputcurrentabnormal","2号UPS 输入电流异常","1","0","0","1","0","cmd-126","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["127","4.19.38.2","nxr_2_Outputabnormalvoltage","2号UPS 输出电压异常","1","0","0","1","0","cmd-127","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","F0:故障,"]
["130","4.19.38.2","nxr_2_AcinputlinevoltageAB","2号UPS 交流输入线电压AB","1","0","0","1","0","cmd-130","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["131","4.19.38.2","nxr_2_AcinputlinevoltageBC","2号UPS 交流输入线电压BC","1","0","0","1","0","cmd-131","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["132","4.19.38.2","nxr_2_AcinputlinevoltageCA","2号UPS 交流输入线电压CA","1","0","0","1","0","cmd-132","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["133","4.19.38.2","nxr_2_Aphaseinputcurrent","2号UPS A相输入电流","1","0","0","1","0","cmd-133","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["134","4.19.38.2","nxr_2_Bphaseinputcurrent","2号UPS B相输入电流","1","0","0","1","0","cmd-134","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["135","4.19.38.2","nxr_2_CPhaseinputcurrent","2号UPS C相输入电流","1","0","0","1","0","cmd-135","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["136","4.19.38.2","nxr_2_Inputfrequency","2号UPS 输入频率","1","0","0","1","0","cmd-136","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["137","4.19.38.2","nxr_2_Aphaseinputpowerfactor","2号UPS A相输入功率因数","1","0","0","1","0","cmd-137","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["138","4.19.38.2","nxr_2_Bphaseinputpowerfactor","2号UPS B相输入功率因数","1","0","0","1","0","cmd-138","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["139","4.19.38.2","nxr_2_Cphaseinputpowerfactor","2号UPS C相输入功率因数","1","0","0","1","0","cmd-139","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["140","4.19.38.2","nxr_2_Aphasebypassvoltage","2号UPS A相旁路电压","1","0","0","1","0","cmd-140","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["141","4.19.38.2","nxr_2_Bphasebypassvoltage","2号UPS B相旁路电压","1","0","0","1","0","cmd-141","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["142","4.19.38.2","nxr_2_CPhasebypassvoltage","2号UPS C相旁路电压","1","0","0","1","0","cmd-142","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["143","4.19.38.2","nxr_2_Bypassfrequency","2号UPS 旁路频率","1","0","0","1","0","cmd-143","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["146","4.19.38.2","nxr_2_Aphaseoutputpowerfactor","2号UPS A相输出功率因数","1","0","0","1","0","cmd-146","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["147","4.19.38.2","nxr_2_Bphaseoutputpowerfactor","2号UPS B相输出功率因数","1","0","0","1","0","cmd-147","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["148","4.19.38.2","nxr_2_Cphaseoutputpowerfactor","2号UPS C相输出功率因数","1","0","0","1","0","cmd-148","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["149","4.19.38.2","nxr_2_Aphaseoutputthanpeak","2号UPS A相输出峰值比","1","0","0","1","0","cmd-149","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["150","4.19.38.2","nxr_2_Bphaseoutputthanpeak","2号UPS B相输出峰值比","1","0","0","1","0","cmd-150","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["151","4.19.38.2","nxr_2_Cphaseoutputthanpeak","2号UPS C相输出峰值比","1","0","0","1","0","cmd-151","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["152","4.19.38.2","nxr_2_Aphaseoutputactivepower","2号UPS A相输出有功功率","1","0","0","1","0","cmd-152","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["153","4.19.38.2","nxr_2_Bphaseoutputactivepower","2号UPS B相输出有功功率","1","0","0","1","0","cmd-153","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["154","4.19.38.2","nxr_2_Cphaseoutputactivepower","2号UPS C相输出有功功率","1","0","0","1","0","cmd-154","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["155","4.19.38.2","nxr_2_Aphaseoutputreactivepower","2号UPS A相输出无功功率","1","0","0","1","0","cmd-155","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["156","4.19.38.2","nxr_2_Bphaseoutputreactivepower","2号UPS B相输出无功功率","1","0","0","1","0","cmd-156","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["157","4.19.38.2","nxr_2_Cphaseoutputreactivepower","2号UPS C相输出无功功率","1","0","0","1","0","cmd-157","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["158","4.19.38.2","nxr_2_Aphaseoutputpowerinstalled","2号UPS A相输出视在功率","1","0","0","1","0","cmd-158","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["159","4.19.38.2","nxr_2_Bphaseoutputpowerinstalled","2号UPS B相输出视在功率","1","0","0","1","0","cmd-159","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["160","4.19.38.2","nxr_2_Cphaseoutputpowerinstalled","2号UPS C相输出视在功率","1","0","0","1","0","cmd-160","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["161","4.19.38.2","nxr_2_Aphaseoutputloadpercentage","2号UPS A相输出负载百分比","1","0","0","1","0","cmd-161","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["162","4.19.38.2","nxr_2_Bphaseoutputloadpercentage","2号UPS B相输出负载百分比","1","0","0","1","0","cmd-162","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["163","4.19.38.2","nxr_2_Cphaseoutputloadpercentage","2号UPS C相输出负载百分比","1","0","0","1","0","cmd-163","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["165","4.19.38.2","nxr_2_SystemAphaseoutputactivepower","2号UPS 系统A相输出有功功率","1","0","0","1","0","cmd-165","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["166","4.19.38.2","nxr_2_SystemBphaseoutputactivepower","2号UPS 系统B相输出有功功率","1","0","0","1","0","cmd-166","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["167","4.19.38.2","nxr_2_SystemCphaseoutputactivepower","2号UPS 系统C相输出有功功率","1","0","0","1","0","cmd-167","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["168","4.19.38.2","nxr_2_SysteminstalledAphaseoutputpower","2号UPS 系统A相输出视在功率","1","0","0","1","0","cmd-168","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["169","4.19.38.2","nxr_2_SysteminstalledBphaseoutputpower","2号UPS 系统B相输出视在功率","1","0","0","1","0","cmd-169","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["170","4.19.38.2","nxr_2_SysteminstalledCphaseoutputpower","2号UPS 系统C相输出视在功率","1","0","0","1","0","cmd-170","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["171","4.19.38.2","nxr_2_SystemAphaseoutputreactivepower","2号UPS 系统A相输出无功功率","1","0","0","1","0","cmd-171","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["172","4.19.38.2","nxr_2_SystemBphaseoutputreactivepower","2号UPS 系统B相输出无功功率","1","0","0","1","0","cmd-172","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["173","4.19.38.2","nxr_2_SystemCphaseoutputreactivepower","2号UPS 系统C相输出无功功率","1","0","0","1","0","cmd-173","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["176","4.19.38.2","nxr_2_Batterybackuptime","2号UPS 电池后备时间","1","0","0","1","0","cmd-176","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["177","4.19.38.2","nxr_2_Arebatteryvoltage","2号UPS 正电池电压","1","0","0","1","0","cmd-177","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["178","4.19.38.2","nxr_2_Arebatteryelectriccurrent","2号UPS 正电池电流","1","0","0","1","0","cmd-178","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["179","4.19.38.2","nxr_2_Negativebatteryvoltage","2号UPS 负电池电压","1","0","0","1","0","cmd-179","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["180","4.19.38.2","nxr_2_Negativebatteryelectriccurrent","2号UPS 负电池电流","1","0","0","1","0","cmd-180","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["181","4.19.38.2","nxr_2_Batteryagingcoefficient","2号UPS 电池老化系数","1","0","0","1","0","cmd-181","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["182","4.19.38.2","nxr_2_Batterytemperature","2号UPS 电池温度","1","0","0","1","0","cmd-182","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["183","4.19.38.2","nxr_2_Environmenttemperature","2号UPS 环境温度","1","0","0","1","0","cmd-183","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","4.19.38.2","nxr_2_Communications","2号UPS通信状态","1000","0","0","1","0",null,null,"0","60","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","26",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]