{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":100,"n_cols":78,"rows_kept":100,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述","备注1","备注2"]
["1","4.14.26.1","EA99I_1_BatteryVolt","1号UPS电池电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.14.26.1","EA99I_1_BatteryCapacity","1号UPS电池容量","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.14.26.1","EA99I_1_BatteryTime","1号UPS电池剩余时间","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.14.26.1","EA99I_1_BatteryCur","1号UPS电池电流","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.14.26.1","EA99I_1_BatteryTemp","1号UPS电池温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.14.26.1","EA99I_1_InputFrequency","1号UPS输入频率","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.14.26.1","EA99I_1_BypassFrequency","1号UPS旁路频率","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.14.26.1","EA99I_1_OutputFrequency","1号UPS输出频率","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.14.26.1","EA99I_1_RectifierRotationError","1号UPS输入相序反","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["10","4.14.26.1","EA99I_1_LowBatteryShutdonw","1号UPS电池低关机","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["11","4.14.26.1","EA99I_1_LowBattery","1号UPS电池低","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["12","4.14.26.1","EA99I_1_Threein","1号UPS输入输出类型","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["13","4.14.26.1","EA99I_1_BackUpACNormal","1号UPSUPS运行方式","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["14","4.14.26.1","EA99I_1_Charge","1号UPS电池充电状态","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["15","4.14.26.1","EA99I_1_RectifierOperating","1号UPS整流器工作","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["16","4.14.26.1","EA99I_1_BypassFrequencyFail","1号UPS旁路频率故障","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["17","4.14.26.1","EA99I_1_ManualBypassBreaker","1号UPS旁路开关","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["18","4.14.26.1","EA99I_1_BypassAC","1号UPS旁路直流","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["19","4.14.26.1","EA99I_1_StaticSwitch","1号UPS静态开关","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["20","4.14.26.1","EA99I_1_InverterOperating","1号UPS逆变器工作","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["21","4.14.26.1","EA99I_1_EmergencyStop","1号UPS紧急停止","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["22","4.14.26.1","EA99I_1_HighDCShutdown","1号UPS高直流关机","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["23","4.14.26.1","EA99I_1_ManualBypassBreakerShutdown","1号UPS旁路开关关机","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["24","4.14.26.1","EA99I_1_OverLoadShutdown","1号UPS过载关机","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["25","4.14.26.1","EA99I_1_InverterOPFailShutdown","1号UPS逆变输出故障关机","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["26","4.14.26.1","EA99I_1_OverTemperatureShutdown","1号UPS温度过高关机","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["27","4.14.26.1","EA99I_1_ShortCircuitShutdown","1号UPS短路关机","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["28","4.14.26.1","EA99I_1_RIPVoltage","1号UPSR相输入电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.14.26.1","EA99I_1_SIPVoltage","1号UPSS相输入电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.14.26.1","EA99I_1_TIPVoltage","1号UPST相输入电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.14.26.1","EA99I_1_RBypassACVoltage","1号UPSR相旁路交流电压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.14.26.1","EA99I_1_SBypassACVoltage","1号UPSS相旁路交流电压","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.14.26.1","EA99I_1_TBypassACVoltage","1号UPST相旁路交流电压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.14.26.1","EA99I_1_ROPValtage","1号UPSR相输出电压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.14.26.1","EA99I_1_SOPValtage","1号UPSS相输出电压","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.14.26.1","EA99I_1_TOPValtage","1号UPST相输出电压","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.14.26.1","EA99I_1_RLoadPrecent","1号UPSR相负载%","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","4.14.26.1","EA99I_1_SLoadPrecent","1号UPSS相负载%","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","4.14.26.1","EA99I_1_TLoadPrecent","1号UPST相负载%","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","4.14.26.1","EA99I_1_Ipvoltage","1号UPS输入电压","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","4.14.26.1","EA99I_1_IPFaultvoltage","1号UPS故障输入电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","4.14.26.1","EA99I_1_Opvoltage","1号UPS输出电压","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["43","4.14.26.1","EA99I_1_InputCurrent","1号UPS输出电流","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["44","4.14.26.1","EA99I_1_InputFrequency","1号UPS输入频率","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["47","4.14.26.1","EA99I_1_UtilityFail","1号UPS市电故障","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["48","4.14.26.1","EA99I_1_BatteryLow","1号UPS电池低","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["49","4.14.26.1","EA99I_1_BypassActive","1号UPS旁路激活","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["50","4.14.26.1","EA99I_1_UPSFailed","1号UPS电池电压故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["30","4.14.26.1","EA99I_1_Communications","1号UPS通信状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]
[]
["1","4.14.26.2","EA99I_2_BatteryVolt","2号UPS电池电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.14.26.2","EA99I_2_BatteryCapacity","2号UPS电池容量","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.14.26.2","EA99I_2_BatteryTime","2号UPS电池剩余时间","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.14.26.2","EA99I_2_BatteryCur","2号UPS电池电流","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.14.26.2","EA99I_2_BatteryTemp","2号UPS电池温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.14.26.2","EA99I_2_InputFrequency","2号UPS输入频率","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.14.26.2","EA99I_2_BypassFrequency","2号UPS旁路频率","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.14.26.2","EA99I_2_OutputFrequency","2号UPS输出频率","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.14.26.2","EA99I_2_RectifierRotationError","2号UPS输入相序反","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["10","4.14.26.2","EA99I_2_LowBatteryShutdonw","2号UPS电池低关机","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["11","4.14.26.2","EA99I_2_LowBattery","2号UPS电池低","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["12","4.14.26.2","EA99I_2_Threein","2号UPS输入输出类型","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["13","4.14.26.2","EA99I_2_BackUpACNormal","2号UPSUPS运行方式","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["14","4.14.26.2","EA99I_2_Charge","2号UPS电池充电状态","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["15","4.14.26.2","EA99I_2_RectifierOperating","2号UPS整流器工作","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["16","4.14.26.2","EA99I_2_BypassFrequencyFail","2号UPS旁路频率故障","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["17","4.14.26.2","EA99I_2_ManualBypassBreaker","2号UPS旁路开关","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["18","4.14.26.2","EA99I_2_BypassAC","2号UPS旁路直流","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["19","4.14.26.2","EA99I_2_StaticSwitch","2号UPS静态开关","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["20","4.14.26.2","EA99I_2_InverterOperating","2号UPS逆变器工作","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["21","4.14.26.2","EA99I_2_EmergencyStop","2号UPS紧急停止","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["22","4.14.26.2","EA99I_2_HighDCShutdown","2号UPS高直流关机","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["23","4.14.26.2","EA99I_2_ManualBypassBreakerShutdown","2号UPS旁路开关关机","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["24","4.14.26.2","EA99I_2_OverLoadShutdown","2号UPS过载关机","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["25","4.14.26.2","EA99I_2_InverterOPFailShutdown","2号UPS逆变输出故障关机","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["26","4.14.26.2","EA99I_2_OverTemperatureShutdown","2号UPS温度过高关机","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["27","4.14.26.2","EA99I_2_ShortCircuitShutdown","2号UPS短路关机","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["28","4.14.26.2","EA99I_2_RIPVoltage","2号UPSR相输入电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.14.26.2","EA99I_2_SIPVoltage","2号UPSS相输入电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.14.26.2","EA99I_2_TIPVoltage","2号UPST相输入电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.14.26.2","EA99I_2_RBypassACVoltage","2号UPSR相旁路交流电压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.14.26.2","EA99I_2_SBypassACVoltage","2号UPSS相旁路交流电压","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.14.26.2","EA99I_2_TBypassACVoltage","2号UPST相旁路交流电压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.14.26.2","EA99I_2_ROPValtage","2号UPSR相输出电压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.14.26.2","EA99I_2_SOPValtage","2号UPSS相输出电压","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.14.26.2","EA99I_2_TOPValtage","2号UPST相输出电压","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.14.26.2","EA99I_2_RLoadPrecent","2号UPSR相负载%","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","4.14.26.2","EA99I_2_SLoadPrecent","2号UPSS相负载%","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","4.14.26.2","EA99I_2_TLoadPrecent","2号UPST相负载%","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","4.14.26.2","EA99I_2_Ipvoltage","2号UPS输入电压","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","4.14.26.2","EA99I_2_IPFaultvoltage","2号UPS故障输入电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","4.14.26.2","EA99I_2_Opvoltage","2号UPS输出电压","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["43","4.14.26.2","EA99I_2_InputCurrent","2号UPS输出电流","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["44","4.14.26.2","EA99I_2_InputFrequency","2号UPS输入频率","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["47","4.14.26.2","EA99I_2_UtilityFail","2号UPS市电故障","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["48","4.14.26.2","EA99I_2_BatteryLow","2号UPS电池低","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["49","4.14.26.2","EA99I_2_BypassActive","2号UPS旁路激活","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["50","4.14.26.2","EA99I_2_UPSFailed","2号UPS电池电压故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["30","4.14.26.2","EA99I_2_Communications","2号UPS通信状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":56,"n_cols":78,"rows_kept":56,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述","备注1","备注2"]
["1","4.14.26.1","EA99I_1_BatteryVolt","1号UPS电池电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.14.26.1","EA99I_1_BatteryCapacity","1号UPS电池容量","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.14.26.1","EA99I_1_BatteryTime","1号UPS电池剩余时间","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.14.26.1","EA99I_1_BatteryCur","1号UPS电池电流","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.14.26.1","EA99I_1_BatteryTemp","1号UPS电池温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.14.26.1","EA99I_1_InputFrequency","1号UPS输入频率","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.14.26.1","EA99I_1_BypassFrequency","1号UPS旁路频率","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.14.26.1","EA99I_1_OutputFrequency","1号UPS输出频率","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.14.26.1","EA99I_1_RectifierRotationError","1号UPS整流器回转错误","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["10","4.14.26.1","EA99I_1_LowBatteryShutdonw","1号UPS电池低关机","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["11","4.14.26.1","EA99I_1_LowBattery","1号UPS电池低","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["12","4.14.26.1","EA99I_1_Threein","1号UPSThree in","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["13","4.14.26.1","EA99I_1_BackUpACNormal","1号UPS备份/AC正常","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["14","4.14.26.1","EA99I_1_Charge","1号UPS充电","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["15","4.14.26.1","EA99I_1_RectifierOperating","1号UPS整流器工作","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["16","4.14.26.1","EA99I_1_BypassFrequencyFail","1号UPS旁路频率故障","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["17","4.14.26.1","EA99I_1_ManualBypassBreaker","1号UPS旁路开关","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["18","4.14.26.1","EA99I_1_BypassAC","1号UPS旁路直流","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["19","4.14.26.1","EA99I_1_StaticSwitch","1号UPS静态开关","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["20","4.14.26.1","EA99I_1_InverterOperating","1号UPS逆变器工作","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["21","4.14.26.1","EA99I_1_EmergencyStop","1号UPS紧急停止","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["22","4.14.26.1","EA99I_1_HighDCShutdown","1号UPS高直流关机","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["23","4.14.26.1","EA99I_1_ManualBypassBreakerShutdown","1号UPS旁路开关关机","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["24","4.14.26.1","EA99I_1_OverLoadShutdown","1号UPS过载关机","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["25","4.14.26.1","EA99I_1_InverterOPFailShutdown","1号UPS逆变输出故障关机","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["26","4.14.26.1","EA99I_1_OverTemperatureShutdown","1号UPS温度过高关机","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["27","4.14.26.1","EA99I_1_ShortCircuitShutdown","1号UPS短路关机","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["28","4.14.26.1","EA99I_1_RIPVoltage","1号UPSR相输入电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.14.26.1","EA99I_1_SIPVoltage","1号UPSS相输入电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.14.26.1","EA99I_1_TIPVoltage","1号UPST相输入电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.14.26.1","EA99I_1_RBypassACVoltage","1号UPSR相旁路交流电压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.14.26.1","EA99I_1_SBypassACVoltage","1号UPSS相旁路交流电压","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.14.26.1","EA99I_1_TBypassACVoltage","1号UPST相旁路交流电压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.14.26.1","EA99I_1_ROPValtage","1号UPSR相输出电压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.14.26.1","EA99I_1_SOPValtage","1号UPSS相输出电压","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.14.26.1","EA99I_1_TOPValtage","1号UPST相输出电压","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.14.26.1","EA99I_1_RLoadPrecent","1号UPSR相负载%","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","4.14.26.1","EA99I_1_SLoadPrecent","1号UPSS相负载%","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","4.14.26.1","EA99I_1_TLoadPrecent","1号UPST相负载%","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","4.14.26.1","EA99I_1_Ipvoltage","1号UPS输入电压","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","4.14.26.1","EA99I_1_IPFaultvoltage","1号UPS故障输入电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","4.14.26.1","EA99I_1_Opvoltage","1号UPS输出电压","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["43","4.14.26.1","EA99I_1_InputCurrent","1号UPS输出电流","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["44","4.14.26.1","EA99I_1_InputFrequency","1号UPS输入频率","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["45","4.14.26.1","EA99I_1_BatteryVoltage","1号UPS电池电压","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["46","4.14.26.1","EA99I_1_Temperature","1号UPS温度","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["47","4.14.26.1","EA99I_1_UtilityFail","1号UPS市电故障","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["48","4.14.26.1","EA99I_1_BatteryLow","1号UPS电池低","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["49","4.14.26.1","EA99I_1_BypassActive","1号UPS旁路在线","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["50","4.14.26.1","EA99I_1_UPSFailed","1号UPSUPS故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["51","4.14.26.1","EA99I_1_UPSOnline","1号UPSUPS备机","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["52","4.14.26.1","EA99I_1_UPSTest","1号UPSUPS测试","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["53","4.14.26.1","EA99I_1_ShutdownActive","1号UPSUPS关机","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["54","4.14.26.1","EA99I_1_BeeperOn","1号UPS蜂鸣器开","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["30","4.14.26.1","EA99I_1_Communications","1号UPS通信状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]