{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":45,"n_cols":76,"rows_kept":45,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.38.1","APCSilcon_1_OutputVoltageL1","1号UPS 输出电压U1","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","1","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["2","4.19.38.1","APCSilcon_1_OutputVoltageL2","1号UPS 输出电压U2","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["3","4.19.38.1","APCSilcon_1_OutputVoltageL3","1号UPS 输出电压U3","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["4","4.19.38.1","APCSilcon_1_MainsVoltageL1","1号UPS 主路输入电压U1","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["5","4.19.38.1","APCSilcon_1_MainsVoltageL2","1号UPS 主路输入电压U2","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["6","4.19.38.1","APCSilcon_1_MainsVoltageL3","1号UPS 主路输入电压U3","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["7","4.19.38.1","APCSilcon_1_BypassVoltageL1","1号UPS 旁路输入电压U1","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["8","4.19.38.1","APCSilcon_1_BypassVoltageL2","1号UPS 旁路输入电压U2","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["9","4.19.38.1","APCSilcon_1_BypassVoltageL3","1号UPS 旁路输入电压U3","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["10","4.19.38.1","APCSilcon_1_MainsCurrentL1","1号UPS 主路输入电流I1","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["11","4.19.38.1","APCSilcon_1_MainsCurrentL2","1号UPS 主路输入电流I2","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["12","4.19.38.1","APCSilcon_1_MainsCurrentL3","1号UPS 主路输入电流I3","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["13","4.19.38.1","APCSilcon_1_OutputCurrentL1","1号UPS 输出电流I1","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["14","4.19.38.1","APCSilcon_1_OutputCurrentL2","1号UPS 输出电流I2","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["15","4.19.38.1","APCSilcon_1_OutputCurrentL3","1号UPS 输出电流I3","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["16","4.19.38.1","APCSilcon_1_OutputPeakCurrentL1","1号UPS 输出峰值电流I1","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["17","4.19.38.1","APCSilcon_1_OutputPeakCurrentL2","1号UPS 输出峰值电流I2","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["18","4.19.38.1","APCSilcon_1_OutputPeakCurrentL3","1号UPS 输出峰值电流I3","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["19","4.19.38.1","APCSilcon_1_BatteryCurrent","1号UPS 电池电流","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["20","4.19.38.1","APCSilcon_1_BatteryVoltage","1号UPS 电池电压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["21","4.19.38.1","APCSilcon_1_BatteryTemperature","1号UPS 电池温度","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["22","4.19.38.1","APCSilcon_1_Frequency","1号UPS 频率","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["23","4.19.38.1","APCSilcon_1_SystemLoadinPercent","1号UPS 系统负载百分比","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["24","4.19.38.1","APCSilcon_1_BatteryTimeLeft","1号UPS 电池剩余时间","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","3","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["25","4.19.38.1","APCSilcon_1_OutputVoltageOutofRange","1号UPS 输出电压越限","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["26","4.19.38.1","APCSilcon_1_BatteryOperation","1号UPS 电池供电","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["27","4.19.38.1","APCSilcon_1_BypassOperation","1号UPS 旁路供电","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["28","4.19.38.1","APCSilcon_1_BatteryVoltageLow","1号UPS 电池电压过低","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["29","4.19.38.1","APCSilcon_1_BatteryVoltagehigh","1号UPS 电池电压过高","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["30","4.19.38.1","APCSilcon_1_CommonFault","1号UPS 一般故障","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["31","4.19.38.1","APCSilcon_1_OutputCurrentM100","1号UPS 输出电流>100%","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["32","4.19.38.1","APCSilcon_1_StaticSwitchTemM100","1号UPS 静态开关温度>100℃","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["33","4.19.38.1","APCSilcon_1_Systempushedon","1号UPS 系统Pushed on","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","3","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["34","4.19.38.1","APCSilcon_1_Inverteroff","1号UPS 逆变器关闭","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["35","4.19.38.1","APCSilcon_1_Systemnotsynchronized","1号UPS 系统不同步","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["36","4.19.38.1","APCSilcon_1_Batterychargecurrentlimit","1号UPS 电池充电电流受限","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["37","4.19.38.1","APCSilcon_1_Batterynotconnected","1号UPS 电池开关","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["38","4.19.38.1","APCSilcon_1_Mainstransformeroverheated","1号UPS 主变压器过热","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["39","4.19.38.1","APCSilcon_1_Inverteroverheated","1号UPS 逆变器过热","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["40","4.19.38.1","APCSilcon_1_Batteryvoltagelowwarning  ","1号UPS 电池电压过低警告","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["41","4.19.38.1","APCSilcon_1_InvertercurrentM100","1号UPS 逆变器电流>100%","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["42","4.19.38.1","APCSilcon_1_OutputcurrentM150","1号UPS 输出电流>150%","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["43","4.19.38.1","APCSilcon_1_Bypassvoltageoutofrange","1号UPS 旁路电压越限","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]
["44","4.19.38.1","APCSilcon_1_Mainsvoltageoutofrange ","1号UPS 主路电压越限","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","告警,"]