{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":20,"n_cols":76,"rows_kept":20,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["73","4.15.31.1","UPS_InputVolA","A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["57","4.15.31.1","UPS_InputVolB","B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["58","4.15.31.1","UPS_InputVolC","C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["59","4.15.31.1","UPS_OutputVolA","A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["60","4.15.31.1","UPS_OutputVolB","B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["61","4.15.31.1","UPS_OutputVolC","C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["62","4.15.31.1","UPS_LoadA","A相负载","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["63","4.15.31.1","UPS_LoadB","B相负载","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["64","4.15.31.1","UPS_LoadC","C相负载","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["65","4.15.31.1","UPS_Temp","温度","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["66","4.15.31.1","UPS_Freq","频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["67","4.15.31.1","UPS_BatteryVol","电池电压","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["68","4.15.31.1","UPS_RemainTime","电池剩余时间","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["69","4.15.31.1","UPS_Status","UPS状态","1","0","0","1","3","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["70","4.15.31.1","UPS_Rectifier","UPS逆变器","1","0","0","1","3","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["71","4.15.31.1","UPS_PowerSupply","UPS供电方式","1","0","0","1","3","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["72","4.15.31.1","UPS_BatteryStatus","电池状态","1","0","0","1","3","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["72","4.15.31.1","UPS_ChargeStatus","充电状态","1","0","0","1","3","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["61","4.15.31.1","ups1_status","UPS通信","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":19,"n_cols":76,"rows_kept":19,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["73","4.15.31.1","UPS_InputVolA","A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["57","4.15.31.1","UPS_InputVolB","B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["58","4.15.31.1","UPS_InputVolC","C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["59","4.15.31.1","UPS_OutputVolA","A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["60","4.15.31.1","UPS_OutputVolB","B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["61","4.15.31.1","UPS_OutputVolC","C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["62","4.15.31.1","UPS_LoadA","A相负载","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["63","4.15.31.1","UPS_LoadB","B相负载","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["64","4.15.31.1","UPS_LoadC","C相负载","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["65","4.15.31.1","UPS_Temp","温度","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["66","4.15.31.1","UPS_Freq","频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["67","4.15.31.1","UPS_BatteryVol","电池电压","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["68","4.15.31.1","UPS_RemainTime","电池剩余时间","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["69","4.15.31.1","UPS_Status","UPS状态","1","0","0","1","3","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["70","4.15.31.1","UPS_Rectifier","UPS逆变器","1","0","0","1","3","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["71","4.15.31.1","UPS_PowerSupply","UPS供电方式","1","0","0","1","3","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["72","4.15.31.1","UPS_BatteryStatus","电池状态","1","0","0","1","3","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0"]
["61","4.15.31.1","ups1_status","UPS通信","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]