{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":66,"n_cols":76,"rows_kept":66,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.14.26.1","XCP_1_OutputLineVoltageAB","输出线电压AB","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.14.26.1","XCP_1_OutputLineVoltageBC","输出线电压BC","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.14.26.1","XCP_1_OutputLineVoltageAC","输出线电压AC","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.14.26.1","XCP_1_InputLineVoltageAB","输入线电压AB","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.14.26.1","XCP_1_InputLineVoltageBC","输入线电压BC","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.14.26.1","XCP_1_InputLineVoltageAC","输入线电压AC","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.14.26.1","XCP_1_BypassLineInputVoltageAB","旁路输入线电压AB","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.14.26.1","XCP_1_BypassLineInputVoltageBC","旁路输入线电压BC","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.14.26.1","XCP_1_BypassLineInputVoltageCA","旁路输入线电压CA","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["10","4.14.26.1","XCP_1_InputCurrentA","输入电流A相","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["11","4.14.26.1","XCP_1_InputCurrentB","输入电流B相","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["12","4.14.26.1","XCP_1_InputCurrentC","输入电流C相","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["13","4.14.26.1","XCP_1_OutputPower","输出功率（W）","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","w","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["14","4.14.26.1","XCP_1_InputPower","输入功率（W）","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","w","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["15","4.14.26.1","XCP_1_OutputApparentPower","输出视在功率（VA）","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","va","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["16","4.14.26.1","XCP_1_InputApparentPower","输入视在功率（VA）","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","va","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["17","4.14.26.1","XCP_1_OutputFrequency","输出频率","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["18","4.14.26.1","XCP_1_InputFrequency","输入频率","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["19","4.14.26.1","XCP_1_InverterFrequency","逆变器频率","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["20","4.14.26.1","XCP_1_BypassFrequency","旁路频率","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["21","4.14.26.1","XCP_1_BatteryElectricCurrent","电池电流","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","-100","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["22","4.14.26.1","XCP_1_BatteryVoltage","电池电压","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["23","4.14.26.1","XCP_1_BatteryRemainingPercentage","电池剩余百分比","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["24","4.14.26.1","XCP_1_BatteryRemainingTime","电池剩余时间","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["25","4.14.26.1","XCP_1_InverterAPhaseVoltage","逆变器A相电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["26","4.14.26.1","XCP_1_InverterBPhaseVoltage","逆变器B相电压","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["27","4.14.26.1","XCP_1_InverterCPhaseVoltage","逆变器C相电压","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["28","4.14.26.1","XCP_1_APhaseLoadCurrent","A相负载电流","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.14.26.1","XCP_1_BPhaseLoadCurrent","B相负载电流","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.14.26.1","XCP_1_CPhaseLoadCurrent","C相负载电流","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.14.26.1","XCP_1_APhaseOutputRatio","A相电流输出比率","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.14.26.1","XCP_1_BPhaseOutputRatio","B相电流输出比率","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.14.26.1","XCP_1_CPhaseOutputRatio","C相电流输出比率","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.14.26.1","XCP_1_APhaseOutputVoltage","A相输出电压","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.14.26.1","XCP_1_BPhaseOutputVoltage","B相输出电压","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.14.26.1","XCP_1_CPhaseOutputVoltage","C相输出电压","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.14.26.1","XCP_1_InverterVoltagePressure","逆变器电压过压","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["38","4.14.26.1","XCP_1_InverterVoltageOwePressure","逆变器电压欠压","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["39","4.14.26.1","XCP_1_MoreLimitedFrequencyInverter","逆变器频率越限","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["40","4.14.26.1","XCP_1_BypassVoltageOver","旁路电压过压","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["41","4.14.26.1","XCP_1_BypassVoltageOwePressur","旁路电压欠压","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["42","4.14.26.1","XCP_1_BypassMoreLimitedFrequency","旁路频率越限","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["43","4.14.26.1","XCP_1_InputVoltageOver","输入电压过压","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["44","4.14.26.1","XCP_1_InputVoltageOwePressure","输入电压欠压","1","0","0","1","0","cmd-61","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["45","4.14.26.1","XCP_1_InputFrequencyMoreLimited","输入频率越限","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["46","4.14.26.1","XCP_1_OutputVoltageOver","输出电压过压","1","0","0","1","0","cmd-63","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["47","4.14.26.1","XCP_1_OutputVoltageOwePressure","输出电压欠压","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["48","4.14.26.1","XCP_1_OutputFrequencyMoreLimited","输出频率越限","1","0","0","1","0","cmd-65","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["49","4.14.26.1","XCP_1_OutputOverload","输出过载","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["50","4.14.26.1","XCP_1_RectifierFault","整流器故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["51","4.14.26.1","XCP_1_InverterFault","逆变器故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["52","4.14.26.1","XCP_1_BatteryConnectionFailure","电池连接故障","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["53","4.14.26.1","XCP_1_BypassSwitchFault","旁路开关故障","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["54","4.14.26.1","XCP_1_BatteryCurrentLimit","电池电流越限","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["55","4.14.26.1","XCP_1_Shutdown","关机","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["56","4.14.26.1","XCP_1_BatteryVoltage","电池欠压","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["57","4.14.26.1","XCP_1_PowerSupplyFault","供电故障","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["58","4.14.26.1","XCP_1_RadiatorOverTemperature","散热器超温","1","0","0","1","0","cmd-82","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["59","4.14.26.1","XCP_1_TheRadiatorTemperatureFeelingFault","散热器温感故障","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["60","4.14.26.1","XCP_1_EmergencyShutdown","紧急关机","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["61","4.14.26.1","XCP_1_BatteryPowerSupply","由电池供电","1","0","0","1","0","cmd-92","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["62","4.14.26.1","XCP_1_TurnBypassWork","转旁路工作","1","0","0","1","0","cmd-93","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["63","4.14.26.1","XCP_1_BatteriesNeedToReplace","电池需替换","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["64","4.14.26.1","XCP_1_FanFault","风扇故障","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["34","4.14.26.1","XCP_1_Communications","爱赛克UPS通信状态","1000","0","0","1","0",null,null,"0","60","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":96,"n_cols":76,"rows_kept":96,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.14.26.1","XCP_1_ByInstalled","旁路已安装","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.14.26.1","XCP_1_OutputBreakerOpen","输出开关关闭","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.14.26.1","XCP_1_BypassOn","转旁路","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.14.26.1","XCP_1_BatteryOn","由电池供电","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.14.26.1","XCP_1_InveterOn","逆变器工作","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.14.26.1","XCP_1_BatteryTimeWarning","电池备用时间报警","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.14.26.1","XCP_1_RectifierOn","整流器工作","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.14.26.1","XCP_1_BypassReady","旁路准备就绪","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.14.26.1","XCP_1_LoadSwitch","负荷开关","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["10","4.14.26.1","XCP_1_InverterOutputSwitch","逆变器输出开关","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["11","4.14.26.1","XCP_1_BatterySwitch","电池开关","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["12","4.14.26.1","XCP_1_StaticBypassSwitch","静态旁路开关","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["13","4.14.26.1","XCP_1_BypassSwitch","旁路开关","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["14","4.14.26.1","XCP_1_RectifierInputSwitch","整流器输入开关","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["15","4.14.26.1","XCP_1_OutputLineVoltageAB","输出线电压AB","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["16","4.14.26.1","XCP_1_OutputLineVoltageBC","输出线电压BC","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["17","4.14.26.1","XCP_1_OutputLineVoltageAC","输出线电压AC","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["18","4.14.26.1","XCP_1_InputLineVoltageAB","输入线电压AB","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["19","4.14.26.1","XCP_1_InputLineVoltageBC","输入线电压BC","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["20","4.14.26.1","XCP_1_InputLineVoltageAC","输入线电压AC","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["21","4.14.26.1","XCP_1_BypassLineInputVoltageAB","旁路输入线电压AB","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["22","4.14.26.1","XCP_1_BypassLineInputVoltageBC","旁路输入线电压BC","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["23","4.14.26.1","XCP_1_BypassLineInputVoltageCA","旁路输入线电压CA","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["24","4.14.26.1","XCP_1_InputCurrentA","输入电流A相","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["25","4.14.26.1","XCP_1_InputCurrentB","输入电流B相","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["26","4.14.26.1","XCP_1_InputCurrentC","输入电流C相","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["27","4.14.26.1","XCP_1_OutputPower","输出功率（W）","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","w","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["28","4.14.26.1","XCP_1_InputPower","输入功率（W）","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","w","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.14.26.1","XCP_1_OutputApparentPower","输出视在功率（VA）","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","va","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.14.26.1","XCP_1_InputApparentPower","输入视在功率（VA）","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","va","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.14.26.1","XCP_1_OutputPowerFactor","输出功率因子","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.14.26.1","XCP_1_InputPowerFactor","输入功率因子","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.14.26.1","XCP_1_OutputFrequency","输出频率","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.14.26.1","XCP_1_InputFrequency","输入频率","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.14.26.1","XCP_1_InverterFrequency","逆变器频率","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.14.26.1","XCP_1_BypassFrequency","旁路频率","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.14.26.1","XCP_1_BatteryElectricCurrent","电池电流","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","4.14.26.1","XCP_1_BatteryVoltage","电池电压","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","4.14.26.1","XCP_1_BatteryRemainingPercentage","电池剩余百分比","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","4.14.26.1","XCP_1_BatteryRemainingTime","电池剩余时间","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","4.14.26.1","XCP_1_InverterAPhaseVoltage","逆变器A相电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","4.14.26.1","XCP_1_InverterBPhaseVoltage","逆变器B相电压","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["43","4.14.26.1","XCP_1_InverterCPhaseVoltage","逆变器C相电压","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["44","4.14.26.1","XCP_1_APhaseLoadCurrent","A相负载电流","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["45","4.14.26.1","XCP_1_BPhaseLoadCurrent","B相负载电流","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["46","4.14.26.1","XCP_1_CPhaseLoadCurrent","C相负载电流","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["47","4.14.26.1","XCP_1_APhaseOutputRatio","A相电流输出比率","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["48","4.14.26.1","XCP_1_BPhaseOutputRatio","B相电流输出比率","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["49","4.14.26.1","XCP_1_CPhaseOutputRatio","C相电流输出比率","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["50","4.14.26.1","XCP_1_VoltageRatio","电压比率","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["51","4.14.26.1","XCP_1_APhaseOutputVoltage","A相输出电压","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["52","4.14.26.1","XCP_1_BPhaseOutputVoltage","B相输出电压","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["53","4.14.26.1","XCP_1_CPhaseOutputVoltage","C相输出电压","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["54","4.14.26.1","XCP_1_InverterVoltagePressure","逆变器电压过压","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["55","4.14.26.1","XCP_1_InverterVoltageOwePressure","逆变器电压欠压","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["56","4.14.26.1","XCP_1_MoreLimitedFrequencyInverter","逆变器频率越限","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["57","4.14.26.1","XCP_1_BypassVoltageOver","旁路电压过压","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["58","4.14.26.1","XCP_1_BypassVoltageOwePressur","旁路电压欠压","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["59","4.14.26.1","XCP_1_BypassMoreLimitedFrequency","旁路频率越限","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["60","4.14.26.1","XCP_1_InputVoltageOver","输入电压过压","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["61","4.14.26.1","XCP_1_InputVoltageOwePressure","输入电压欠压","1","0","0","1","0","cmd-61","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["62","4.14.26.1","XCP_1_InputFrequencyMoreLimited","输入频率越限","1","0","0","1","0","cmd-62","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["63","4.14.26.1","XCP_1_OutputVoltageOver","输出电压过压","1","0","0","1","0","cmd-63","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["64","4.14.26.1","XCP_1_OutputVoltageOwePressure","输出电压欠压","1","0","0","1","0","cmd-64","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["65","4.14.26.1","XCP_1_OutputFrequencyMoreLimited","输出频率越限","1","0","0","1","0","cmd-65","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["66","4.14.26.1","XCP_1_OutputOverload","输出过载","1","0","0","1","0","cmd-66","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["67","4.14.26.1","XCP_1_DcVoltageOver","直流电压过压","1","0","0","1","0","cmd-67","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["68","4.14.26.1","XCP_1_DcVoltageOwePressure","直流电压欠压","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["69","4.14.26.1","XCP_1_RectifierFault","整流器故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["70","4.14.26.1","XCP_1_InverterFault","逆变器故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["71","4.14.26.1","XCP_1_BatteryConnectionFailure","电池连接故障","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["72","4.14.26.1","XCP_1_BypassSwitchFault","旁路开关故障","1","0","0","1","0","cmd-72","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["73","4.14.26.1","XCP_1_RectifierNotCalibration","整流器未标定","1","0","0","1","0","cmd-73","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["74","4.14.26.1","XCP_1_OutputNotCalibration","输出未标定","1","0","0","1","0","cmd-74","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["75","4.14.26.1","XCP_1_InverterNotCalibration","逆变器未标定","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["76","4.14.26.1","XCP_1_BatteryCurrentLimit","电池电流越限","1","0","0","1","0","cmd-76","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["77","4.14.26.1","XCP_1_OutputCurrentOverRated current","输出电流超过额定电流","1","0","0","1","0","cmd-77","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["78","4.14.26.1","XCP_1_Shutdown","关机","1","0","0","1","0","cmd-78","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["79","4.14.26.1","XCP_1_BatteryVoltage","电池欠压","1","0","0","1","0","cmd-79","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["80","4.14.26.1","XCP_1_BatteryDcVoltagePressure","电池直流电压过压","1","0","0","1","0","cmd-80","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["81","4.14.26.1","XCP_1_PowerSupplyFault","供电故障","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["82","4.14.26.1","XCP_1_RadiatorOverTemperature","散热器超温","1","0","0","1","0","cmd-82","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["83","4.14.26.1","XCP_1_TheRadiatorTemperatureFeelingFault","散热器温感故障","1","0","0","1","0","cmd-83","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["84","4.14.26.1","XCP_1_NetworkNotResponse","网络不响应","1","0","0","1","0","cmd-84","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["85","4.14.26.1","XCP_1_InputSequenceFault","输入相序故障","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["86","4.14.26.1","XCP_1_EmergencyShutdown","紧急关机","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["87","4.14.26.1","XCP_1_BypassInputPowerLost","旁路输入掉电","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["88","4.14.26.1","XCP_1_BatterySwitchOn","电池开关打开","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["89","4.14.26.1","XCP_1_InverterConnectionBroken","逆变器连接断开","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["90","4.14.26.1","XCP_1_CompletelyDdischargeaBattery","电池完全放电","1","0","0","1","0","cmd-90","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["91","4.14.26.1","XCP_1_BatteryNotCharging","电池未充电","1","0","0","1","0","cmd-91","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["92","4.14.26.1","XCP_1_BatteryPowerSupply","由电池供电","1","0","0","1","0","cmd-92","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["93","4.14.26.1","XCP_1_TurnBypassWork","转旁路工作","1","0","0","1","0","cmd-93","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["94","4.14.26.1","XCP_1_BatteriesNeedToReplace","电池需替换","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["95","4.14.26.1","XCP_1_FanFault","风扇故障","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]