{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":43,"n_cols":76,"rows_kept":43,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.15.27.1","Bagkee_1_BatteryVoltage","电池电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","1","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.15.27.1","Bagkee_1_BatteryCapacity","电池容量百分比","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.15.27.1","Bagkee_1_BatteryDuration","电池维持时间","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.15.27.1","Bagkee_1_BatteryChargeCurrent","电池充电电流","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.15.27.1","Bagkee_1_BatteryTemperature","电池温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.15.27.1","Bagkee_1_InputFrequency","输入频率","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.15.27.1","Bagkee_1_BypassFrequency","旁路频率","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.15.27.1","Bagkee_1_OutputFrequency","输出频率","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.15.27.1","Bagkee_1_PhaseError","相序错误","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["10","4.15.27.1","Bagkee_1_ShutdownByBatteryLow","电池低压关机","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["11","4.15.27.1","Bagkee_1_LowBattery","电池低压","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","4","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["12","4.15.27.1","Bagkee_1_BatteryCharge","电池供电","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","3","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["13","4.15.27.1","Bagkee_1_BatteryChargeConditon","充电状态","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["14","4.15.27.1","Bagkee_1_RectifierWorking","整流器工作","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["15","4.15.27.1","Bagkee_1_InputFrequencyAnomaly","输入频率异常","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","3","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["16","4.15.27.1","Bagkee_1_ManualBypass","手动旁路","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["17","4.15.27.1","Bagkee_1_ElectricitySituation","市电情况","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["18","4.15.27.1","Bagkee_1_OutputSituation","输出情况","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["19","4.15.27.1","Bagkee_1_InverterWork","逆变器工作","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["20","4.15.27.1","Bagkee_1_UPSShutdown","UPS停机","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["21","4.15.27.1","Bagkee_1_DCBusVoltageShutdown","DC总线高压停机","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["22","4.15.27.1","Bagkee_1_ManualShutdown","手动停机","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["23","4.15.27.1","Bagkee_1_OverloadShutdown","过载停机","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["24","4.15.27.1","Bagkee_1_InverterFailureShutdown","逆变故障停机","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["25","4.15.27.1","Bagkee_1_TemperatureFaultShutdown","温度故障停机","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["26","4.15.27.1","Bagkee_1_ShortCircuitFaultShutdown","短路故障停机","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["27","4.15.27.1","Bagkee_1_AphaseInputVoltage","A相输入电压","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","3","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["28","4.15.27.1","Bagkee_1_BphaseInputVoltage","B相输入电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.15.27.1","Bagkee_1_CphaseInputVoltage","C相输入电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.15.27.1","Bagkee_1_ABypassVoltage","A相旁路电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.15.27.1","Bagkee_1_BBypassVoltage","B相旁路电压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.15.27.1","Bagkee_1_CBypassVoltage","C相旁路电压","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.15.27.1","Bagkee_1_AOutputVoltage","A相输出电压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.15.27.1","Bagkee_1_BOutputVoltage","B相输出电压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.15.27.1","Bagkee_1_COutputVoltage","C相输出电压","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.15.27.1","Bagkee_1_APhaseLoadPercentage","A相负载百分比","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.15.27.1","Bagkee_1_BPhaseLoadPercentage","B相负载百分比","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","4.15.27.1","Bagkee_1_CPhaseLoadPercentage","C相负载百分比","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","4.15.27.1","Bagkee_1_InputVoltage","输入电压","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","4.15.27.1","Bagkee_1_FailureVoltage","故障电压","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","4.15.27.1","Bagkee_1_OutputVoltage","输出电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","4.15.27.1","Bagkee_1_LoadCapacity","负载容量","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":43,"n_cols":76,"rows_kept":43,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.15.27.1","Bagkee_1_BatteryVoltage","电池电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","1","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.15.27.1","Bagkee_1_BatteryCapacity","电池容量百分比","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.15.27.1","Bagkee_1_BatteryDuration","电池维持时间","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.15.27.1","Bagkee_1_BatteryChargeCurrent","电池充电电流","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.15.27.1","Bagkee_1_BatteryTemperature","电池温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.15.27.1","Bagkee_1_InputFrequency","输入频率","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.15.27.1","Bagkee_1_BypassFrequency","旁路频率","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.15.27.1","Bagkee_1_OutputFrequency","输出频率","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.15.27.1","Bagkee_1_PhaseError","相序错误","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["10","4.15.27.1","Bagkee_1_ShutdownByBatteryLow","电池低压关机","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["11","4.15.27.1","Bagkee_1_LowBattery","电池低压","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","4","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["12","4.15.27.1","Bagkee_1_BatteryCharge","电池供电","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","3","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["13","4.15.27.1","Bagkee_1_BatteryChargeConditon","充电状态","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["14","4.15.27.1","Bagkee_1_RectifierWorking","整流器工作","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["15","4.15.27.1","Bagkee_1_InputFrequencyAnomaly","输入频率异常","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","3","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["16","4.15.27.1","Bagkee_1_ManualBypass","手动旁路","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["17","4.15.27.1","Bagkee_1_ElectricitySituation","市电情况","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["18","4.15.27.1","Bagkee_1_OutputSituation","输出情况","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["19","4.15.27.1","Bagkee_1_InverterWork","逆变器工作","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["20","4.15.27.1","Bagkee_1_UPSShutdown","UPS停机","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["21","4.15.27.1","Bagkee_1_DCBusVoltageShutdown","DC总线高压停机","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["22","4.15.27.1","Bagkee_1_ManualShutdown","手动停机","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["23","4.15.27.1","Bagkee_1_OverloadShutdown","过载停机","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["24","4.15.27.1","Bagkee_1_InverterFailureShutdown","逆变故障停机","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["25","4.15.27.1","Bagkee_1_TemperatureFaultShutdown","温度故障停机","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["26","4.15.27.1","Bagkee_1_ShortCircuitFaultShutdown","短路故障停机","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["27","4.15.27.1","Bagkee_1_AphaseInputVoltage","A相输入电压","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","3","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["28","4.15.27.1","Bagkee_1_BphaseInputVoltage","B相输入电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.15.27.1","Bagkee_1_CphaseInputVoltage","C相输入电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.15.27.1","Bagkee_1_ABypassVoltage","A相旁路电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.15.27.1","Bagkee_1_BBypassVoltage","B相旁路电压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.15.27.1","Bagkee_1_CBypassVoltage","C相旁路电压","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.15.27.1","Bagkee_1_AOutputVoltage","A相输出电压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.15.27.1","Bagkee_1_BOutputVoltage","B相输出电压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.15.27.1","Bagkee_1_COutputVoltage","C相输出电压","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.15.27.1","Bagkee_1_APhaseLoadPercentage","A相负载百分比","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.15.27.1","Bagkee_1_BPhaseLoadPercentage","B相负载百分比","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","4.15.27.1","Bagkee_1_CPhaseLoadPercentage","C相负载百分比","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","4.15.27.1","Bagkee_1_InputVoltage","输入电压","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","4.15.27.1","Bagkee_1_FailureVoltage","故障电压","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","4.15.27.1","Bagkee_1_OutputVoltage","输出电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","4.15.27.1","Bagkee_1_LoadCapacity","负载容量","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","27",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]