{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":52,"n_cols":76,"rows_kept":52,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.15.30.1","SantakQ6_1_AIPVoltage","1号UPS 输入电压","5","4","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.15.30.1","SantakQ6_1_InputFrequency","1号UPS 输入频率","5","4","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.15.30.1","SantakQ6_1_AOPVoltage","1号UPS 输出电压","5","4","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.15.30.1","SantakQ6_1_OutputFrequency","1号UPS 输出频率","5","4","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.15.30.1","SantakQ6_1_ORPMaxCurrentPrecent","1号UPS 输出电流百分比","5","4","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.15.30.1","SantakQ6_1_PBatteryVoltage","1号UPS 正电池电压","5","4","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.15.30.1","SantakQ6_1_NBatteryVoltage","1号UPS 负电池电压","5","4","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.15.30.1","SantakQ6_1_EnvTemp","1号UPS 环境温度","5","4","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.15.30.1","SantakQ6_1_RunTime","1号UPS 电池剩余运行时间","5","4","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","S","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","99999999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.15.30.1","SantakQ6_1_ChargePrecent","1号UPS 电池容量","5","4","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.15.30.1","SantakQ6_1_SysModel","1号UPS 系统模式","5","4","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.15.30.1","SantakQ6_1_BatteryModel","1号UPS 电池测试状态","5","4","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.15.30.1","SantakQ6_1_AOPPower","1号UPS 输出功率","5","4","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.15.30.1","SantakQ6_1_ACOPPower","1号UPS 视在功率","5","4","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Kva","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.15.30.1","SantakQ6_1_TotalPower","1号UPS 总输出功率","5","4","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.15.30.1","SantakQ6_1_TotalComplexPower","1号UPS 总视在功率","5","4","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Kva","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.15.30.1","SantakQ6_1_ORPCurrent","1号UPS 输出电流","5","4","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.15.30.1","SantakQ6_1_OPLoadPrecent","1号UPS 负载(%)","5","4","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.15.30.1","SantakQ6_1_UtilityFail","1号UPS 市电电压异常","5","4","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["15","4.15.30.1","SantakQ6_1_BatteryLowVol","1号UPS 电池低电压","5","4","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["16","4.15.30.1","SantakQ6_1_ByPassOn","1号UPS 旁路","5","4","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["17","4.15.30.1","SantakQ6_1_Fault","1号UPS 故障","5","4","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["18","4.15.30.1","SantakQ6_1_Standby","1号UPS 为后备式","5","4","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["19","4.15.30.1","SantakQ6_1_Shutdown","1号UPS 关机","5","4","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["34","4.15.30.1","SantakQ6_1_Communications","1号UPS 通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]
[]
["1","4.15.30.2","SantakQ6_2_AIPVoltage","2号UPS 输入电压","5","4","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.15.30.2","SantakQ6_2_InputFrequency","2号UPS 输入频率","5","4","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.15.30.2","SantakQ6_2_AOPVoltage","2号UPS 输出电压","5","4","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.15.30.2","SantakQ6_2_OutputFrequency","2号UPS 输出频率","5","4","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.15.30.2","SantakQ6_2_ORPMaxCurrentPrecent","2号UPS 输出电流百分比","5","4","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.15.30.2","SantakQ6_2_PBatteryVoltage","2号UPS 正电池电压","5","4","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.15.30.2","SantakQ6_2_NBatteryVoltage","2号UPS 负电池电压","5","4","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.15.30.2","SantakQ6_2_EnvTemp","2号UPS 环境温度","5","4","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.15.30.2","SantakQ6_2_RunTime","2号UPS 电池剩余运行时间","5","4","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","S","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","99999999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.15.30.2","SantakQ6_2_ChargePrecent","2号UPS 电池容量","5","4","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.15.30.2","SantakQ6_2_SysModel","2号UPS 系统模式","5","4","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.15.30.2","SantakQ6_2_BatteryModel","2号UPS 电池测试状态","5","4","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.15.30.2","SantakQ6_2_AOPPower","2号UPS 输出功率","5","4","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.15.30.2","SantakQ6_2_ACOPPower","2号UPS 视在功率","5","4","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Kva","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.15.30.2","SantakQ6_2_TotalPower","2号UPS 总输出功率","5","4","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.15.30.2","SantakQ6_2_TotalComplexPower","2号UPS 总视在功率","5","4","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Kva","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.15.30.2","SantakQ6_2_ORPCurrent","2号UPS 输出电流","5","4","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.15.30.2","SantakQ6_2_OPLoadPrecent","2号UPS 负载(%)","5","4","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.15.30.2","SantakQ6_2_UtilityFail","2号UPS 市电电压异常","5","4","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["15","4.15.30.2","SantakQ6_2_BatteryLowVol","2号UPS 电池低电压","5","4","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["16","4.15.30.2","SantakQ6_2_ByPassOn","2号UPS 旁路","5","4","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["17","4.15.30.2","SantakQ6_2_Fault","2号UPS 故障","5","4","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["18","4.15.30.2","SantakQ6_2_Standby","2号UPS 为后备式","5","4","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["19","4.15.30.2","SantakQ6_2_Shutdown","2号UPS 关机","5","4","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["34","4.15.30.2","SantakQ6_2_Communications","2号UPS 通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]