{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":35,"n_cols":76,"rows_kept":35,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","6.47.168.1","AIR_1_Temp","回风温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","0.1000000015","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0","0"]
["2","6.47.168.1","AIR_1_Humidity","回风湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","0.1000000015","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0","0"]
["3","6.47.168.1","AIR_1_SwitchStatus","空调开关状态","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","1","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","4","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","关机,"]
["4","6.47.168.1","AIR_1_FanStatus","风机状态","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","1","168",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","6.47.168.1","AIR_1_Compressor1Status","压缩机1状态","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","2","168",null,null,"0","1","1",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","6.47.168.1","AIR_1_Compressor2Status","压缩机2状态","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","3","168",null,null,"0","2","2",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","6.47.168.1","AIR_1_Heater1Status","加热器1状态","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","4","168",null,null,"0","3","3",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","6.47.168.1","AIR_1_Heater2Status","加热器2状态","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","5","168",null,null,"0","4","4",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","6.47.168.1","AIR_1_DehumidificationStatus","除湿状态","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","6","168",null,null,"0","5","5",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","6.47.168.1","AIR_1_WetStatus","加湿状态","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","7","168",null,null,"0","6","6",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","6.47.168.1","AIR_1_WorkStatus","空调工作状态","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","7","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"7","0","11","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","10","0,1,2,3,4,5,6,8,9,10,","告警关机,手动,逻辑关机,空调关机,告警待机,待机,静默关机,警告关机,报警关机,静默,"]
["12","6.47.168.1","AIR_1_CustomAlarmType1","自定义告警类型1","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","12","1,2,5,7,10,22,23,24,25,31,58,59,","压缩机1高压,压缩机1低压,电加热过热,风机故障,漏水,机房温度过高,机房温度过低,机房湿度过高,机房湿度过低,温湿度传感器故障,压缩机2高压,压缩机2低压,"]
["13","6.47.168.1","AIR_1_CustomAlarmType2","自定义告警类型2","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","257","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","12","1,2,5,7,10,22,23,24,25,31,58,59,","压缩机1高压,压缩机1低压,电加热过热,风机故障,漏水,机房温度过高,机房温度过低,机房湿度过高,机房湿度过低,温湿度传感器故障,压缩机2高压,压缩机2低压,"]
["14","6.47.168.1","AIR_1_CustomAlarmType3","自定义告警类型3","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","258","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","12","1,2,5,7,10,22,23,24,25,31,58,59,","压缩机1高压,压缩机1低压,电加热过热,风机故障,漏水,机房温度过高,机房温度过低,机房湿度过高,机房湿度过低,温湿度传感器故障,压缩机2高压,压缩机2低压,"]
["15","6.47.168.1","AIR_1_CustomAlarmType4","自定义告警类型4","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","259","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","12","1,2,5,7,10,22,23,24,25,31,58,59,","压缩机1高压,压缩机1低压,电加热过热,风机故障,漏水,机房温度过高,机房温度过低,机房湿度过高,机房湿度过低,温湿度传感器故障,压缩机2高压,压缩机2低压,"]
["16","6.47.168.1","AIR_1_ReturnAirTemperatureLimitUp","回风温度上限","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","6.47.168.1","AIR_1_ReturnAirTemperatureLimitDown","回风温度下限","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","6.47.168.1","AIR_1_CeilingReturnAirHumidityUp","回风湿度上限","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","6.47.168.1","AIR_1_CeilingReturnAirHumidityDown","回风湿度下限","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","6.47.168.1","AIR_1_HumiditySetPoint","空调湿度设定点","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","6.47.168.1","AIR_1_HumidityRange","空调湿度控制比例带","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","6.47.168.1","AIR_1_TempSetPoint","空调温度设定点","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","6.47.168.1","AIR_1_TempRange","空调温度控制比例带","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","6.47.168.1","AIR_1_TimeofWork","空调工作时间","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","88888","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","6.47.168.1","AIR_1_RemoteSwitch","遥控空调开关机","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","6.47.168.1","AIR_1_SetPowerOnTemperature","设定空调开机温度(NO)","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","6.47.168.1","AIR_1_SetPowerOffHumidity","设定空调关机温度(NO)","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","6.47.168.1","AIR_1_SetTemperatureLimitUp","设定回风温度上限","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","6.47.168.1","AIR_1_SetTemperatureLimitDown","设定回风温度下限","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","6.47.168.1","AIR_1_SetHumidityLimitUp","设定回风湿度上限","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","6.47.168.1","AIR_1_SetHumidityLimitDown","设定回风湿度下限","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","6.47.168.1","AIR_1_SetTemperature","设定空调温度","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","10.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","6.47.168.1","AIR_1_SetHumidity","设定空调湿度","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","6.47.168.1","AIR_1_AlarmConfirm","告警确认复位","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","0","168",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]