{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":56,"n_cols":76,"rows_kept":56,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["332","6.35.140.1","EmersonCM_ShutDownOnLine","远程关机","1","0","0","1","0","cmd-2",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["333","6.35.140.1","EmersonCM_WakeOnLine","远程开机","1","0","0","1","0","cmd-1",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["334","6.35.140.1","EmersonCM_SetTemp","一号一楼空调2温度设定","1","0","0","1","0","cmd-4",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["335","6.35.140.1","EmersonCM_SetHum","一号一楼空调2湿度设定","1","1","0","1","11","cmd-5",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["336","6.35.140.1","EmersonCM_UnitStatus","一号一楼空调2机组状态","1","1","0","1","11","cmd-6",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["337","6.35.140.1","EmersonCM_Compressor1_Status","一号一楼空调2压缩机1状态","1","1","0","1","11","cmd-8",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["338","6.35.140.1","EmersonCM_Compressor2_Status","一号一楼空调2压缩机2状态","1","1","0","1","11","cmd-9",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["339","6.35.140.1","EmersonCM_Heater1_Status","一号一楼空调2加热器1状态","1","1","0","1","11","cmd-10",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["340","6.35.140.1","EmersonCM_Heater2_Status","一号一楼空调2加热器2状态","1","1","0","1","11","cmd-11",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["341","6.35.140.1","EmersonCM_HumidifierState","一号一楼空调2加湿器状态","1","1","0","1","11","cmd-12",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["342","6.35.140.1","EmersonCM_DehumidifierState","一号一楼空调2除湿器状态","1","1","0","1","11","cmd-13",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["343","6.35.140.1","EmersonCM_FanState","一号一楼空调2风机状态","1","1","0","1","11","cmd-14",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["344","6.35.140.1","EmersonCM_CoolingMode","一号一楼空调2制冷模式","1","1","0","1","11","cmd-17",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["345","6.35.140.1","EmersonCM_HeatingMode","一号一楼空调2加热模式","1","1","0","1","11","cmd-18",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["346","6.35.140.1","EmersonCM_HumidificationMode","一号一楼空调2加湿模式","1","1","0","1","11","cmd-19",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["347","6.35.140.1","EmersonCM_DehumidificationMode","一号一楼空调2除湿模式","1","1","0","1","11","cmd-20",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["348","6.35.140.1","EmersonCM_AirTemperature","一号一楼空调2空调温度","1","1","0","1","11","cmd-22",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["349","6.35.140.1","EmersonCM_AirHumidity","一号一楼空调2空调湿度","1","1","0","1","11","cmd-23",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["350","6.35.140.1","EmersonCM_HighTemperatureAlarm","一号一楼空调1高温","1","1","0","1","11","cmd-24",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["351","6.35.140.1","EmersonCM_LowTemperatureAlarm","一号一楼空调1低温","1","1","0","1","11","cmd-25",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["352","6.35.140.1","EmersonCM_HighHumidityAlarm","一号一楼空调1高湿","1","1","0","1","11","cmd-26",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["353","6.35.140.1","EmersonCM_LowHumidityAlarm","一号一楼空调1低湿","1","1","0","1","11","cmd-27",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["354","6.35.140.1","EmersonCM_AirLossAlarm","一号一楼空调1气流丢失","1","1","0","1","11","cmd-28",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["355","6.35.140.1","EmersonCM_LowPressureCompressor1_Alarm","一号一楼空调1压缩机1低压","1","1","0","1","11","cmd-30",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["356","6.35.140.1","EmersonCM_HighPressureCompressor1_Alarm","一号一楼空调1压缩机1高压","1","1","0","1","11","cmd-31",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["357","6.35.140.1","EmersonCM_LowPressureCompressor2_Alarm","一号一楼空调1压缩机2低压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["358","6.35.140.1","EmersonCM_HighPressureCompressor2_Alarm","一号一楼空调1压缩机2高压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["359","6.35.140.2","EmersonCM_2_ShutDownOnLine","远程关机","1","0","0","1","0","cmd-2",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["360","6.35.140.2","EmersonCM_2_WakeOnLine","远程开机","1","0","0","1","0","cmd-1",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["361","6.35.140.2","EmersonCM_2_SetTemp","一号一楼空调2温度设定","1","0","0","1","0","cmd-4",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["362","6.35.140.2","EmersonCM_2_SetHum","一号一楼空调2湿度设定","1","1","0","1","11","cmd-5",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["363","6.35.140.2","EmersonCM_2_UnitStatus","一号一楼空调2机组状态","1","1","0","1","11","cmd-6",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["364","6.35.140.2","EmersonCM_2_Compressor1_Status","一号一楼空调2压缩机1状态","1","1","0","1","11","cmd-8",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["365","6.35.140.2","EmersonCM_2_Compressor2_Status","一号一楼空调2压缩机2状态","1","1","0","1","11","cmd-9",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["366","6.35.140.2","EmersonCM_2_Heater1_Status","一号一楼空调2加热器1状态","1","1","0","1","11","cmd-10",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["367","6.35.140.2","EmersonCM_2_Heater2_Status","一号一楼空调2加热器2状态","1","1","0","1","11","cmd-11",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["368","6.35.140.2","EmersonCM_2_HumidifierState","一号一楼空调2加湿器状态","1","1","0","1","11","cmd-12",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["369","6.35.140.2","EmersonCM_2_DehumidifierState","一号一楼空调2除湿器状态","1","1","0","1","11","cmd-13",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["370","6.35.140.2","EmersonCM_2_FanState","一号一楼空调2风机状态","1","1","0","1","11","cmd-14",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["371","6.35.140.2","EmersonCM_2_CoolingMode","一号一楼空调2制冷模式","1","1","0","1","11","cmd-17",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["372","6.35.140.2","EmersonCM_2_HeatingMode","一号一楼空调2加热模式","1","1","0","1","11","cmd-18",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["373","6.35.140.2","EmersonCM_2_HumidificationMode","一号一楼空调2加湿模式","1","1","0","1","11","cmd-19",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["374","6.35.140.2","EmersonCM_2_DehumidificationMode","一号一楼空调2除湿模式","1","1","0","1","11","cmd-20",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["375","6.35.140.2","EmersonCM_2_AirTemperature","一号一楼空调2空调温度","1","1","0","1","11","cmd-22",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["376","6.35.140.2","EmersonCM_2_AirHumidity","一号一楼空调2空调湿度","1","1","0","1","11","cmd-23",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["377","6.35.140.2","EmersonCM_2_HighTemperatureAlarm","一号一楼空调2高温","1","1","0","1","11","cmd-24",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["378","6.35.140.2","EmersonCM_2_LowTemperatureAlarm","一号一楼空调2低温","1","1","0","1","11","cmd-25",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["379","6.35.140.2","EmersonCM_2_HighHumidityAlarm","一号一楼空调2高湿","1","1","0","1","11","cmd-26",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["380","6.35.140.2","EmersonCM_2_LowHumidityAlarm","一号一楼空调2低湿","1","1","0","1","11","cmd-27",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["381","6.35.140.2","EmersonCM_2_AirLossAlarm","一号一楼空调2气流丢失","1","1","0","1","11","cmd-28",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["382","6.35.140.2","EmersonCM_2_LowPressureCompressor1_Alarm","一号一楼空调2压缩机1低压","1","1","0","1","11","cmd-30",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["383","6.35.140.2","EmersonCM_2_HighPressureCompressor1_Alarm","一号一楼空调2压缩机1高压","1","1","0","1","11","cmd-31",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["384","6.35.140.2","EmersonCM_2_LowPressureCompressor2_Alarm","一号一楼空调2压缩机2低压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["385","6.35.140.2","EmersonCM_2_HighPressureCompressor2_Alarm","一号一楼空调2压缩机2高压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["441","6.35.140.1","EmersonCM_1_ComStatus","一号楼一楼空调串口通信","1000","0","0","1","0","cmd-10",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":56,"n_cols":76,"rows_kept":56,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["332","6.35.140.1","EmersonCM_ShutDownOnLine","远程关机","1","0","0","1","0","cmd-2",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["333","6.35.140.1","EmersonCM_WakeOnLine","远程开机","1","0","0","1","0","cmd-1",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["334","6.35.140.1","EmersonCM_SetTemp","一号一楼空调2温度设定","1","0","0","1","0","cmd-4",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["335","6.35.140.1","EmersonCM_SetHum","一号一楼空调2湿度设定","1","1","0","1","11","cmd-5",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["336","6.35.140.1","EmersonCM_UnitStatus","一号一楼空调2机组状态","1","1","0","1","11","cmd-6",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["337","6.35.140.1","EmersonCM_Compressor1_Status","一号一楼空调2压缩机1状态","1","1","0","1","11","cmd-8",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["338","6.35.140.1","EmersonCM_Compressor2_Status","一号一楼空调2压缩机2状态","1","1","0","1","11","cmd-9",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["339","6.35.140.1","EmersonCM_Heater1_Status","一号一楼空调2加热器1状态","1","1","0","1","11","cmd-10",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["340","6.35.140.1","EmersonCM_Heater2_Status","一号一楼空调2加热器2状态","1","1","0","1","11","cmd-11",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["341","6.35.140.1","EmersonCM_HumidifierState","一号一楼空调2加湿器状态","1","1","0","1","11","cmd-12",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["342","6.35.140.1","EmersonCM_DehumidifierState","一号一楼空调2除湿器状态","1","1","0","1","11","cmd-13",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["343","6.35.140.1","EmersonCM_FanState","一号一楼空调2风机状态","1","1","0","1","11","cmd-14",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["344","6.35.140.1","EmersonCM_CoolingMode","一号一楼空调2制冷模式","1","1","0","1","11","cmd-17",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["345","6.35.140.1","EmersonCM_HeatingMode","一号一楼空调2加热模式","1","1","0","1","11","cmd-18",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["346","6.35.140.1","EmersonCM_HumidificationMode","一号一楼空调2加湿模式","1","1","0","1","11","cmd-19",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["347","6.35.140.1","EmersonCM_DehumidificationMode","一号一楼空调2除湿模式","1","1","0","1","11","cmd-20",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["348","6.35.140.1","EmersonCM_AirTemperature","一号一楼空调2空调温度","1","1","0","1","11","cmd-22",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["349","6.35.140.1","EmersonCM_AirHumidity","一号一楼空调2空调湿度","1","1","0","1","11","cmd-23",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["350","6.35.140.1","EmersonCM_HighTemperatureAlarm","一号一楼空调1高温","1","1","0","1","11","cmd-24",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["351","6.35.140.1","EmersonCM_LowTemperatureAlarm","一号一楼空调1低温","1","1","0","1","11","cmd-25",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["352","6.35.140.1","EmersonCM_HighHumidityAlarm","一号一楼空调1高湿","1","1","0","1","11","cmd-26",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["353","6.35.140.1","EmersonCM_LowHumidityAlarm","一号一楼空调1低湿","1","1","0","1","11","cmd-27",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["354","6.35.140.1","EmersonCM_AirLossAlarm","一号一楼空调1气流丢失","1","1","0","1","11","cmd-28",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["355","6.35.140.1","EmersonCM_LowPressureCompressor1_Alarm","一号一楼空调1压缩机1低压","1","1","0","1","11","cmd-30",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["356","6.35.140.1","EmersonCM_HighPressureCompressor1_Alarm","一号一楼空调1压缩机1高压","1","1","0","1","11","cmd-31",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["357","6.35.140.1","EmersonCM_LowPressureCompressor2_Alarm","一号一楼空调1压缩机2低压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["358","6.35.140.1","EmersonCM_HighPressureCompressor2_Alarm","一号一楼空调1压缩机2高压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["359","6.35.140.2","EmersonCM_2_ShutDownOnLine","远程关机","1","0","0","1","0","cmd-2",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["360","6.35.140.2","EmersonCM_2_WakeOnLine","远程开机","1","0","0","1","0","cmd-1",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["361","6.35.140.2","EmersonCM_2_SetTemp","一号一楼空调2温度设定","1","0","0","1","0","cmd-4",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["362","6.35.140.2","EmersonCM_2_SetHum","一号一楼空调2湿度设定","1","1","0","1","11","cmd-5",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["363","6.35.140.2","EmersonCM_2_UnitStatus","一号一楼空调2机组状态","1","1","0","1","11","cmd-6",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["364","6.35.140.2","EmersonCM_2_Compressor1_Status","一号一楼空调2压缩机1状态","1","1","0","1","11","cmd-8",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["365","6.35.140.2","EmersonCM_2_Compressor2_Status","一号一楼空调2压缩机2状态","1","1","0","1","11","cmd-9",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["366","6.35.140.2","EmersonCM_2_Heater1_Status","一号一楼空调2加热器1状态","1","1","0","1","11","cmd-10",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["367","6.35.140.2","EmersonCM_2_Heater2_Status","一号一楼空调2加热器2状态","1","1","0","1","11","cmd-11",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["368","6.35.140.2","EmersonCM_2_HumidifierState","一号一楼空调2加湿器状态","1","1","0","1","11","cmd-12",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["369","6.35.140.2","EmersonCM_2_DehumidifierState","一号一楼空调2除湿器状态","1","1","0","1","11","cmd-13",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["370","6.35.140.2","EmersonCM_2_FanState","一号一楼空调2风机状态","1","1","0","1","11","cmd-14",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["371","6.35.140.2","EmersonCM_2_CoolingMode","一号一楼空调2制冷模式","1","1","0","1","11","cmd-17",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["372","6.35.140.2","EmersonCM_2_HeatingMode","一号一楼空调2加热模式","1","1","0","1","11","cmd-18",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["373","6.35.140.2","EmersonCM_2_HumidificationMode","一号一楼空调2加湿模式","1","1","0","1","11","cmd-19",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["374","6.35.140.2","EmersonCM_2_DehumidificationMode","一号一楼空调2除湿模式","1","1","0","1","11","cmd-20",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["375","6.35.140.2","EmersonCM_2_AirTemperature","一号一楼空调2空调温度","1","1","0","1","11","cmd-22",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["376","6.35.140.2","EmersonCM_2_AirHumidity","一号一楼空调2空调湿度","1","1","0","1","11","cmd-23",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["377","6.35.140.2","EmersonCM_2_HighTemperatureAlarm","一号一楼空调2高温","1","1","0","1","11","cmd-24",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["378","6.35.140.2","EmersonCM_2_LowTemperatureAlarm","一号一楼空调2低温","1","1","0","1","11","cmd-25",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["379","6.35.140.2","EmersonCM_2_HighHumidityAlarm","一号一楼空调2高湿","1","1","0","1","11","cmd-26",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["380","6.35.140.2","EmersonCM_2_LowHumidityAlarm","一号一楼空调2低湿","1","1","0","1","11","cmd-27",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["381","6.35.140.2","EmersonCM_2_AirLossAlarm","一号一楼空调2气流丢失","1","1","0","1","11","cmd-28",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["382","6.35.140.2","EmersonCM_2_LowPressureCompressor1_Alarm","一号一楼空调2压缩机1低压","1","1","0","1","11","cmd-30",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["383","6.35.140.2","EmersonCM_2_HighPressureCompressor1_Alarm","一号一楼空调2压缩机1高压","1","1","0","1","11","cmd-31",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["384","6.35.140.2","EmersonCM_2_LowPressureCompressor2_Alarm","一号一楼空调2压缩机2低压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["385","6.35.140.2","EmersonCM_2_HighPressureCompressor2_Alarm","一号一楼空调2压缩机2高压","1","1","0","1","11","cmd-32",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","0,","报警,"]
["441","6.35.140.1","EmersonCM_1_ComStatus","一号楼一楼空调串口通信","1000","0","0","1","0","cmd-10",null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","140","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]