{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":42,"n_cols":76,"rows_kept":42,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.3.5.1","AP9622_1_TempExceeded","空调* 内部温度过高","4","2","1","3","1",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","1","5",null,null,"0","6","6",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["2","4.3.5.1","AP9622_1_BypassByFault","空调* 故障转旁路","4","2","1","3","2",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","2","5",null,null,"0","4","4",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["2","4.3.5.1","AP9622_1_LowBattery","空调* 低电池","4","2","1","3","3",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","3","5",null,null,"0","6","6",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["3","4.3.5.1","AP9622_1_Overload","空调* 过载","4","2","1","3","3",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","4","5",null,null,"0","5","5",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["4","4.3.5.1","AP9622_1_BatteryVoltageHigh","空调* 电池电压高","4","2","1","3","4",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","5","5",null,null,"0","8","8",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["5","4.3.5.1","AP9622_1_OutputVoltageOut","空调* 输出电压超限","4","2","1","3","4",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","6","5",null,null,"0","5","5",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["6","4.3.5.1","AP9622_1_BypassByOverload","空调* 过载转旁路","4","2","1","3","5",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","7","5",null,null,"0","11","11",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["7","4.3.5.1","AP9622_1_BypassOutOfRange","空调* 旁路超限","4","2","1","3","5",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","8","5",null,null,"0","7","7",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["8","4.3.5.1","AP9622_1_CapacitorsLowCurrent","空调* 电容器电流故障","4","2","1","3","6",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","9","5",null,null,"0","10","10",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["9","4.3.5.1","AP9622_1_BatteryMonitorAlarm","空调* 电池监视器","4","2","1","3","6",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","10","5",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["10","4.3.5.1","AP9622_1_RectifierFuseBlown","空调* 整流器保险丝","4","2","1","3","7",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","11","5",null,null,"0","1","1",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["11","4.3.5.1","AP9622_1_InverterFuseBlown","空调* 逆变器保险丝","4","2","1","3","7",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","12","5",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["12","4.3.5.1","AP9622_1_HighBatteryTemp","空调* 电池高温","4","2","1","3","9",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","13","5",null,null,"0","9","9",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["13","4.3.5.1","AP9622_1_BatteryCapacity","空调* 电池容量","4","2","1","3","17",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.3.5.1","AP9622_1_RuntimeRemaining","空调* 电池剩余时间","4","2","1","3","18",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.3.5.1","AP9622_1_BatteryVoltage","空调* 电池电压","4","2","1","3","22",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.3.5.1","AP9622_1_InternalTemp","空调* 内部温度","4","2","1","3","19",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.3.5.1","AP9622_1_BatteryCurrent","空调* 电池电流","4","2","1","3","23",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.3.5.1","AP9622_1_OutputFrequency","空调* 输出频率","4","2","1","3","24",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.3.5.1","AP9622_1_InputVoltageA","空调* A相输入电压","4","2","1","3","25",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.3.5.1","AP9622_1_InputVoltageB","空调* B相输入电压","4","2","1","3","26",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.3.5.1","AP9622_1_InputVoltageC","空调* C相输入电压","4","2","1","3","27",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.3.5.1","AP9622_1_InputCurrentA","空调* A相输入电流","4","2","1","3","28",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.3.5.1","AP9622_1_InputCurrentB","空调* B相输入电流","4","2","1","3","29",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.3.5.1","AP9622_1_InputCurrentC","空调* C相输入电流","4","2","1","3","30",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.3.5.1","AP9622_1_BypassInputVoltageA","空调* A相旁路电压","4","2","1","3","31",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.3.5.1","AP9622_1_BypassInputVoltageB","空调* B相旁路电压","4","2","1","3","32",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.3.5.1","AP9622_1_BypassInputVoltageC","空调* C相旁路电压","4","2","1","3","33",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.3.5.1","AP9622_1_OutputActiveA","空调* A相有功功率","4","2","1","3","40",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Kw","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.3.5.1","AP9622_1_OutputActiveB","空调* B相有功功率","4","2","1","3","41",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Kw","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.3.5.1","AP9622_1_OutputActiveC","空调* C相有功功率","4","2","1","3","42",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Kw","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","4.3.5.1","AP9622_1_OutputVoltageA","空调* A相输出电压","4","2","1","3","49",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","4.3.5.1","AP9622_1_OutputVoltageB","空调* B相输出电压","4","2","1","3","50",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.3.5.1","AP9622_1_OutputVoltageC","空调* C相输出电压","4","2","1","3","51",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","4.3.5.1","AP9622_1_OutputCurrentA","空调* A相输出电流","4","2","1","3","52",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["35","4.3.5.1","AP9622_1_OutputCurrentB","空调* B相输出电流","4","2","1","3","53",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","4.3.5.1","AP9622_1_OutputCurrentC","空调* C相输出电流","4","2","1","3","54",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","4.3.5.1","AP9622_1_OutputLoadA","空调* A相输出负载","4","2","1","3","33",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["35","4.3.5.1","AP9622_1_OutputLoadB","空调* B相输出负载","4","2","1","3","34",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","4.3.5.1","AP9622_1_OutputLoadC","空调* C相输出负载","4","2","1","3","35",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.3.5.1","AP9622_NetStatus","空调* 通讯状态状态","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","5",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]