{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":34,"n_cols":76,"rows_kept":34,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.38.1","UPS* 1_nxl_systemStatus","UPS* 系统状态","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.1.1.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","告警,"]
["2","4.19.38.1","UPS* 1_nxl_inletAirTemperature","UPS* 进风温度","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.1.2.0","public","0","0","0","0","5","35","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"20","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.38.1","UPS* 1_nxl_dcBusVoltage","UPS* 直流母线电压","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.1.3.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.38.1","UPS* 1_nxl_inputLineVoltageAB","UPS* 输入线电压AB","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.2.1.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.38.1","UPS* 1_nxl_inputLineVoltageBC","UPS* 输入线电压BC","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.2.2.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.38.1","UPS* 1_nxl_inputLineVoltageCA","UPS* 输入线电压CA","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.2.3.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.38.1","UPS* 1_nxl_inputCurrentA","UPS* 输入电流A","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.2.4.0","public","0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.38.1","UPS* 1_nxl_inputCurrentB","UPS* 输入电流B","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.2.5.0","public","0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.38.1","UPS* 1_nxl_inputCurrentC","UPS* 输入电流C","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.2.6.0","public","0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.38.1","UPS* 1_nxl_inputFrequency","UPS* 输入频率","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.2.7.0","public","0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"45","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.38.1","UPS* 1_nxl_outputPhaseVoltageA","UPS* 输出相电压A","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.1.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.38.1","UPS* 1_nxl_outputPhaseVoltageB","UPS* 输出相电压B","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.2.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.38.1","UPS* 1_nxl_outputPhaseVoltageC","UPS* 输出相电压C","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.3.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.38.1","UPS* 1_nxl_outputLineVoltageAB","UPS* 输出线电压AB","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.4.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.38.1","UPS* 1_nxl_outputLineVoltageBC","UPS* 输出线电压BC","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.5.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.38.1","UPS* 1_nxl_outputLineVoltageCA","UPS* 输出线电压CA","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.6.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.38.1","UPS* 1_nxl_outputCurrentA","UPS* 输出电流A","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.7.0","public","0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.38.1","UPS* 1_nxl_outputCurrentB","UPS* 输出电流B","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.8.0","public","0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.38.1","UPS* 1_nxl_outputCurrentC","UPS* 输出电流C","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.9.0","public","0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.38.1","UPS* 1_nxl_outputFrequency","UPS* 输出频率","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.10.0","public","0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.38.1","UPS* 1_nxl_outputActivePower","UPS* 输出有功功率","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.11.0","public","0","0","0","0","0","0","0","0","0","Kw","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.38.1","UPS* 1_nxl_outputApparentPower","UPS* 输出视在功率","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.12.0","public","0","0","0","0","0","0","0","0","0","Kw","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.38.1","UPS* 1_nxl_outputLoadA","UPS* 输出负载A","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.13.0","public","0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.38.1","UPS* 1_nxl_outputLoadB","UPS* 输出负载B","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.14.0","public","0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.38.1","UPS* 1_nxl_outputLoadC","UPS* 输出负载C","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.3.15.0","public","0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.38.1","UPS* 1_nxl_batteryCurrent","UPS* 电池电流","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.4.1.0","public","0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.38.1","UPS* 1_nxl_batteryCapacity","UPS* 电池容量","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.4.2.0","public","0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.38.1","UPS* 1_nxl_batteryTimeRemaining","UPS* 电池剩余时间","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.4.3.0","public","0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","8888","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.38.1","UPS* 1_nxl_bypassLineVoltageAB","UPS* 旁路线电压AB","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.5.1.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.38.1","UPS* 1_nxl_bypassLineVoltageBC","UPS* 旁路线电压BC","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.5.2.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","4.19.38.1","UPS* 1_nxl_bypassLineVoltageCA","UPS* 旁路线电压CA","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.5.3.0","public","0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","4.19.38.1","UPS* 1_nxl_bypassFrequency","UPS* 旁路频率","1","0","0","1","0",null,null,"0","60","720","1","1.3.6.1.4.1.13400.2.18.2.5.4.0","public","0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.19.38.1","UPS* 1_nxl_NetStatus","UPS* 通信状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","38",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]