{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":35,"n_cols":76,"rows_kept":35,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.136.1","UH31_1_ACInputPhaseVoltageA","UPS* 交流输入相电压A","101","4","0","1","0","cmd-1","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.136.1","UH31_1_ACInputPhaseVoltageB","UPS* 交流输入相电压B","101","4","0","1","0","cmd-2","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.136.1","UH31_1_ACInputPhaseVoltageC","UPS* 交流输入相电压C","101","4","0","1","0","cmd-3","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.136.1","UH31_1_ACOutputPhaseVoltageA","UPS* 交流输出相电压A","101","4","0","1","0","cmd-4","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.136.1","UH31_1_ACOutputPhaseVoltageB","UPS* 交流输出相电压B","101","4","0","1","0","cmd-5","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.136.1","UH31_1_ACOutputPhaseVoltageC","UPS* 交流输出相电压C","101","4","0","1","0","cmd-6","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.136.1","UH31_1_ACOutputCurrentA","UPS* 交流输出电流A","101","4","0","1","0","cmd-7","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.136.1","UH31_1_ACOutputCurrentB","UPS* 交流输出电流B","101","4","0","1","0","cmd-8","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.136.1","UH31_1_ACOutputCurrentC","UPS* 交流输出电流C","101","4","0","1","0","cmd-9","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.136.1","UH31_1_OutputFrequent","UPS* 输出频率","101","4","0","1","0","cmd-11","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.136.1","UH31_1_ACInputFrequency","UPS* 交流输入频率","101","4","0","1","0","cmd-15","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.136.1","UH31_1_LoadSize","UPS* 负载","101","4","0","1","0","cmd-16","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.136.1","UH31_1_BatteryCapacity","UPS* 电池容量","101","4","0","1","0","cmd-17","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.136.1","UH31_1_MachineTemperature","UPS* 机内温度","101","4","0","1","0","cmd-18","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","℃","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.136.1","UH31_1_BypassVoltage","UPS* 旁路电压","101","4","0","1","0","cmd-19","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.136.1","UH31_1_BatteryVoltageNegativeGroup","UPS* 负组电池电压","101","4","0","1","0","cmd-20","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.136.1","UH31_1_PowerSupply","UPS* 供电方式","1","1","0","1","0","cmd-21","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.136.1","UH31_1_PowerShutdown","UPS* 开机关机","1","1","0","1","0","cmd-26","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.136.1","UH31_1_UPSSupply","UPS* 供电","1","1","0","1","0","cmd-27","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.136.1","UH31_1_APhaseMainsVoltage","UPS* A相市电电压","1","1","0","1","0","cmd-29","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","3","1,2,224,","掉电，超限,欠压，"]
["21","4.19.136.1","UH31_1_Rectifier","UPS* 整流器","1","1","0","1","0","cmd-30","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","故障,"]
["22","4.19.136.1","UH31_1_Reversible","UPS* 逆变器","1","1","0","1","0","cmd-31","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","故障,"]
["23","4.19.136.1","UH31_1_BypassVolatage","UPS* 旁路电压","1","1","0","1","0","cmd-32","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","1，2,","低于下限，超限,"]
["24","4.19.136.1","UH31_1_TheTotalBatteryVoltage","UPS* 蓄电池总电压","1","1","0","1","0","cmd-33","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","4","1,2,240,227，","低于下限，高于上限,故障，预告警，"]
["25","4.19.136.1","UH31_1_ChargerFault","UPS* 充电器故障","1","1","0","1","0","cmd-36","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","报警,"]
["26","4.19.136.1","UH31_1_OutputShortCircuit","UPS* 输出短路","1","1","0","1","0","cmd-37","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","报警,"]
["27","4.19.136.1","UH31_1_OutputOverload","UPS* 输出过载","1","1","0","1","0","cmd-38","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","报警,"]
["28","4.19.136.1","UH31_1_RadiatorTemperature","UPS* 散热器温度","1","1","0","1","0","cmd-39","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","过高,"]
["29","4.19.136.1","UH31_1_MainsFrequency","UPS* 市电频率","1","1","0","1","0","cmd-40","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","224,","超限,"]
["30","4.19.136.1","UH31_1_LackOfZeroFault","UPS* 缺零故障","1","1","0","1","0","cmd-41","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","224,","报警,"]
["31","4.19.136.1","UH31_1_InputPhase","UPS* 输入缺相","1","1","0","1","0","cmd-42","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","224,","报警,"]
["32","4.19.136.1","UH31_1_BPhaseMainsVoltage","UPS* B相市电电压","1","1","0","1","0","cmd-43","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","3","1,2,224,","掉电，超限,欠压，"]
["33","4.19.136.1","UH31_1_CPhaseMainsVoltage","UPS* C相市电电压","1","1","0","1","0","cmd-44","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","3","1,2,224,","掉电，超限,欠压，"]
["34","4.19.136.1","UH31_1_status","UPS* 通信状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","136",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]