{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":70,"n_cols":76,"rows_kept":70,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.40.1","UL33_1_AC_InputPhaseVoltageA","UPS* 交流输入相电压A","1","0","0","1","0","cmd-1","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.40.1","UL33_1_AC_InputPhaseVoltageB","UPS* 交流输入相电压B","1","0","0","1","0","cmd-2","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.40.1","UL33_1_AC_InputPhaseVoltageC","UPS* 交流输入相电压C","1","0","0","1","0","cmd-3","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.40.1","UL33_1_AC_OutputPhaseVoltageA","UPS* 交流输出相电压A","1","0","0","1","0","cmd-4","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.40.1","UL33_1_AC_OutputPhaseVoltageB","UPS* 交流输出相电压B","1","0","0","1","0","cmd-5","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.40.1","UL33_1_AC_OutputPhaseVoltageC","UPS* 交流输出相电压C","1","0","0","1","0","cmd-6","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.40.1","UL33_1_AC_OutputCurrentA","UPS* 交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.40.1","UL33_1_AC_OutputCurrentB","UPS* 交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.40.1","UL33_1_AC_OutputCurrentC","UPS* 交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.40.1","UL33_1_AC_BatteryVoltage","UPS* 电池电压","1","0","0","1","0","cmd-10","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.40.1","UL33_1_AC_OutputFrequency","UPS* 输出频率（三相一致）","1","0","0","1","0","cmd-11","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.40.1","UL33_1_AC_InputLineVoltageAB","UPS* 交流输入线电压AB","1","0","0","1","0","cmd-12","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.40.1","UL33_1_AC_InputLineVoltageBC","UPS* 交流输入线电压BC","1","0","0","1","0","cmd-13","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.40.1","UL33_1_AC_InputLineVoltageCA","UPS* 交流输入线电压CA","1","0","0","1","0","cmd-14","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.40.1","UL33_1_ACInputCurrentA","UPS* A相输入电流","1","0","0","1","0","cmd-15","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","50","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.40.1","UL33_1_ACInputCurrentB","UPS* B相输入电流","1","0","0","1","0","cmd-16","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","50","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.40.1","UL33_1_ACInputCurrentC","UPS* C相输入电流","1","0","0","1","0","cmd-17","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","50","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.40.1","UL33_1_ACInputFrequency","UPS* 输入频率（三相一致）","1","0","0","1","0","cmd-18","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.40.1","UL33_1_ACAphaseBypassVoltage","UPS* A相旁路电压","1","0","0","1","0","cmd-19","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.40.1","UL33_1_ACBphaseBypassVoltage","UPS* B相旁路电压","1","0","0","1","0","cmd-20","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.40.1","UL33_1_ACCphaseBypassVoltage","UPS* C相旁路电压","1","0","0","1","0","cmd-21","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.40.1","UL33_1_ACAphaseBypassCurrent","UPS* A相旁路电流","1","0","0","1","0","cmd-22","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.40.1","UL33_1_ACBphaseBypassCurrent","UPS* B相旁路电流","1","0","0","1","0","cmd-23","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.40.1","UL33_1_ACCphaseBypassCurrent","UPS* C相旁路电流","1","0","0","1","0","cmd-24","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.40.1","UL33_1_ACBypassFrequency","UPS* 旁路频率（三相一致）","1","0","0","1","0","cmd-25","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.40.1","UL33_1_ACBatteryTemperature","UPS* 电池温度","1","0","0","1","0","cmd-26","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","℃","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.40.1","UL33_1_ACAphaseOutputActivePower","UPS* A相输出有功功率","1","0","0","1","0","cmd-27","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","KW","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","-32767","32767","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.40.1","UL33_1_ACBphaseOutputActivePower","UPS* B相输出有功功率","1","0","0","1","0","cmd-28","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","KW","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","-32767","32767","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.40.1","UL33_1_ACCphaseOutputActivePower","UPS* C相输出有功功率","1","0","0","1","0","cmd-29","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","KW","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","-32767","32767","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.40.1","UL33_1_ACBatteryCurrent","UPS* 电池电流","1","0","0","1","0","cmd-30","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","A","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","4.19.40.1","UL33_1_ACRemainingBatteryBackupTime","UPS* 电池剩余后备时间","1","0","0","1","0","cmd-31","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Min","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","4.19.40.1","UL33_1_ACAphaseOutputApparentPower","UPS* A相输出视在功率","1","0","0","1","0","cmd-32","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","KW","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","-32767","32767","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.19.40.1","UL33_1_ACBphaseOutputApparentPower","UPS* B相输出视在功率","1","0","0","1","0","cmd-33","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","KW","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","-32767","32767","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","4.19.40.1","UL33_1_ACCphaseOutputApparentPower","UPS* C相输出视在功率","1","0","0","1","0","cmd-34","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","KW","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","-32767","32767","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["35","4.19.40.1","UL33_1_ACAphaseOutputpercentage","UPS* A相输出负载百分比","1","0","0","1","0","cmd-35","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","4.19.40.1","UL33_1_ACBphaseOutputpercentage","UPS* B相输出负载百分比","1","0","0","1","0","cmd-36","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["37","4.19.40.1","UL33_1_ACCphaseOutputpercentage","UPS* C相输出负载百分比","1","0","0","1","0","cmd-37","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["38","4.19.40.1","UL33_1_ACTemperature","UPS* 环境温度","1","0","0","1","0","cmd-38","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","℃","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["39","4.19.40.1","UL33_1_ACAphaseOutputPeakRatio","UPS* A相输出峰值比","1","0","0","1","0","cmd-39","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["40","4.19.40.1","UL33_1_ACBphaseOutputPeakRatio","UPS* B相输出峰值比","1","0","0","1","0","cmd-40","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["41","4.19.40.1","UL33_1_ACCphaseOutputPeakRatio","UPS* C相输出峰值比","1","0","0","1","0","cmd-41","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["42","4.19.40.1","UL33_1_ACPowerSupply","UPS* 供电方式","1","0","0","1","0","cmd-42","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","1","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"1","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","2,233,","旁路供电,均不供电,"]
["43","4.19.40.1","UL33_1_ACBatterySelfTest","UPS* 电池自检状态","1","0","0","1","0","cmd-43","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["44","4.19.40.1","UL33_1_ACAllChargeOrFloat","UPS* 均充/浮充（正组）","1","0","0","1","0","cmd-44","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["45","4.19.40.1","UL33_1_ACOffState","UPS* 开机/关机","1","0","0","1","0","cmd-45","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","228","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"228","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","229,","UPS关机,"]
["46","4.19.40.1","UL33_1_ACUPSPowerSupply","UPS* 供电","1","0","0","1","0","cmd-46","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","232","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"232","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","3","231,232,233，","电池逆变供电，市电逆变供电，市电电池联合供电,"]
["47","4.19.40.1","UL33_1_ACSynORasynchronous","UPS* 同步/不同步","1","0","0","1","0","cmd-53","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["48","4.19.40.1","UL33_1_ACMainsVoltage","UPS* 市电电压","1","0","0","1","0","cmd-54","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","2，3,","异常，欠压,"]
["49","4.19.40.1","UL33_1_ACRectifierStatus","UPS* 整流器状态","1","0","0","1","0","cmd-55","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","故障,"]
["50","4.19.40.1","UL33_1_ACInverterStatus","UPS* 逆变器状态","1","0","0","1","0","cmd-56","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","249,","故障,"]
["51","4.19.40.1","UL33_1_ACBypassConditions","UPS* 旁路情况（电压或频率）","1","0","0","1","0","cmd-57","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","2","1，2,","超出跟踪范围，超出保护范围,"]
["52","4.19.40.1","UL33_1_ACTheTotalBatteryVoltageStatus","UPS* 蓄电池总电压状态","1","0","0","1","0","cmd-58","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","5","1,2,3,240，225,","电池无，低于下限，高于上限，接反，预告警,"]
["53","4.19.40.1","UL33_1_ACBatterySelfTestResults","UPS* 电池自检结果","1","0","0","1","0","cmd-59","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","需要更换电池,"]
["54","4.19.40.1","UL33_1_ACMainsFrequency","UPS* 市电频率","1","0","0","1","0","cmd-60","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","异常,"]
["55","4.19.40.1","UL33_1_ACInverterFanFailure","UPS* 逆变风扇故障","1","0","0","1","0","cmd-68","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["56","4.19.40.1","UL33_1_ACRectifierFanFailure","UPS* 整流风扇故障","1","0","0","1","0","cmd-69","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["57","4.19.40.1","UL33_1_ACBatteryContactorFailure","UPS* 电池接触器故障","1","0","0","1","0","cmd-70","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["58","4.19.40.1","UL33_1_ACMainRoadContactorException","UPS* 主路接触器异常","1","0","0","1","0","cmd-71","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["59","4.19.40.1","UL33_1_ACOutputOverload","UPS* 本机输出过载","1","0","0","1","0","cmd-75","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","过载,"]
["60","4.19.40.1","UL33_1_ACAbnormalShutdownBypass","UPS* 旁路异常关机","1","0","0","1","0","cmd-81","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","异常,"]
["61","4.19.40.1","UL33_1_AC_OutputOvervoltage","UPS* 交流输出过压","1","0","0","1","0","cmd-85","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","异常,"]
["62","4.19.40.1","UL33_1_ACCurrentOutput","UPS* 输出冲击过流","1","0","0","1","0","cmd-86","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","故障,"]
["63","4.19.40.1","UL33_1_ACOverCurrentInverter","UPS* 逆变模块过流","1","0","0","1","0","cmd-87","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","故障,"]
["64","4.19.40.1","UL33_1_ACOverCurrentRectifier","UPS* 整流模块过流","1","0","0","1","0","cmd-88","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","故障,"]
["65","4.19.40.1","UL33_1_ACBypassLoadImpact","UPS* 负载冲击转旁路","1","0","0","1","0","cmd-89","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","240,","故障,"]
["66","4.19.40.1","UL33_1_ACTemperatureHigh","UPS* 环境温度过高","1","0","0","1","0","cmd-94","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","告警,"]
["67","4.19.40.1","UL33_1_ACRectifierCommunicationFailure","UPS* 整流通讯故障","1","0","0","1","0","cmd-95","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","240,","告警,"]
["68","4.19.40.1","UL33_1_ACInverterCommunicationFailure","UPS* 逆变通讯故障","1","0","0","1","0","cmd-96","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","240,","告警,"]
["69","4.19.40.1","UL33_1_LinkStatus","UPS* 通讯状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","断线告警,"]