{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":13,"n_cols":76,"rows_kept":13,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.15.30.1","ups1_OutputVol","UPS* 输出电压","5","4","0","1","0","cmd-3","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["2","4.15.30.1","ups1_InputFreq","UPS* 输入频率","5","4","0","1","0","cmd-5","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["3","4.15.30.1","ups1_BatteryVol","UPS* 电池电压","5","4","0","1","0","cmd-6","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["4","4.15.30.1","ups1_EnvTemp","UPS* 环境温度","5","4","0","1","0","cmd-7","type-1","0","60","720","1",null,null,"0","0","0","0","5","35","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"20","0","100","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0","0"]
["5","4.15.30.1","ups1_InputVolFault","UPS* 市电电压异常","1","1","0","1","0","cmd-8","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","告警,"]
["6","4.15.30.1","ups1_BatteryLowVol","UPS* 电池低电压","1","1","0","1","0","cmd-9","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","告警,"]
["7","4.15.30.1","ups1_ByPass","UPS* 旁路","1","1","0","1","0","cmd-10","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","告警,"]
["8","4.15.30.1","ups1_Fault","UPS* 故障","1","1","0","1","0","cmd-11","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","告警,"]
["9","4.15.30.1","ups1_Buzzer","UPS* 蜂鸣器","1","1","0","1","0","cmd-13","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","告警,"]
["10","4.15.30.1","ups1_A_PhaseInputVol","UPS* 输入电压","5","4","0","1","0","cmd-1","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["11","4.15.30.1","ups1_Load","UPS* 负载","5","4","0","1","0","cmd-4","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0"]
["12","4.15.30.1","ups1_ComStatus","UPS* 串口通信状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","30",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线告警,"]