{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":20,"n_cols":76,"rows_kept":20,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.15.31.1","UPS_1_InputVolA","UPS* A相输入电压","1","0","0","1","0","cmd-1","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.15.31.1","UPS_1_InputVolB","UPS* B相输入电压","1","0","0","1","0","cmd-2","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.15.31.1","UPS_1_InputVolC","UPS* C相输入电压","1","0","0","1","0","cmd-3","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.15.31.1","UPS_1_OutputVolA","UPS* A相输出电压","1","0","0","1","0","cmd-4","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.15.31.1","UPS_1_OutputVolB","UPS* B相输出电压","1","0","0","1","0","cmd-5","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.15.31.1","UPS_1_OutputVolC","UPS* C相输出电压","1","0","0","1","0","cmd-6","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","500","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.15.31.1","UPS_1_LoadA","UPS* A相负载","1","0","0","1","0","cmd-7","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.15.31.1","UPS_1_LoadB","UPS* B相负载","1","0","0","1","0","cmd-8","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.15.31.1","UPS_1_LoadC","UPS* C相负载","1","0","0","1","0","cmd-9","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","%","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.15.31.1","UPS_1_Temp","UPS* 温度","1","0","0","1","0","cmd-10","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","℃","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.15.31.1","UPS_1_Freq","UPS* 频率","1","0","0","1","0","cmd-11","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.15.31.1","UPS_1_BatteryVol","UPS* 电池电压","1","0","0","1","0","cmd-12","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","V","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.15.31.1","UPS_1_RemainTime","UPS* 电池剩余UPS* 时间","1","0","0","1","0","cmd-13","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0","Min","900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.15.31.1","UPS_1_Status","UPS* 状态","1","0","0","1","0","cmd-14","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.15.31.1","UPS_1_Rectifier","UPS* 逆变器","1","0","0","1","0","cmd-15","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.15.31.1","UPS_1_PowerSupply","UPS* 供电方式","1","0","0","1","0","cmd-16","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.15.31.1","UPS_1_BatteryStatus","UPS* 电池状态","1","0","0","1","0","cmd-17","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.15.31.1","UPS_1_ChargeStatus","UPS* 充电状态","1","0","0","1","0","cmd-18","type-1","0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","5","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.15.31.1","UPS_1_NetStatus","UPS* 通信状态","1000","0","0","1","0",null,null,"0","60","720","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","31",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]