{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":86,"n_cols":76,"rows_kept":86,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.37.1","uha3r_1_IPVoltA","1号UPS A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.37.1","uha3r_1_IPVoltB","1号UPS B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.37.1","uha3r_1_IPVoltC","1号UPS C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.37.1","uha3r_1_OPVoltA","1号UPS A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.37.1","uha3r_1_OPVoltB","1号UPS B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.37.1","uha3r_1_OPVoltC","1号UPS C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.37.1","uha3r_1_OPCurA","1号UPS A相输出电流","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.37.1","uha3r_1_OPCurB","1号UPS B相输出电流","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.37.1","uha3r_1_OPCurC","1号UPS C相输出电流","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.37.1","uha3r_1_DCIPVoltB1","1号UPS 直流输入电压(电池组1)","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.37.1","uha3r_1_OPFrequency","1号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.37.1","uha3r_1_DCIPVoltB2","1号UPS 直流输入电压(电池组2)","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.37.1","uha3r_1_ACILVoltAB","1号UPS 交流输入线电压AB","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.37.1","uha3r_1_ACILVoltBC","1号UPS 交流输入线电压BC","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.37.1","uha3r_1_ACILVoltCA","1号UPS 交流输入线电压CA","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.37.1","uha3r_1_IPCurA","1号UPS A相输入电流","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.37.1","uha3r_1_IPCurB","1号UPS B相输入电流","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.37.1","uha3r_1_IPCurC","1号UPS C相输入电流","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.37.1","uha3r_1_IPFrequency","1号UPS 输入频率","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.37.1","uha3r_1_BPVoltA","1号UPS A相旁路电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.37.1","uha3r_1_BPVoltB","1号UPS B相旁路电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.37.1","uha3r_1_BPVoltC","1号UPS C相旁路电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.37.1","uha3r_1_BPFrequency","1号UPS 旁路频率","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.37.1","uha3r_1_OPPowerA","1号UPS A相输出有功功率","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.37.1","uha3r_1_OPPowerB","1号UPS B相输出有功功率","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.37.1","uha3r_1_OPPowerC","1号UPS C相输出有功功率","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.37.1","uha3r_1_OPPowerAP","1号UPS A相输出负载百分比","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.37.1","uha3r_1_OPPowerBP","1号UPS B相输出负载百分比","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.37.1","uha3r_1_OPPowerCP","1号UPS C相输出负载百分比","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.37.1","uha3r_1_PowerSupplyMode","1号UPS 供电方式","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["31","4.19.37.1","uha3r_1_PowerONOFF","1号UPS 整机开关状态","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","224,","关机,"]
["32","4.19.37.1","uha3r_1_MainPFailuer","1号UPS 主路电压异常","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","异常,"]
["33","4.19.37.1","uha3r_1_Rectifier","1号UPS 整流器状态","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["34","4.19.37.1","uha3r_1_Inverter","1号UPS 逆变器状态","1","0","0","1","0","cmd-99","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["35","4.19.37.1","uha3r_1_PassBy","1号UPS 旁路状态","1","0","0","1","0","cmd-100","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","超限,"]
["36","4.19.37.1","uha3r_1_Fans","1号UPS 风扇故障","1","0","0","1","0","cmd-114","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["37","4.19.37.1","uha3r_1_TempOver","1号UPS 环境温度过高","1","0","0","1","0","cmd-115","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","过温,"]
["38","4.19.37.1","uha3r_1_IMShutDown","1号UPS 紧急关机","1","0","0","1","0","cmd-116","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","紧急关机,"]
["39","4.19.37.1","uha3r_1_PassByShutdown","1号UPS 旁路异常关机","1","0","0","1","0","cmd-120","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","异常,"]
["40","4.19.37.1","uha3r_1_RectifierCommu","1号UPS 整流通讯故障","1","0","0","1","0","cmd-169","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["41","4.19.37.1","uha3r_1_InverterCommu","1号UPS 逆变通讯故障","1","0","0","1","0","cmd-170","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["1","4.19.37.1","uha3r_1_Communications","1号UPS 通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]
[]
["1","4.19.37.2","uha3r_2_IPVoltA","2号UPS A相输入电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.37.2","uha3r_2_IPVoltB","2号UPS B相输入电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.37.2","uha3r_2_IPVoltC","2号UPS C相输入电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.37.2","uha3r_2_OPVoltA","2号UPS A相输出电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.37.2","uha3r_2_OPVoltB","2号UPS B相输出电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.37.2","uha3r_2_OPVoltC","2号UPS C相输出电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.37.2","uha3r_2_OPCurA","2号UPS A相输出电流","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.37.2","uha3r_2_OPCurB","2号UPS B相输出电流","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.37.2","uha3r_2_OPCurC","2号UPS C相输出电流","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.37.2","uha3r_2_DCIPVoltB1","2号UPS 直流输入电压(电池组1)","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.37.2","uha3r_2_OPFrequency","2号UPS 输出频率","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.37.2","uha3r_2_DCIPVoltB2","2号UPS 直流输入电压(电池组2)","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.37.2","uha3r_2_ACILVoltAB","2号UPS 交流输入线电压AB","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.37.2","uha3r_2_ACILVoltBC","2号UPS 交流输入线电压BC","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.37.2","uha3r_2_ACILVoltCA","2号UPS 交流输入线电压CA","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.37.2","uha3r_2_IPCurA","2号UPS A相输入电流","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.37.2","uha3r_2_IPCurB","2号UPS B相输入电流","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.37.2","uha3r_2_IPCurC","2号UPS C相输入电流","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.37.2","uha3r_2_IPFrequency","2号UPS 输入频率","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.37.2","uha3r_2_BPVoltA","2号UPS A相旁路电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.37.2","uha3r_2_BPVoltB","2号UPS B相旁路电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.37.2","uha3r_2_BPVoltC","2号UPS C相旁路电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.37.2","uha3r_2_BPFrequency","2号UPS 旁路频率","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.37.2","uha3r_2_OPPowerA","2号UPS A相输出有功功率","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.37.2","uha3r_2_OPPowerB","2号UPS B相输出有功功率","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.37.2","uha3r_2_OPPowerC","2号UPS C相输出有功功率","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.37.2","uha3r_2_OPPowerAP","2号UPS A相输出负载百分比","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.37.2","uha3r_2_OPPowerBP","2号UPS B相输出负载百分比","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.37.2","uha3r_2_OPPowerCP","2号UPS C相输出负载百分比","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.37.2","uha3r_2_PowerSupplyMode","2号UPS 供电方式","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["31","4.19.37.2","uha3r_2_PowerONOFF","2号UPS 整机开关状态","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","224,","关机,"]
["32","4.19.37.2","uha3r_2_MainPFailuer","2号UPS 主路电压异常","1","0","0","1","0","cmd-97","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","异常,"]
["33","4.19.37.2","uha3r_2_Rectifier","2号UPS 整流器状态","1","0","0","1","0","cmd-98","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["34","4.19.37.2","uha3r_2_Inverter","2号UPS 逆变器状态","1","0","0","1","0","cmd-99","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["35","4.19.37.2","uha3r_2_PassBy","2号UPS 旁路状态","1","0","0","1","0","cmd-100","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","超限,"]
["36","4.19.37.2","uha3r_2_Fans","2号UPS 风扇故障","1","0","0","1","0","cmd-114","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["37","4.19.37.2","uha3r_2_TempOver","2号UPS 环境温度过高","1","0","0","1","0","cmd-115","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","过温,"]
["38","4.19.37.2","uha3r_2_IMShutDown","2号UPS 紧急关机","1","0","0","1","0","cmd-116","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","紧急关机,"]
["39","4.19.37.2","uha3r_2_PassByShutdown","2号UPS 旁路异常关机","1","0","0","1","0","cmd-120","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","异常,"]
["40","4.19.37.2","uha3r_2_RectifierCommu","2号UPS 整流通讯故障","1","0","0","1","0","cmd-169","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["41","4.19.37.2","uha3r_2_InverterCommu","2号UPS 逆变通讯故障","1","0","0","1","0","cmd-170","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","240,","故障,"]
["1","4.19.37.2","uha3r_2_Communications","2号UPS 通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","37",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]