{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":55,"n_cols":78,"rows_kept":55,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述","备注1","备注2"]
["1","4.14.26.1","EA800_1_BatteryVolt","电池电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","v","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.14.26.1","EA800_1_BatteryCapacity","电池容量","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.14.26.1","EA800_1_BatteryTime","电池剩余时间","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Min","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.14.26.1","EA800_1_BatteryCur","电池电流","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.14.26.1","EA800_1_BatteryTemp","电池温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.14.26.1","EA800_1_InputFrequency","输入频率","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.14.26.1","EA800_1_BypassFrequency","旁路频率","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.14.26.1","EA800_1_OutputFrequency","输出频率","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.14.26.1","EA800_1_RectifierRotationError","整流器回转错误","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["10","4.14.26.1","EA800_1_LowBatteryShutdonw","电池低关机","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["11","4.14.26.1","EA800_1_LowBattery","电池低","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["12","4.14.26.1","EA800_1_Threein","Three in","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["13","4.14.26.1","EA800_1_BackUpACNormal","备份/AC正常","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["14","4.14.26.1","EA800_1_Charge","充电","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["15","4.14.26.1","EA800_1_RectifierOperating","整流器工作","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["16","4.14.26.1","EA800_1_BypassFrequencyFail","旁路频率故障","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","报警描述"]
["17","4.14.26.1","EA800_1_ManualBypassBreaker","旁路开关","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["18","4.14.26.1","EA800_1_BypassAC","旁路直流","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["19","4.14.26.1","EA800_1_StaticSwitch","静态开关","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["20","4.14.26.1","EA800_1_InverterOperating","逆变器工作","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["21","4.14.26.1","EA800_1_EmergencyStop","紧急停止","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["22","4.14.26.1","EA800_1_HighDCShutdown","高直流关机","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["23","4.14.26.1","EA800_1_ManualBypassBreakerShutdown","旁路开关关机","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["24","4.14.26.1","EA800_1_OverLoadShutdown","过载关机","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["25","4.14.26.1","EA800_1_InverterOPFailShutdown","逆变输出故障关机","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["26","4.14.26.1","EA800_1_OverTemperatureShutdown","温度过高关机","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["27","4.14.26.1","EA800_1_ShortCircuitShutdown","短路关机","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["28","4.14.26.1","EA800_1_RIPVoltage","R相输入电压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","4.14.26.1","EA800_1_SIPVoltage","S相输入电压","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","4.14.26.1","EA800_1_TIPVoltage","T相输入电压","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","4.14.26.1","EA800_1_RBypassACVoltage","R相旁路交流电压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","4.14.26.1","EA800_1_SBypassACVoltage","S相旁路交流电压","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","4.14.26.1","EA800_1_TBypassACVoltage","T相旁路交流电压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","4.14.26.1","EA800_1_ROPValtage","R相输出电压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","4.14.26.1","EA800_1_SOPValtage","S相输出电压","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","4.14.26.1","EA800_1_TOPValtage","T相输出电压","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","4.14.26.1","EA800_1_RLoadPrecent","R相负载%","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","4.14.26.1","EA800_1_SLoadPrecent","S相负载%","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","4.14.26.1","EA800_1_TLoadPrecent","T相负载%","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","4.14.26.1","EA800_1_Ipvoltage","输入电压","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","4.14.26.1","EA800_1_IPFaultvoltage","故障输入电压","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","4.14.26.1","EA800_1_Opvoltage","输出电压","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["43","4.14.26.1","EA800_1_InputCurrent","输出电流","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["44","4.14.26.1","EA800_1_InputFrequency","输入频率","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["45","4.14.26.1","EA800_1_BatteryVoltage","电池电压","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["46","4.14.26.1","EA800_1_Temperature","温度","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["47","4.14.26.1","EA800_1_UtilityFail","市电故障","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["48","4.14.26.1","EA800_1_BatteryLow","电池低","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["49","4.14.26.1","EA800_1_BypassActive","旁路在线","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["50","4.14.26.1","EA800_1_UPSFailed","UPS故障","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["51","4.14.26.1","EA800_1_UPSOnline","UPS备机","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["52","4.14.26.1","EA800_1_UPSTest","UPS测试","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["53","4.14.26.1","EA800_1_ShutdownActive","UPS关机","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]
["54","4.14.26.1","EA800_1_BeeperOn","蜂鸣器开","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,","状态描述"]