{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":132,"n_cols":76,"rows_kept":132,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.40.1","UL33_1_AC_InputPhaseVoltageA","UPS主机交流输入相电压A","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.40.1","UL33_1_AC_InputPhaseVoltageB","UPS主机交流输入相电压B","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.40.1","UL33_1_AC_InputPhaseVoltageC","UPS主机交流输入相电压C","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.40.1","UL33_1_AC_OutputPhaseVoltageA","UPS主机交流输出相电压A","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.40.1","UL33_1_AC_OutputPhaseVoltageB","UPS主机交流输出相电压B","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.40.1","UL33_1_AC_OutputPhaseVoltageC","UPS主机交流输出相电压C","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.40.1","UL33_1_AC_OutputCurrentA","UPS主机交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.40.1","UL33_1_AC_OutputCurrentB","UPS主机交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.40.1","UL33_1_AC_OutputCurrentC","UPS主机交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.40.1","UL33_1_AC_BatteryVoltage","UPS主机电池电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.40.1","UL33_1_AC_OutputFrequency","UPS主机输出频率（三相一致）","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.40.1","UL33_1_AC_InputLineVoltageAB","UPS主机交流输入线电压AB","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.40.1","UL33_1_AC_InputLineVoltageBC","UPS主机交流输入线电压BC","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.40.1","UL33_1_AC_InputLineVoltageCA","UPS主机交流输入线电压CA","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.40.1","UL33_1_ACInputCurrentA","UPS主机A相输入电流","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.40.1","UL33_1_ACInputCurrentB","UPS主机B相输入电流","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.40.1","UL33_1_ACInputCurrentC","UPS主机C相输入电流","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.40.1","UL33_1_ACInputFrequency","UPS主机输入频率（三相一致）","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.40.1","UL33_1_ACAphaseBypassVoltage","UPS主机A相旁路电压","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.40.1","UL33_1_ACBphaseBypassVoltage","UPS主机B相旁路电压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.40.1","UL33_1_ACCphaseBypassVoltage","UPS主机C相旁路电压","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.40.1","UL33_1_ACAphaseBypassCurrent","UPS主机A相旁路电流","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.40.1","UL33_1_ACBphaseBypassCurrent","UPS主机B相旁路电流","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.40.1","UL33_1_ACCphaseBypassCurrent","UPS主机C相旁路电流","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.40.1","UL33_1_ACBypassFrequency","UPS主机旁路频率（三相一致）","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.40.1","UL33_1_ACBatteryTemperature","UPS主机电池温度","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.40.1","UL33_1_ACAphaseOutputActivePower","UPS主机A相输出有功功率","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.40.1","UL33_1_ACBphaseOutputActivePower","UPS主机B相输出有功功率","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.40.1","UL33_1_ACCphaseOutputActivePower","UPS主机C相输出有功功率","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.40.1","UL33_1_ACBatteryCurrent","UPS主机电池电流","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","4.19.40.1","UL33_1_ACRemainingBatteryBackupTime","UPS主机电池剩余后备时间","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","60000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","4.19.40.1","UL33_1_ACAphaseOutputApparentPower","UPS主机A相输出视在功率","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.19.40.1","UL33_1_ACBphaseOutputApparentPower","UPS主机B相输出视在功率","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","4.19.40.1","UL33_1_ACCphaseOutputApparentPower","UPS主机C相输出视在功率","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["35","4.19.40.1","UL33_1_ACAphaseOutputpercentage","UPS主机A相输出负载百分比","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","4.19.40.1","UL33_1_ACBphaseOutputpercentage","UPS主机B相输出负载百分比","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["37","4.19.40.1","UL33_1_ACCphaseOutputpercentage","UPS主机C相输出负载百分比","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["38","4.19.40.1","UL33_1_ACTemperature","UPS主机环境温度","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["39","4.19.40.1","UL33_1_ACPowerSupply","UPS主机供电方式","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["40","4.19.40.1","UL33_1_ACBatterySelfTest","UPS主机电池自检状态","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["41","4.19.40.1","UL33_1_ACAllChargeOrFloat","UPS主机均充/浮充（正组）","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["42","4.19.40.1","UL33_1_ACOffState","UPS主机开机/关机","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","228","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","229,","UPS关机,"]
["43","4.19.40.1","UL33_1_ACUPSPowerSupply","UPS主机UPS供电","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","232","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","231，233,","电池逆变供电,电池市电联合逆变供电,"]
["44","4.19.40.1","UL33_1_ACSynORasynchronous","UPS主机同步/不同步","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["45","4.19.40.1","UL33_1_ACMainsVoltage","UPS主机市电电压","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","2，3,","异常,欠压,"]
["46","4.19.40.1","UL33_1_ACRectifierStatus","UPS主机整流器状态","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["47","4.19.40.1","UL33_1_ACInverterStatus","UPS主机逆变器状态","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","249,","故障,"]
["48","4.19.40.1","UL33_1_ACBypassConditions","UPS主机旁路情况（电压或频率）","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","1,2,","超出跟踪范围,超出保护范围,"]
["49","4.19.40.1","UL33_1_ACTheTotalBatteryVoltageStatus","UPS主机蓄电池总电压状态","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","5","1,2,3,240,225,","无电池,低于下限,高于上限,接反,预告警,"]
["50","4.19.40.1","UL33_1_ACBatterySelfTestResults","UPS主机电池自检结果","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","需要更换电池,"]
["51","4.19.40.1","UL33_1_ACMainsFrequency","UPS主机市电频率","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["52","4.19.40.1","UL33_1_ACInverterFanFailure","UPS主机逆变风扇故障","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["53","4.19.40.1","UL33_1_ACRectifierFanFailure","UPS主机整流风扇故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["54","4.19.40.1","UL33_1_ACBatteryContactorFailure","UPS主机电池接触器故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["55","4.19.40.1","UL33_1_ACMainRoadContactorException","UPS主机主路接触器异常","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["56","4.19.40.1","UL33_1_ACOutputOverload","UPS主机本机输出过载","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","过载,"]
["57","4.19.40.1","UL33_1_ACAbnormalShutdownBypass","UPS主机旁路异常关机","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["58","4.19.40.1","UL33_1_AC_OutputOvervoltage","UPS主机交流输出过压","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["59","4.19.40.1","UL33_1_ACCurrentOutput","UPS主机输出冲击过流","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["60","4.19.40.1","UL33_1_ACOverCurrentInverter","UPS主机逆变模块过流","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["61","4.19.40.1","UL33_1_ACOverCurrentRectifier","UPS主机整流模块过流","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["62","4.19.40.1","UL33_1_ACBypassLoadImpact","UPS主机负载冲击转旁路","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["63","4.19.40.1","UL33_1_ACTemperatureHigh","UPS主机环境温度过高","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","2,","告警,"]
["64","4.19.40.1","UL33_1_ACRectifierCommunicationFailure","UPS主机整流通讯故障","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["65","4.19.40.1","UL33_1_ACInverterCommunicationFailure","UPS主机逆变通讯故障","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["66","4.19.40.1","UL33_2_AC_InputPhaseVoltageA","UPS从机交流输入相电压A","1","0","0","1","0","cmd-99","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["67","4.19.40.1","UL33_2_AC_InputPhaseVoltageB","UPS从机交流输入相电压B","1","0","0","1","0","cmd-100","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["68","4.19.40.1","UL33_2_AC_InputPhaseVoltageC","UPS从机交流输入相电压C","1","0","0","1","0","cmd-101","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["69","4.19.40.1","UL33_2_AC_OutputPhaseVoltageA","UPS从机交流输出相电压A","1","0","0","1","0","cmd-102","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["70","4.19.40.1","UL33_2_AC_OutputPhaseVoltageB","UPS从机交流输出相电压B","1","0","0","1","0","cmd-103","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["71","4.19.40.1","UL33_2_AC_OutputPhaseVoltageC","UPS从机交流输出相电压C","1","0","0","1","0","cmd-104","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["72","4.19.40.1","UL33_2_AC_OutputCurrentA","UPS从机交流输出电流A","1","0","0","1","0","cmd-105","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["73","4.19.40.1","UL33_2_AC_OutputCurrentB","UPS从机交流输出电流B","1","0","0","1","0","cmd-106","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["74","4.19.40.1","UL33_2_AC_OutputCurrentC","UPS从机交流输出电流C","1","0","0","1","0","cmd-107","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["75","4.19.40.1","UL33_2_AC_BatteryVoltage","UPS从机电池电压","1","0","0","1","0","cmd-108","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["76","4.19.40.1","UL33_2_AC_OutputFrequency","UPS从机输出频率（三相一致）","1","0","0","1","0","cmd-109","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["77","4.19.40.1","UL33_2_AC_InputLineVoltageAB","UPS从机交流输入线电压AB","1","0","0","1","0","cmd-110","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["78","4.19.40.1","UL33_2_AC_InputLineVoltageBC","UPS从机交流输入线电压BC","1","0","0","1","0","cmd-111","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","4.19.40.1","UL33_2_AC_InputLineVoltageCA","UPS从机交流输入线电压CA","1","0","0","1","0","cmd-112","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["80","4.19.40.1","UL33_2_ACInputCurrentA","UPS从机A相输入电流","1","0","0","1","0","cmd-113","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["81","4.19.40.1","UL33_2_ACInputCurrentB","UPS从机B相输入电流","1","0","0","1","0","cmd-114","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["82","4.19.40.1","UL33_2_ACInputCurrentC","UPS从机C相输入电流","1","0","0","1","0","cmd-115","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["83","4.19.40.1","UL33_2_ACInputFrequency","UPS从机输入频率（三相一致）","1","0","0","1","0","cmd-116","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["84","4.19.40.1","UL33_2_ACAphaseBypassVoltage","UPS从机A相旁路电压","1","0","0","1","0","cmd-117","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["85","4.19.40.1","UL33_2_ACBphaseBypassVoltage","UPS从机B相旁路电压","1","0","0","1","0","cmd-118","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["86","4.19.40.1","UL33_2_ACCphaseBypassVoltage","UPS从机C相旁路电压","1","0","0","1","0","cmd-119","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["87","4.19.40.1","UL33_2_ACAphaseBypassCurrent","UPS从机A相旁路电流","1","0","0","1","0","cmd-120","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["88","4.19.40.1","UL33_2_ACBphaseBypassCurrent","UPS从机B相旁路电流","1","0","0","1","0","cmd-121","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["89","4.19.40.1","UL33_2_ACCphaseBypassCurrent","UPS从机C相旁路电流","1","0","0","1","0","cmd-122","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["90","4.19.40.1","UL33_2_ACBypassFrequency","UPS从机旁路频率（三相一致）","1","0","0","1","0","cmd-123","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["91","4.19.40.1","UL33_2_ACBatteryTemperature","UPS从机电池温度","1","0","0","1","0","cmd-124","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["92","4.19.40.1","UL33_2_ACAphaseOutputActivePower","UPS从机A相输出有功功率","1","0","0","1","0","cmd-125","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["93","4.19.40.1","UL33_2_ACBphaseOutputActivePower","UPS从机B相输出有功功率","1","0","0","1","0","cmd-126","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["94","4.19.40.1","UL33_2_ACCphaseOutputActivePower","UPS从机C相输出有功功率","1","0","0","1","0","cmd-127","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["95","4.19.40.1","UL33_2_ACBatteryCurrent","UPS从机电池电流","1","0","0","1","0","cmd-128","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["96","4.19.40.1","UL33_2_ACRemainingBatteryBackupTime","UPS从机电池剩余后备时间","1","0","0","1","0","cmd-129","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","60000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["97","4.19.40.1","UL33_2_ACAphaseOutputApparentPower","UPS从机A相输出视在功率","1","0","0","1","0","cmd-130","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["98","4.19.40.1","UL33_2_ACBphaseOutputApparentPower","UPS从机B相输出视在功率","1","0","0","1","0","cmd-131","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["99","4.19.40.1","UL33_2_ACCphaseOutputApparentPower","UPS从机C相输出视在功率","1","0","0","1","0","cmd-132","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["100","4.19.40.1","UL33_2_ACAphaseOutputpercentage","UPS从机A相输出负载百分比","1","0","0","1","0","cmd-133","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["101","4.19.40.1","UL33_2_ACBphaseOutputpercentage","UPS从机B相输出负载百分比","1","0","0","1","0","cmd-134","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["102","4.19.40.1","UL33_2_ACCphaseOutputpercentage","UPS从机C相输出负载百分比","1","0","0","1","0","cmd-135","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["103","4.19.40.1","UL33_2_ACTemperature","UPS从机环境温度","1","0","0","1","0","cmd-136","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["104","4.19.40.1","UL33_2_ACPowerSupply","UPS从机供电方式","1","0","0","1","0","cmd-140","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["105","4.19.40.1","UL33_2_ACBatterySelfTest","UPS从机电池自检状态","1","0","0","1","0","cmd-141","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["106","4.19.40.1","UL33_2_ACAllChargeOrFloat","UPS从机均充/浮充（正组）","1","0","0","1","0","cmd-142","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["107","4.19.40.1","UL33_2_ACOffState","UPS从机开机/关机","1","0","0","1","0","cmd-143","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","228","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","229,","UPS关机,"]
["108","4.19.40.1","UL33_2_ACUPSPowerSupply","UPS从机UPS供电","1","0","0","1","0","cmd-144","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","232","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","231，233,","电池逆变供电,电池市电联合逆变供电,"]
["109","4.19.40.1","UL33_2_ACSynORasynchronous","UPS从机同步/不同步","1","0","0","1","0","cmd-151","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["110","4.19.40.1","UL33_2_ACMainsVoltage","UPS从机市电电压","1","0","0","1","0","cmd-152","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","2，3,","异常,欠压,"]
["111","4.19.40.1","UL33_2_ACRectifierStatus","UPS从机整流器状态","1","0","0","1","0","cmd-153","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["112","4.19.40.1","UL33_2_ACInverterStatus","UPS从机逆变器状态","1","0","0","1","0","cmd-154","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","249,","故障,"]
["113","4.19.40.1","UL33_2_ACBypassConditions","UPS从机旁路情况（电压或频率）","1","0","0","1","0","cmd-155","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","1,2,","超出跟踪范围,超出保护范围,"]
["114","4.19.40.1","UL33_2_ACTheTotalBatteryVoltageStatus","UPS从机蓄电池总电压状态","1","0","0","1","0","cmd-156","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","5","1,2,3,240,225,","无电池,低于下限,高于上限,接反,预告警,"]
["115","4.19.40.1","UL33_2_ACBatterySelfTestResults","UPS从机电池自检结果","1","0","0","1","0","cmd-157","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","需要更换电池,"]
["116","4.19.40.1","UL33_2_ACMainsFrequency","UPS从机市电频率","1","0","0","1","0","cmd-158","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["117","4.19.40.1","UL33_2_ACInverterFanFailure","UPS从机逆变风扇故障","1","0","0","1","0","cmd-166","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["118","4.19.40.1","UL33_2_ACRectifierFanFailure","UPS从机整流风扇故障","1","0","0","1","0","cmd-167","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["119","4.19.40.1","UL33_2_ACBatteryContactorFailure","UPS从机电池接触器故障","1","0","0","1","0","cmd-168","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["120","4.19.40.1","UL33_2_ACMainRoadContactorException","UPS从机主路接触器异常","1","0","0","1","0","cmd-169","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["121","4.19.40.1","UL33_2_ACOutputOverload","UPS从机本机输出过载","1","0","0","1","0","cmd-173","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","过载,"]
["122","4.19.40.1","UL33_2_ACAbnormalShutdownBypass","UPS从机旁路异常关机","1","0","0","1","0","cmd-179","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["123","4.19.40.1","UL33_2_AC_OutputOvervoltage","UPS从机交流输出过压","1","0","0","1","0","cmd-183","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["124","4.19.40.1","UL33_2_ACCurrentOutput","UPS从机输出冲击过流","1","0","0","1","0","cmd-184","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["125","4.19.40.1","UL33_2_ACOverCurrentInverter","UPS从机逆变模块过流","1","0","0","1","0","cmd-185","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["126","4.19.40.1","UL33_2_ACOverCurrentRectifier","UPS从机整流模块过流","1","0","0","1","0","cmd-186","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["127","4.19.40.1","UL33_2_ACBypassLoadImpact","UPS从机负载冲击转旁路","1","0","0","1","0","cmd-187","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["128","4.19.40.1","UL33_2_ACTemperatureHigh","UPS从机环境温度过高","1","0","0","1","0","cmd-192","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","2,","告警,"]
["129","4.19.40.1","UL33_2_ACRectifierCommunicationFailure","UPS从机整流通讯故障","1","0","0","1","0","cmd-193","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["130","4.19.40.1","UL33_2_ACInverterCommunicationFailure","UPS从机逆变通讯故障","1","0","0","1","0","cmd-194","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","256","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["131","4.19.40.1","UL33_1_LinkStatus","通讯状态","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","断线告警,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":137,"n_cols":76,"rows_kept":137,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.19.40.1","UL33_1_AC_InputPhaseVoltageA","交流输入相电压A","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","4.19.40.1","UL33_1_AC_InputPhaseVoltageB","交流输入相电压B","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","4.19.40.1","UL33_1_AC_InputPhaseVoltageC","交流输入相电压C","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","4.19.40.1","UL33_1_AC_OutputPhaseVoltageA","交流输出相电压A","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","4.19.40.1","UL33_1_AC_OutputPhaseVoltageB","交流输出相电压B","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","4.19.40.1","UL33_1_AC_OutputPhaseVoltageC","交流输出相电压C","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","4.19.40.1","UL33_1_AC_OutputCurrentA","交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","4.19.40.1","UL33_1_AC_OutputCurrentB","交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","4.19.40.1","UL33_1_AC_OutputCurrentC","交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","4.19.40.1","UL33_1_AC_BatteryVoltage","电池电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","4.19.40.1","UL33_1_AC_OutputFrequency","输出频率（三相一致）","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","4.19.40.1","UL33_1_AC_InputLineVoltageAB","交流输入线电压AB","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","4.19.40.1","UL33_1_AC_InputLineVoltageBC","交流输入线电压BC","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","4.19.40.1","UL33_1_AC_InputLineVoltageCA","交流输入线电压CA","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","4.19.40.1","UL33_1_ACInputCurrentA","A相输入电流","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","4.19.40.1","UL33_1_ACInputCurrentB","B相输入电流","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","4.19.40.1","UL33_1_ACInputCurrentC","C相输入电流","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","4.19.40.1","UL33_1_ACInputFrequency","输入频率（三相一致）","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","4.19.40.1","UL33_1_ACAphaseBypassVoltage","A相旁路电压","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","4.19.40.1","UL33_1_ACBphaseBypassVoltage","B相旁路电压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","4.19.40.1","UL33_1_ACCphaseBypassVoltage","C相旁路电压","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","4.19.40.1","UL33_1_ACAphaseBypassCurrent","A相旁路电流","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","4.19.40.1","UL33_1_ACBphaseBypassCurrent","B相旁路电流","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","4.19.40.1","UL33_1_ACCphaseBypassCurrent","C相旁路电流","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["25","4.19.40.1","UL33_1_ACBypassFrequency","旁路频率（三相一致）","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["26","4.19.40.1","UL33_1_ACBatteryTemperature","电池温度","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["27","4.19.40.1","UL33_1_ACAphaseOutputActivePower","A相输出有功功率","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["28","4.19.40.1","UL33_1_ACBphaseOutputActivePower","B相输出有功功率","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["29","4.19.40.1","UL33_1_ACCphaseOutputActivePower","C相输出有功功率","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["30","4.19.40.1","UL33_1_ACBatteryCurrent","电池电流","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["31","4.19.40.1","UL33_1_ACRemainingBatteryBackupTime","电池剩余后备时间","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["32","4.19.40.1","UL33_1_ACAphaseOutputApparentPower","A相输出视在功率","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","4.19.40.1","UL33_1_ACBphaseOutputApparentPower","B相输出视在功率","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["34","4.19.40.1","UL33_1_ACCphaseOutputApparentPower","C相输出视在功率","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["35","4.19.40.1","UL33_1_ACAphaseOutputpercentage","A相输出负载百分比","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","4.19.40.1","UL33_1_ACBphaseOutputpercentage","B相输出负载百分比","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["37","4.19.40.1","UL33_1_ACCphaseOutputpercentage","C相输出负载百分比","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["38","4.19.40.1","UL33_1_ACTemperature","环境温度","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["39","4.19.40.1","UL33_1_ACAphaseOutputPeakRatio","A相输出峰值比","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["40","4.19.40.1","UL33_1_ACBphaseOutputPeakRatio","B相输出峰值比","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["41","4.19.40.1","UL33_1_ACCphaseOutputPeakRatio","C相输出峰值比","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["42","4.19.40.1","UL33_1_ACPowerSupply","供电方式","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["43","4.19.40.1","UL33_1_ACBatterySelfTest","电池自检状态","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["44","4.19.40.1","UL33_1_ACAllChargeOrFloat","均充/浮充（正组）","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["45","4.19.40.1","UL33_1_ACOffState","开机/关机","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","228","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","229,","UPS关机,"]
["46","4.19.40.1","UL33_1_ACUPSPowerSupply","UPS供电","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","232","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","231，233,","电池逆变供电,电池市电联合逆变供电,"]
["47","4.19.40.1","UL33_1_ACSynORasynchronous","同步/不同步","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["48","4.19.40.1","UL33_1_ACMainsVoltage","市电电压","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","2，3,","异常,欠压,"]
["49","4.19.40.1","UL33_1_ACRectifierStatus","整流器状态","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["50","4.19.40.1","UL33_1_ACInverterStatus","逆变器状态","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","249,","故障,"]
["51","4.19.40.1","UL33_1_ACBypassConditions","旁路情况（电压或频率）","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","1,2,","超出跟踪范围,超出保护范围,"]
["52","4.19.40.1","UL33_1_ACTheTotalBatteryVoltageStatus","蓄电池总电压状态","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","5","1,2,3,240,225,","无电池,低于下限,高于上限,接反,预告警,"]
["53","4.19.40.1","UL33_1_ACBatterySelfTestResults","电池自检结果","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","需要更换电池,"]
["54","4.19.40.1","UL33_1_ACMainsFrequency","市电频率","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["55","4.19.40.1","UL33_1_ACInverterFanFailure","逆变风扇故障","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["56","4.19.40.1","UL33_1_ACRectifierFanFailure","整流风扇故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["57","4.19.40.1","UL33_1_ACBatteryContactorFailure","电池接触器故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["58","4.19.40.1","UL33_1_ACMainRoadContactorException","主路接触器异常","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["59","4.19.40.1","UL33_1_ACOutputOverload","本机输出过载","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","过载,"]
["60","4.19.40.1","UL33_1_ACAbnormalShutdownBypass","旁路异常关机","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["61","4.19.40.1","UL33_1_AC_OutputOvervoltage","交流输出过压","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["62","4.19.40.1","UL33_1_ACCurrentOutput","输出冲击过流","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["63","4.19.40.1","UL33_1_ACOverCurrentInverter","逆变模块过流","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["64","4.19.40.1","UL33_1_ACOverCurrentRectifier","整流模块过流","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["65","4.19.40.1","UL33_1_ACBypassLoadImpact","负载冲击转旁路","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["66","4.19.40.1","UL33_1_ACTemperatureHigh","环境温度过高","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","2,","告警,"]
["67","4.19.40.1","UL33_1_ACRectifierCommunicationFailure","整流通讯故障","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["68","4.19.40.1","UL33_1_ACInverterCommunicationFailure","逆变通讯故障","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["69","4.19.40.2","UL33_2_AC_InputPhaseVoltageA","交流输入相电压A","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["70","4.19.40.2","UL33_2_AC_InputPhaseVoltageB","交流输入相电压B","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["71","4.19.40.2","UL33_2_AC_InputPhaseVoltageC","交流输入相电压C","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["72","4.19.40.2","UL33_2_AC_OutputPhaseVoltageA","交流输出相电压A","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["73","4.19.40.2","UL33_2_AC_OutputPhaseVoltageB","交流输出相电压B","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["74","4.19.40.2","UL33_2_AC_OutputPhaseVoltageC","交流输出相电压C","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["75","4.19.40.2","UL33_2_AC_OutputCurrentA","交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["76","4.19.40.2","UL33_2_AC_OutputCurrentB","交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["77","4.19.40.2","UL33_2_AC_OutputCurrentC","交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["78","4.19.40.2","UL33_2_BatteryVoltage","电池电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","4.19.40.2","UL33_2_OutputFrequency","输出频率（三相一致）","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["80","4.19.40.2","UL33_2_AC_InputLineVoltageAB","交流输入线电压AB","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["81","4.19.40.2","UL33_2_AC_InputLineVoltageBC","交流输入线电压BC","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["82","4.19.40.2","UL33_2_AC_InputLineVoltageCA","交流输入线电压CA","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["83","4.19.40.2","UL33_2_InputCurrentA","A相输入电流","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["84","4.19.40.2","UL33_2_InputCurrentB","B相输入电流","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["85","4.19.40.2","UL33_2_InputCurrentC","C相输入电流","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["86","4.19.40.2","UL33_2_InputFrequency","输入频率（三相一致）","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["87","4.19.40.2","UL33_2_AphaseBypassVoltage","A相旁路电压","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["88","4.19.40.2","UL33_2_BphaseBypassVoltage","B相旁路电压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["89","4.19.40.2","UL33_2_CphaseBypassVoltage","C相旁路电压","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["90","4.19.40.2","UL33_2_AphaseBypassCurrent","A相旁路电流","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["91","4.19.40.2","UL33_2_BphaseBypassCurrent","B相旁路电流","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["92","4.19.40.2","UL33_2_CphaseBypassCurrent","C相旁路电流","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["93","4.19.40.2","UL33_2_BypassFrequency","旁路频率（三相一致）","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["94","4.19.40.2","UL33_2_BatteryTemperature","电池温度","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["95","4.19.40.2","UL33_2_AphaseOutputActivePower","A相输出有功功率","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["96","4.19.40.2","UL33_2_BphaseOutputActivePower","B相输出有功功率","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["97","4.19.40.2","UL33_2_CphaseOutputActivePower","C相输出有功功率","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["98","4.19.40.2","UL33_2_BatteryCurrent","电池电流","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["99","4.19.40.2","UL33_2_RemainingBatteryBackupTime","电池剩余后备时间","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["100","4.19.40.2","UL33_2_AphaseOutputApparentPower","A相输出视在功率","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["101","4.19.40.2","UL33_2_BphaseOutputApparentPower","B相输出视在功率","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["102","4.19.40.2","UL33_2_CphaseOutputApparentPower","C相输出视在功率","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["103","4.19.40.2","UL33_2_AphaseOutputpercentage","A相输出负载百分比","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["104","4.19.40.2","UL33_2_BphaseOutputpercentage","B相输出负载百分比","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["105","4.19.40.2","UL33_2_CphaseOutputpercentage","C相输出负载百分比","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["106","4.19.40.2","UL33_2_Temperature","环境温度","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["107","4.19.40.2","UL33_2_AphaseOutputPeakRatio","A相输出峰值比","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["108","4.19.40.2","UL33_2_BphaseOutputPeakRatio","B相输出峰值比","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["109","4.19.40.2","UL33_2_CphaseOutputPeakRatio","C相输出峰值比","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["110","4.19.40.2","UL33_2_PowerSupply","供电方式","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["111","4.19.40.2","UL33_2_BatterySelfTest","电池自检状态","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["112","4.19.40.2","UL33_2_AllChargeOrFloat","均充/浮充（正组）","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["113","4.19.40.2","UL33_2_OffState","开机/关机","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","228","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","229,","UPS关机,"]
["114","4.19.40.2","UL33_2_UPSPowerSupply","UPS供电","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","232","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","231，233,","电池逆变供电,电池市电联合逆变供电,"]
["115","4.19.40.2","UL33_2_SynORasynchronous","同步/不同步","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["116","4.19.40.2","UL33_2_MainsVoltage","市电电压","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","2，3,","异常,欠压,"]
["117","4.19.40.2","UL33_2_RectifierStatus","整流器状态","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["118","4.19.40.2","UL33_2_InverterStatus","逆变器状态","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","249,","故障,"]
["119","4.19.40.2","UL33_2_BypassConditions","旁路情况（电压或频率）","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","1,2,","超出跟踪范围,超出保护范围,"]
["120","4.19.40.2","UL33_2_TheTotalBatteryVoltageStatus","蓄电池总电压状态","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","5","1,2,3,240,225,","无电池,低于下限,高于上限,接反,预告警,"]
["121","4.19.40.2","UL33_2_BatterySelfTestResults","电池自检结果","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","需要更换电池,"]
["122","4.19.40.2","UL33_2_MainsFrequency","市电频率","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["123","4.19.40.2","UL33_2_InverterFanFailure","逆变风扇故障","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["124","4.19.40.2","UL33_2_RectifierFanFailure","整流风扇故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["125","4.19.40.2","UL33_2_BatteryContactorFailure","电池接触器故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["126","4.19.40.2","UL33_2_MainRoadContactorException","主路接触器异常","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["127","4.19.40.2","UL33_2_OutputOverload","本机输出过载","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","过载,"]
["128","4.19.40.2","UL33_2_AbnormalShutdownBypass","旁路异常关机","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["129","4.19.40.2","UL33_2_AC_OutputOvervoltage","交流输出过压","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["130","4.19.40.2","UL33_2_CurrentOutput","输出冲击过流","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["131","4.19.40.2","UL33_2_OverCurrentInverter","逆变模块过流","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["132","4.19.40.2","UL33_2_OverCurrentRectifier","整流模块过流","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["133","4.19.40.2","UL33_2_BypassLoadImpact","负载冲击转旁路","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["134","4.19.40.2","UL33_2_TemperatureHigh","环境温度过高","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","2,","告警,"]
["135","4.19.40.2","UL33_2_RectifierCommunicationFailure","整流通讯故障","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["136","4.19.40.2","UL33_2_InverterCommunicationFailure","逆变通讯故障","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]