{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":29,"n_cols":76,"rows_kept":29,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","6.1.65.1","Canatal13_1_V1","1号空调 制冷状态(理论上)","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V2","1号空调 去湿状态(理论上)","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V3","1号空调 风机状态(理论上)","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V4","1号空调 加热状态(理论上)","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V5","1号空调 加湿状态(理论上)","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V6","1号空调 压缩机状态(实际)","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V7","1号空调 风机状态(实际)","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V8","1号空调 加热器状态(实际)","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V9","1号空调 加湿器状态(实际)","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V10","1号空调 机组工作状态","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V11","1号空调 温度高报警","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V12","1号空调 温度低报警","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V13","1号空调 湿度高报警","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V14","1号空调 湿度低报警","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V15","1号空调 相位错报警","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V16","1号空调 加湿器淤塞报警","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V17","1号空调 火警","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V18","1号空调 溢水报警","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V19","1号空调 加热器淤塞报警","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V20","1号空调 压缩机低压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V21","1号空调 压缩机高压","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V22","1号空调 风机过载","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V23","1号空调 机组单联机状态","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V24","1号空调 机组开关机状态","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V25","1号空调 当前温度值","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","100","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V26","1号空调 当前湿度值","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","100","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V27","1号空调 开关机操作","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","100","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_Comus","1号空调通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":29,"n_cols":76,"rows_kept":29,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","6.1.65.1","Canatal13_1_V1","1号空调 制冷状态(理论上)","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V2","1号空调 去湿状态(理论上)","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V3","1号空调 风机状态(理论上)","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V4","1号空调 加热状态(理论上)","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V5","1号空调 加湿状态(理论上)","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V6","1号空调 压缩机状态(实际)","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V7","1号空调 风机状态(实际)","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V8","1号空调 加热器状态(实际)","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V9","1号空调 加湿器状态(实际)","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V10","1号空调 机组工作状态","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V11","1号空调 温度高报警","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V12","1号空调 温度低报警","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V13","1号空调 湿度高报警","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V14","1号空调 湿度低报警","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V15","1号空调 相位错报警","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V16","1号空调 加湿器淤塞报警","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V17","1号空调 火警","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V18","1号空调 溢水报警","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V19","1号空调 加热器淤塞报警","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V20","1号空调 压缩机低压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V21","1号空调 压缩机高压","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V22","1号空调 风机过载","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V23","1号空调 机组单联机状态","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V24","1号空调 机组开关机状态","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V25","1号空调 当前温度值","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","100","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V26","1号空调 当前湿度值","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","100","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_V27","1号空调 开关机操作","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"30","1","100","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0"]
["1","6.1.65.1","Canatal13_1_Comus","1号空调通信状态","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","65",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]