{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":60,"n_cols":76,"rows_kept":60,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","6.8.96.1","ACRD101_1_GroupCoolOutput","1号空调制冷输出功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.1.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","6.8.96.1","ACRD101_1_GroupCoolDemand","1号空调制冷需求功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.2.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","6.8.96.1","ACRD101_1_GroupAirFlowMetric","1号空调空气流量","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.4.0","public","0","0","0","0","0","0","0","0","0","L/S","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","6.8.96.1","ACRD101_1_MaxRackInletTempMetric","1号空调机架最大入口温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.6.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","6.8.96.1","ACRD101_1_MinRackInletTempMetric","1号空调机架最小入口温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.8.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","6.8.96.1","ACRD101_1_MaxReturnAirTempMetric","1号空调最大回风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.10.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","6.8.96.1","ACRD101_1_MinReturnAirTempMetric","1号空调最小回风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.12.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","6.8.96.1","ACRD101_1_CoolSetpointMetric","1号空调制冷温度设定点","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.2.2.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","6.8.96.1","ACRD101_1_SupplyAirSetpointMetric","1号空调送风温度设定点","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.2.7.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","6.8.96.1","ACRD101_1_OperateMode","1号空调操作模式","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.1.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","4","1,3,4,5,","备份,空闲,保留,服务,"]
["10","6.8.96.1","ACRD101_1_Compressor","1号空调压缩机状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.27.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","关,"]
["11","6.8.96.1","ACRD101_1_UnitCoolOutput","1号空调制冷输出功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.2.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","6.8.96.1","ACRD101_1_UnitCoolDemand","1号空调制冷需求功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.3.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","6.8.96.1","ACRD101_1_RackInletTempMetric","1号空调机架入口温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.7.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","6.8.96.1","ACRD101_1_SupplyAirTempMetric","1号空调送风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.9.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","6.8.96.1","ACRD101_1_ReturnAirTempMetric","1号空调回风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.11.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","6.8.96.1","ACRD101_1_SuctionTempMetric","1号空调吸气温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.13.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","6.8.96.1","ACRD101_1_UnitAirFlowMetric","1号空调空气流量","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.5.0","public","0","0","0","0","0","0","0","0","0","L/S","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","6.8.96.1","ACRD101_1_EvaporatorFanSpeed","1号空调风扇速度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.22.0","public","0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["19","6.8.96.1","ACRD101_1_HotGasBypassValvePos","1号空调旁路热气阀门位置","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.29.0","public","0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["20","6.8.96.1","ACRD101_1_InputState","1号空调输入状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.23.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["21","6.8.96.1","ACRD101_1_OutputState","1号空调输出状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.24.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["22","6.8.96.1","ACRD101_1_OHEInputState","1号空调OHE 输入状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.25.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["23","6.8.96.1","ACRD101_1_OHEOutputState","1号空调OHE 输出状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.26.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["24","6.8.96.1","ACRD101_1_FilterDPMetric","1号空调过滤器压差","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.17.0","public","0","0","0","0","0","0","0","0","0","pa","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["25","6.8.96.1","ACRD101_1_SuctionPressureMetric","1号空调吸气压力","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.19.0","public","0","0","0","0","0","0","0","0","0","Kpa","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["26","6.8.96.1","ACRD101_1_DischargePressureMetric","1号空调放气压力","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.21.0","public","0","0","0","0","0","0","0","0","0","Kpa","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["27","6.8.96.1","ACRD101_1_SuperheatTempMetric","1号空调过热温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.15.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["1","6.8.96.1","ACRD101_1_Communications","1号空调通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]
[]
["1","6.8.96.2","ACRD101_2_GroupCoolOutput","2号空调制冷输出功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.1.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","6.8.96.2","ACRD101_2_GroupCoolDemand","2号空调制冷需求功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.2.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","6.8.96.2","ACRD101_2_GroupAirFlowMetric","2号空调空气流量","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.4.0","public","0","0","0","0","0","0","0","0","0","L/S","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","6.8.96.2","ACRD101_2_MaxRackInletTempMetric","2号空调机架最大入口温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.6.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","6.8.96.2","ACRD101_2_MinRackInletTempMetric","2号空调机架最小入口温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.8.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","6.8.96.2","ACRD101_2_MaxReturnAirTempMetric","2号空调最大回风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.10.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","6.8.96.2","ACRD101_2_MinReturnAirTempMetric","2号空调最小回风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.1.12.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","6.8.96.2","ACRD101_2_CoolSetpointMetric","2号空调制冷温度设定点","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.2.2.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","6.8.96.2","ACRD101_2_SupplyAirSetpointMetric","2号空调送风温度设定点","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.2.2.7.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","6.8.96.2","ACRD101_2_OperateMode","2号空调操作模式","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.1.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","4","1,3,4,5,","备份,空闲,保留,服务,"]
["10","6.8.96.2","ACRD101_2_Compressor","2号空调压缩机状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.27.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","10","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","关,"]
["11","6.8.96.2","ACRD101_2_UnitCoolOutput","2号空调制冷输出功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.2.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","6.8.96.2","ACRD101_2_UnitCoolDemand","2号空调制冷需求功率","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.3.0","public","0","0","0","0","0","0","0","0","0","kw","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","6.8.96.2","ACRD101_2_RackInletTempMetric","2号空调机架入口温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.7.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","6.8.96.2","ACRD101_2_SupplyAirTempMetric","2号空调送风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.9.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","6.8.96.2","ACRD101_2_ReturnAirTempMetric","2号空调回风温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.11.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","6.8.96.2","ACRD101_2_SuctionTempMetric","2号空调吸气温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.13.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","6.8.96.2","ACRD101_2_UnitAirFlowMetric","2号空调空气流量","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.5.0","public","0","0","0","0","0","0","0","0","0","L/S","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","6.8.96.2","ACRD101_2_EvaporatorFanSpeed","2号空调风扇速度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.22.0","public","0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["19","6.8.96.2","ACRD101_2_HotGasBypassValvePos","2号空调旁路热气阀门位置","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.29.0","public","0","0","0","0","0","0","0","0","0","%","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["20","6.8.96.2","ACRD101_2_InputState","2号空调输入状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.23.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["21","6.8.96.2","ACRD101_2_OutputState","2号空调输出状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.24.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["22","6.8.96.2","ACRD101_2_OHEInputState","2号空调OHE 输入状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.25.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["23","6.8.96.2","ACRD101_2_OHEOutputState","2号空调OHE 输出状态","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.26.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","2,","关,"]
["24","6.8.96.2","ACRD101_2_FilterDPMetric","2号空调过滤器压差","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.17.0","public","0","0","0","0","0","0","0","0","0","pa","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["25","6.8.96.2","ACRD101_2_SuctionPressureMetric","2号空调吸气压力","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.19.0","public","0","0","0","0","0","0","0","0","0","Kpa","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["26","6.8.96.2","ACRD101_2_DischargePressureMetric","2号空调放气压力","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.21.0","public","0","0","0","0","0","0","0","0","0","Kpa","300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100000","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["27","6.8.96.2","ACRD101_2_SuperheatTempMetric","2号空调过热温度","4","2","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.318.1.1.13.4.5.2.1.15.0","public","0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0"]
["1","6.8.96.2","ACRD101_2_Communications","2号空调通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","107",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]