{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":19,"n_cols":41,"rows_kept":19,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值"]
["108","6.16.107.1","Pex1_ReturnAirTemp","力博1号空调_室内温度","4","2","1","4","30110",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["109","6.16.107.1","Pex1_ReturnAirTempSetPoint","力博1号空调_室内温度设定点","4","2","1","4","30111",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["110","6.16.107.1","Pex1_ReturnAirHumidity","力博1号空调_室内湿度","4","2","1","4","30130",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["111","6.16.107.1","Pex1_ReturnAirHumiditySetPoint","力博1号空调_室内湿度设定点","4","2","1","4","30131",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["112","6.16.107.1","Pex1_Fan","力博1号空调_风机","4","2","1","2","10025",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["113","6.16.107.1","Pex1_Cool","力博1号空调_制冷","4","2","1","2","10026",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["114","6.16.107.1","Pex1_Reheat","力博1号空调_电加热","4","2","1","2","10029",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["115","6.16.107.1","Pex1_ReHumidity","力博1号空调_加湿","4","2","1","2","10030",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["116","6.16.107.1","Pex1_DeReHumidity","力博1号空调_除湿","4","2","1","2","10031",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["117","6.16.107.2","Pex2_ReturnAirTemp","力博2号空调_室内温度","4","2","1","4","30110",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["118","6.16.107.2","Pex2_ReturnAirTempSetPoint","力博2号空调_室内温度设定点","4","2","1","4","30111",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["119","6.16.107.2","Pex2_ReturnAirHumidity","力博2号空调_室内湿度","4","2","1","4","30130",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["120","6.16.107.2","Pex2_ReturnAirHumiditySetPoint","力博2号空调_室内湿度设定点","4","2","1","4","30131",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["121","6.16.107.2","Pex2_Fan","力博2号空调_风机","4","2","1","2","10025",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["122","6.16.107.2","Pex2_Cool","力博2号空调_制冷","4","2","1","2","10026",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["123","6.16.107.2","Pex2_Reheat","力博2号空调_电加热","4","2","1","2","10029",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["124","6.16.107.2","Pex2_ReHumidity","力博2号空调_加湿","4","2","1","2","10030",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]
["125","6.16.107.2","Pex2_DeReHumidity","力博2号空调_除湿","4","2","1","2","10031",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0","3","0","1","0","0","0","0","0","107",null,null,"0"]