{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":137,"n_cols":76,"rows_kept":137,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["416","4.19.40.1","UL33_AC_InputPhaseVoltageA","1号交流输入相电压A","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["417","4.19.40.1","UL33_AC_InputPhaseVoltageB","1号交流输入相电压B","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["418","4.19.40.1","UL33_AC_InputPhaseVoltageC","1号交流输入相电压C","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["419","4.19.40.1","UL33_AC_OutputPhaseVoltageA","1号交流输出相电压A","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["420","4.19.40.1","UL33_AC_OutputPhaseVoltageB","1号交流输出相电压B","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["421","4.19.40.1","UL33_AC_OutputPhaseVoltageC","1号交流输出相电压C","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["422","4.19.40.1","UL33_AC_OutputCurrentA","1号交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["423","4.19.40.1","UL33_AC_OutputCurrentB","1号交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["424","4.19.40.1","UL33_AC_OutputCurrentC","1号交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["425","4.19.40.1","UL33_BatteryVoltage","1号电池电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["426","4.19.40.1","UL33_OutputFrequency","1号输出频率（三相一致）","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["427","4.19.40.1","UL33_AC_InputLineVoltageAB","1号交流输入线电压AB","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["428","4.19.40.1","UL33_AC_InputLineVoltageBC","1号交流输入线电压BC","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["429","4.19.40.1","UL33_AC_InputLineVoltageCA","1号交流输入线电压CA","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["430","4.19.40.1","UL33_InputCurrentA","1号A相输入电流","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["431","4.19.40.1","UL33_InputCurrentB","1号B相输入电流","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["432","4.19.40.1","UL33_InputCurrentC","1号C相输入电流","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["433","4.19.40.1","UL33_InputFrequency","1号输入频率（三相一致）","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["434","4.19.40.1","UL33_AphaseBypassVoltage","1号A相旁路电压","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["435","4.19.40.1","UL33_BphaseBypassVoltage","1号B相旁路电压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["436","4.19.40.1","UL33_CphaseBypassVoltage","1号C相旁路电压","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["437","4.19.40.1","UL33_AphaseBypassCurrent","1号A相旁路电流","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["438","4.19.40.1","UL33_BphaseBypassCurrent","1号B相旁路电流","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["439","4.19.40.1","UL33_CphaseBypassCurrent","1号C相旁路电流","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["440","4.19.40.1","UL33_BypassFrequency","1号旁路频率（三相一致）","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["441","4.19.40.1","UL33_BatteryTemperature","1号电池温度","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["442","4.19.40.1","UL33_AphaseOutputActivePower","1号A相输出有功功率","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["443","4.19.40.1","UL33_BphaseOutputActivePower","1号B相输出有功功率","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["444","4.19.40.1","UL33_CphaseOutputActivePower","1号C相输出有功功率","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["445","4.19.40.1","UL33_BatteryCurrent","1号电池电流","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["446","4.19.40.1","UL33_RemainingBatteryBackupTime","1号电池剩余后备时间","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","99999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["447","4.19.40.1","UL33_AphaseOutputApparentPower","1号A相输出视在功率","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","99999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["448","4.19.40.1","UL33_BphaseOutputApparentPower","1号B相输出视在功率","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","99999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["449","4.19.40.1","UL33_CphaseOutputApparentPower","1号C相输出视在功率","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["450","4.19.40.1","UL33_AphaseOutputpercentage","1号A相输出负载百分比","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["451","4.19.40.1","UL33_BphaseOutputpercentage","1号B相输出负载百分比","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["452","4.19.40.1","UL33_CphaseOutputpercentage","1号C相输出负载百分比","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["453","4.19.40.1","UL33_Temperature","1号环境温度","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["454","4.19.40.1","UL33_AphaseOutputPeakRatio","1号A相输出峰值比","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["455","4.19.40.1","UL33_BphaseOutputPeakRatio","1号B相输出峰值比","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["456","4.19.40.1","UL33_CphaseOutputPeakRatio","1号C相输出峰值比","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["457","4.19.40.1","UL33_PowerSupply","1号供电方式","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["458","4.19.40.1","UL33_BatterySelfTest","1号电池自检状态","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["459","4.19.40.1","UL33_AllChargeOrFloat","1号均充/浮充（正组）","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["460","4.19.40.1","UL33_OffState","1号开机/关机","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","228","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","229,","UPS关机,"]
["461","4.19.40.1","UL33_UPSPowerSupply","1号UPS供电","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","232","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","231，233,","电池逆变供电,电池市电联合逆变供电,"]
["462","4.19.40.1","UL33_SynORasynchronous","1号同步/不同步","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["463","4.19.40.1","UL33_MainsVoltage","1号市电电压","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","2，3,","异常,欠压,"]
["464","4.19.40.1","UL33_RectifierStatus","1号整流器状态","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["465","4.19.40.1","UL33_InverterStatus","1号逆变器状态","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","249,","故障,"]
["466","4.19.40.1","UL33_BypassConditions","1号旁路情况（电压或频率）","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","1,2,","超出跟踪范围,超出保护范围,"]
["467","4.19.40.1","UL33_TheTotalBatteryVoltageStatus","1号蓄电池总电压状态","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","5","1,2,3,240,225,","无电池,低于下限,高于上限,接反,预告警,"]
["468","4.19.40.1","UL33_BatterySelfTestResults","1号电池自检结果","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","需要更换电池,"]
["469","4.19.40.1","UL33_MainsFrequency","1号市电频率","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["470","4.19.40.1","UL33_InverterFanFailure","1号逆变风扇故障","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["471","4.19.40.1","UL33_RectifierFanFailure","1号整流风扇故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["472","4.19.40.1","UL33_BatteryContactorFailure","1号电池接触器故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["473","4.19.40.1","UL33_MainRoadContactorException","1号主路接触器异常","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["474","4.19.40.1","UL33_OutputOverload","1号本机输出过载","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","过载,"]
["475","4.19.40.1","UL33_AbnormalShutdownBypass","1号旁路异常关机","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["476","4.19.40.1","UL33_AC_OutputOvervoltage","1号交流输出过压","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["477","4.19.40.1","UL33_CurrentOutput","1号输出冲击过流","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["478","4.19.40.1","UL33_OverCurrentInverter","1号逆变模块过流","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["479","4.19.40.1","UL33_OverCurrentRectifier","1号整流模块过流","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["480","4.19.40.1","UL33_BypassLoadImpact","1号负载冲击转旁路","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["481","4.19.40.1","UL33_TemperatureHigh","1号环境温度过高","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","2,","告警,"]
["482","4.19.40.1","UL33_RectifierCommunicationFailure","1号整流通讯故障","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["483","4.19.40.1","UL33_InverterCommunicationFailure","1号逆变通讯故障","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["69","4.19.40.2","UL33_1AC_InputPhaseVoltageA","交流输入相电压A","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["70","4.19.40.2","UL33_1AC_InputPhaseVoltageB","交流输入相电压B","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["71","4.19.40.2","UL33_1AC_InputPhaseVoltageC","交流输入相电压C","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["72","4.19.40.2","UL33_1AC_OutputPhaseVoltageA","交流输出相电压A","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["73","4.19.40.2","UL33_1AC_OutputPhaseVoltageB","交流输出相电压B","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["74","4.19.40.2","UL33_1AC_OutputPhaseVoltageC","交流输出相电压C","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["75","4.19.40.2","UL33_1AC_OutputCurrentA","交流输出电流A","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["76","4.19.40.2","UL33_1AC_OutputCurrentB","交流输出电流B","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["77","4.19.40.2","UL33_1AC_OutputCurrentC","交流输出电流C","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["78","4.19.40.2","UL33_1BatteryVoltage","电池电压","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","4.19.40.2","UL33_1OutputFrequency","输出频率（三相一致）","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["80","4.19.40.2","UL33_1AC_InputLineVoltageAB","交流输入线电压AB","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["81","4.19.40.2","UL33_1AC_InputLineVoltageBC","交流输入线电压BC","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["82","4.19.40.2","UL33_1AC_InputLineVoltageCA","交流输入线电压CA","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["83","4.19.40.2","UL33_1InputCurrentA","A相输入电流","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["84","4.19.40.2","UL33_1InputCurrentB","B相输入电流","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["85","4.19.40.2","UL33_1InputCurrentC","C相输入电流","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["86","4.19.40.2","UL33_1InputFrequency","输入频率（三相一致）","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["87","4.19.40.2","UL33_1AphaseBypassVoltage","A相旁路电压","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["88","4.19.40.2","UL33_1BphaseBypassVoltage","B相旁路电压","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["89","4.19.40.2","UL33_1CphaseBypassVoltage","C相旁路电压","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["90","4.19.40.2","UL33_1AphaseBypassCurrent","A相旁路电流","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["91","4.19.40.2","UL33_1BphaseBypassCurrent","B相旁路电流","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["92","4.19.40.2","UL33_1CphaseBypassCurrent","C相旁路电流","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["93","4.19.40.2","UL33_1BypassFrequency","旁路频率（三相一致）","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["94","4.19.40.2","UL33_1BatteryTemperature","电池温度","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["95","4.19.40.2","UL33_1AphaseOutputActivePower","A相输出有功功率","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["96","4.19.40.2","UL33_1BphaseOutputActivePower","B相输出有功功率","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["97","4.19.40.2","UL33_1CphaseOutputActivePower","C相输出有功功率","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","9999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["98","4.19.40.2","UL33_1BatteryCurrent","电池电流","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["99","4.19.40.2","UL33_1RemainingBatteryBackupTime","电池剩余后备时间","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","99999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["100","4.19.40.2","UL33_1AphaseOutputApparentPower","A相输出视在功率","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","99999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["101","4.19.40.2","UL33_1BphaseOutputApparentPower","B相输出视在功率","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","99999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["102","4.19.40.2","UL33_1CphaseOutputApparentPower","C相输出视在功率","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["103","4.19.40.2","UL33_1AphaseOutputpercentage","A相输出负载百分比","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["104","4.19.40.2","UL33_1BphaseOutputpercentage","B相输出负载百分比","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["105","4.19.40.2","UL33_1CphaseOutputpercentage","C相输出负载百分比","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["106","4.19.40.2","UL33_1Temperature","环境温度","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["107","4.19.40.2","UL33_1AphaseOutputPeakRatio","A相输出峰值比","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["108","4.19.40.2","UL33_1BphaseOutputPeakRatio","B相输出峰值比","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","999","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["109","4.19.40.2","UL33_1CphaseOutputPeakRatio","C相输出峰值比","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["110","4.19.40.2","UL33_1PowerSupply","供电方式","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","233,","UPS与旁路均不供电,"]
["111","4.19.40.2","UL33_1BatterySelfTest","电池自检状态","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["112","4.19.40.2","UL33_1AllChargeOrFloat","均充/浮充（正组）","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["113","4.19.40.2","UL33_1OffState","开机/关机","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","228","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","229,","UPS关机,"]
["114","4.19.40.2","UL33_1UPSPowerSupply","UPS供电","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","232","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","2","231，233,","电池逆变供电,电池市电联合逆变供电,"]
["115","4.19.40.2","UL33_1SynORasynchronous","同步/不同步","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["116","4.19.40.2","UL33_1MainsVoltage","市电电压","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","2，3,","异常,欠压,"]
["117","4.19.40.2","UL33_1RectifierStatus","整流器状态","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["118","4.19.40.2","UL33_1InverterStatus","逆变器状态","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","249,","故障,"]
["119","4.19.40.2","UL33_1BypassConditions","旁路情况（电压或频率）","1","0","0","1","0","cmd-57","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","2","1,2,","超出跟踪范围,超出保护范围,"]
["120","4.19.40.2","UL33_1TheTotalBatteryVoltageStatus","蓄电池总电压状态","1","0","0","1","0","cmd-58","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","5","1,2,3,240,225,","无电池,低于下限,高于上限,接反,预告警,"]
["121","4.19.40.2","UL33_1BatterySelfTestResults","电池自检结果","1","0","0","1","0","cmd-59","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","需要更换电池,"]
["122","4.19.40.2","UL33_1MainsFrequency","市电频率","1","0","0","1","0","cmd-60","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["123","4.19.40.2","UL33_1InverterFanFailure","逆变风扇故障","1","0","0","1","0","cmd-68","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["124","4.19.40.2","UL33_1RectifierFanFailure","整流风扇故障","1","0","0","1","0","cmd-69","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["125","4.19.40.2","UL33_1BatteryContactorFailure","电池接触器故障","1","0","0","1","0","cmd-70","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["126","4.19.40.2","UL33_1MainRoadContactorException","主路接触器异常","1","0","0","1","0","cmd-71","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["127","4.19.40.2","UL33_1OutputOverload","本机输出过载","1","0","0","1","0","cmd-75","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","过载,"]
["128","4.19.40.2","UL33_1AbnormalShutdownBypass","旁路异常关机","1","0","0","1","0","cmd-81","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["129","4.19.40.2","UL33_1AC_OutputOvervoltage","交流输出过压","1","0","0","1","0","cmd-85","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","异常,"]
["130","4.19.40.2","UL33_1CurrentOutput","输出冲击过流","1","0","0","1","0","cmd-86","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["131","4.19.40.2","UL33_1OverCurrentInverter","逆变模块过流","1","0","0","1","0","cmd-87","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["132","4.19.40.2","UL33_1OverCurrentRectifier","整流模块过流","1","0","0","1","0","cmd-88","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["133","4.19.40.2","UL33_1BypassLoadImpact","负载冲击转旁路","1","0","0","1","0","cmd-89","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","240,","故障,"]
["134","4.19.40.2","UL33_1TemperatureHigh","环境温度过高","1","0","0","1","0","cmd-94","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","2,","告警,"]
["135","4.19.40.2","UL33_1RectifierCommunicationFailure","整流通讯故障","1","0","0","1","0","cmd-95","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]
["136","4.19.40.2","UL33_1InverterCommunicationFailure","逆变通讯故障","1","0","0","1","0","cmd-96","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","40",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","0","0","0"]