{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":13,"n_cols":41,"rows_kept":13,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值"]
["104","6.7.88.1","stulz1ReturnTemp","1号空调回温温度","1","2","0","1","2","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0","3","0","1","0","0","0","0","0","88",null,null,"0"]
["105","6.7.88.1","stulz1ReturnHumidity","1号空调回温湿度","1","2","0","1","6","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0","3","0","1","0","0","0","0","0","88",null,null,"0"]
["107","6.7.88.1","stulz1Compressor","1号空调模块1压缩机","1","1","0","1","22","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","33","88",null,null,"0"]
["108","6.7.88.1","stulz1Humidification","1号空调模块1加湿器","1","1","0","1","22","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","34","88",null,null,"0"]
["109","6.7.88.1","stulz1DeHumidification","1号空调模块1除湿器","1","1","0","1","22","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","35","88",null,null,"0"]
["112","6.7.88.1","stulz1Reheat3","1号空调模块1电加热器","1","1","0","1","22","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","39","88",null,null,"0"]
["115","6.7.88.1","stulz1ReturnAirTempTooHigh","1号空调室内温度太高","1","1","0","1","133","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","32","88",null,null,"0"]
["116","6.7.88.1","stulz1ReturnAirHumidityTooHigh","1号空调室内湿度太高","1","1","0","1","133","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","33","88",null,null,"0"]
["117","6.7.88.1","stulz1ReturnAirTempTooLow","1号空调室内温度太低","1","1","0","1","133","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","37","88",null,null,"0"]
["118","6.7.88.1","stulz1ReturnAirHumidityTooLow","1号空调室内湿度太低","1","1","0","1","133","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","38","88",null,null,"0"]
["306","6.7.88.1","stulz1Reheat1","1号空调模块1电加热器1","1","1","0","1","22","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","32","88",null,null,"0"]
["307","6.7.88.1","stulz1Fan","1号空调模块1风机","1","1","0","1","22","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","1","3","0","1","0","0","0","0","36","88",null,null,"0"]