{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":85,"n_cols":76,"rows_kept":85,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["51","6.35.139.1","DME30001_RoomTemp","六号一楼空调1室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"20","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["52","6.35.139.1","DME30001_RoomHumidity","六号一楼空调1室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"60","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["53","6.35.139.1","DME30001_TempBias","六号一楼空调1温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["54","6.35.139.1","DME30001_HumidityBias","六号一楼空调1湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["55","6.35.139.1","DME30001_TempSetPoint","六号一楼空调1温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["56","6.35.139.1","DME30001_HumiditySetPoint","六号一楼空调1湿度设定点","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["57","6.35.139.1","DME30001_AirCondition","六号一楼空调1空调状态","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["58","6.35.139.1","DME30001_FanStatus","六号一楼空调1风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["59","6.35.139.1","DME30001_CoolingStatus","六号一楼空调1制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["60","6.35.139.1","DME30001_HeatingStatus","六号一楼空调1加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["61","6.35.139.1","DME30001_WetStatus","六号一楼空调1加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["62","6.35.139.1","DME30001_DehumidificationStatus","六号一楼空调1除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["63","6.35.139.1","DME30001_HighAlarm","六号一楼空调1高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["64","6.35.139.1","DME30001_LowAlarm","六号一楼空调1低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"1","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["65","6.35.139.1","DME30001_HighTempAlarm","六号一楼空调1高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomTemp",{"$nulls":9},"1","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["66","6.35.139.1","DME30001_LowTempAlarm","六号一楼空调1低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomTemp",{"$nulls":9},"1","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["67","6.35.139.1","DME30001_HighHumidityAlarm","六号一楼空调1高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomHumidity",{"$nulls":9},"1","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["68","6.35.139.1","DME30001_LowHumidityAlarm","六号一楼空调1低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomHumidity",{"$nulls":9},"1","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["69","6.35.139.1","DME30001_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["70","6.35.139.1","DME30001_CommunicationFailureAlarm","六号一楼空调1通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["433","6.35.139.1","DME30001_Communications","六号楼一楼空调1串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","通讯中断,"]
["71","6.35.139.2","DME30002_RoomTemp","六号一楼空调2室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["72","6.35.139.2","DME30002_RoomHumidity","六号一楼空调2室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["76","6.35.139.2","DME30002_TempBias","六号一楼空调2温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["77","6.35.139.2","DME30002_HumidityBias","六号一楼空调2湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["78","6.35.139.2","DME30002_TempSetPoint","六号一楼空调2温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","6.35.139.2","DME30002_HumiditySetPoint","六号一楼空调2湿度设定点","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["80","6.35.139.2","DME30002_AirCondition","六号一楼空调2空调状态","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["81","6.35.139.2","DME30002_FanStatus","六号一楼空调2风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["82","6.35.139.2","DME30002_CoolingStatus","六号一楼空调2制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["83","6.35.139.2","DME30002_HeatingStatus","六号一楼空调2加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["84","6.35.139.2","DME30002_WetStatus","六号一楼空调2加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["85","6.35.139.2","DME30002_DehumidificationStatus","六号一楼空调2除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["86","6.35.139.2","DME30002_HighAlarm","六号一楼空调2高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["87","6.35.139.2","DME30002_LowAlarm","六号一楼空调2低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["88","6.35.139.2","DME30002_HighTempAlarm","六号一楼空调2高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomTemp",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["89","6.35.139.2","DME30002_LowTempAlarm","六号一楼空调2低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomTemp",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["90","6.35.139.2","DME30002_HighHumidityAlarm","六号一楼空调2高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomHumidity",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["91","6.35.139.2","DME30002_LowHumidityAlarm","六号一楼空调2低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomHumidity",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["92","6.35.139.2","DME30002_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["93","6.35.139.2","DME30002_CommunicationFailureAlarm","六号一楼空调2通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["434","6.35.139.2","DME30002_Communications","六号楼一楼空调2串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","通讯中断,"]
["94","6.35.139.3","DME30003_RoomTemp","三号五楼空调1室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["95","6.35.139.3","DME30003_RoomHumidity","三号五楼空调1室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["99","6.35.139.3","DME30003_TempBias","三号五楼空调1温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["100","6.35.139.3","DME30003_HumidityBias","三号五楼空调1湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["101","6.35.139.3","DME30003_TempSetPoint","三号五楼空调1温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["102","6.35.139.3","DME30003_HumiditySetPoint","三号五楼空调1湿度设定点","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["103","6.35.139.3","DME30003_AirCondition","三号五楼空调1空调状态","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["104","6.35.139.3","DME30003_FanStatus","三号五楼空调1风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["105","6.35.139.3","DME30003_CoolingStatus","三号五楼空调1制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["106","6.35.139.3","DME30003_HeatingStatus","三号五楼空调1加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["107","6.35.139.3","DME30003_WetStatus","三号五楼空调1加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["108","6.35.139.3","DME30003_DehumidificationStatus","三号五楼空调1除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["109","6.35.139.3","DME30003_HighAlarm","三号五楼空调1高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["110","6.35.139.3","DME30003_LowAlarm","三号五楼空调1低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["111","6.35.139.3","DME30003_HighTempAlarm","三号五楼空调1高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomTemp",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["112","6.35.139.3","DME30003_LowTempAlarm","三号五楼空调1低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomTemp",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["113","6.35.139.3","DME30003_HighHumidityAlarm","三号五楼空调1高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomHumidity",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["114","6.35.139.3","DME30003_LowHumidityAlarm","三号五楼空调1低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomHumidity",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["115","6.35.139.3","DME30003_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["116","6.35.139.3","DME30003_CommunicationFailureAlarm","三号五楼空调1通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["439","6.35.139.3","DME30003_Communications","三号楼5楼空调1串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","通讯中断,"]
["117","6.35.139.4","DME30004_RoomTemp","三号五楼空调2室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["118","6.35.139.4","DME30004_RoomHumidity","三号五楼空调2室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["122","6.35.139.4","DME30004_TempBias","三号五楼空调2温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["123","6.35.139.4","DME30004_HumidityBias","三号五楼空调2湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["124","6.35.139.4","DME30004_TempSetPoint","三号五楼空调2温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["125","6.35.139.4","DME30004_HumiditySetPoint","三号五楼空调2湿度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["126","6.35.139.4","DME30004_AirCondition","三号五楼空调2空调状态","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["127","6.35.139.4","DME30004_FanStatus","三号五楼空调2风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["128","6.35.139.4","DME30004_CoolingStatus","三号五楼空调2制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["129","6.35.139.4","DME30004_HeatingStatus","三号五楼空调2加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["130","6.35.139.4","DME30004_WetStatus","三号五楼空调2加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["131","6.35.139.4","DME30004_DehumidificationStatus","三号五楼空调2除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["132","6.35.139.4","DME30004_HighAlarm","三号五楼空调2高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["133","6.35.139.4","DME30004_LowAlarm","三号五楼空调2低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["134","6.35.139.4","DME30004_HighTempAlarm","三号五楼空调2高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomTemp",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["135","6.35.139.4","DME30004_LowTempAlarm","三号五楼空调2低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomTemp",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["136","6.35.139.4","DME30004_HighHumidityAlarm","三号五楼空调2高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomHumidity",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["137","6.35.139.4","DME30004_LowHumidityAlarm","三号五楼空调2低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomHumidity",{"$nulls":9},"0","0","2","0","0","0","0","0","0","0","1","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["138","6.35.139.4","DME30004_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["139","6.35.139.4","DME30004_CommunicationFailureAlarm","三号五楼空调2通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","报警,"]
["440","6.35.139.4","DME30004_Communications","三号楼5楼空调2串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","1","1,","通讯中断,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":94,"n_cols":76,"rows_kept":94,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["51","6.35.139.1","DME30001_RoomTemp","六号一楼空调1室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["52","6.35.139.1","DME30001_RoomHumidity","六号一楼空调1室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["53","6.35.139.1","DME30001_TempBias","六号一楼空调1温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["54","6.35.139.1","DME30001_HumidityBias","六号一楼空调1湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["55","6.35.139.1","DME30001_TempSetPoint","六号一楼空调1温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["56","6.35.139.1","DME30001_HumiditySetPoint","六号一楼空调1湿度设定点","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["57","6.35.139.1","DME30001_AirCondition","六号一楼空调1空调状态","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["58","6.35.139.1","DME30001_FanStatus","六号一楼空调1风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["59","6.35.139.1","DME30001_CoolingStatus","六号一楼空调1制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["60","6.35.139.1","DME30001_HeatingStatus","六号一楼空调1加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["61","6.35.139.1","DME30001_WetStatus","六号一楼空调1加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["62","6.35.139.1","DME30001_DehumidificationStatus","六号一楼空调1除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["63","6.35.139.1","DME30001_HighAlarm","六号一楼空调1高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["64","6.35.139.1","DME30001_LowAlarm","六号一楼空调1低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["65","6.35.139.1","DME30001_HighTempAlarm","六号一楼空调1高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["66","6.35.139.1","DME30001_LowTempAlarm","六号一楼空调1低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["67","6.35.139.1","DME30001_HighHumidityAlarm","六号一楼空调1高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["68","6.35.139.1","DME30001_LowHumidityAlarm","六号一楼空调1低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30001_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["69","6.35.139.1","DME30001_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["70","6.35.139.1","DME30001_CommunicationFailureAlarm","六号一楼空调1通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["71","6.35.139.2","DME30002_RoomTemp","六号一楼空调2室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["72","6.35.139.2","DME30002_RoomHumidity","六号一楼空调2室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["73","6.35.139.2","DME30002_OutdoorTemp","六号一楼空调2室外温度","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["74","6.35.139.2","DME30002_OpenTemp","六号一楼空调2开机温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["75","6.35.139.2","DME30002_CloseTemp","六号一楼空调2关机温度","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["76","6.35.139.2","DME30002_TempBias","六号一楼空调2温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["77","6.35.139.2","DME30002_HumidityBias","六号一楼空调2湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["78","6.35.139.2","DME30002_TempSetPoint","六号一楼空调2温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["79","6.35.139.2","DME30002_HumiditySetPoint","六号一楼空调2湿度设定点","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["80","6.35.139.2","DME30002_AirCondition","六号一楼空调2空调状态","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["81","6.35.139.2","DME30002_FanStatus","六号一楼空调2风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["82","6.35.139.2","DME30002_CoolingStatus","六号一楼空调2制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["83","6.35.139.2","DME30002_HeatingStatus","六号一楼空调2加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["84","6.35.139.2","DME30002_WetStatus","六号一楼空调2加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["85","6.35.139.2","DME30002_DehumidificationStatus","六号一楼空调2除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["86","6.35.139.2","DME30002_HighAlarm","六号一楼空调2高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["87","6.35.139.2","DME30002_LowAlarm","六号一楼空调2低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["88","6.35.139.2","DME30002_HighTempAlarm","六号一楼空调2高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["89","6.35.139.2","DME30002_LowTempAlarm","六号一楼空调2低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["90","6.35.139.2","DME30002_HighHumidityAlarm","六号一楼空调2高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["91","6.35.139.2","DME30002_LowHumidityAlarm","六号一楼空调2低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30002_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["92","6.35.139.2","DME30002_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["93","6.35.139.2","DME30002_CommunicationFailureAlarm","六号一楼空调2通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["94","6.35.139.3","DME30003_RoomTemp","三号五楼空调1室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["95","6.35.139.3","DME30003_RoomHumidity","三号五楼空调1室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["96","6.35.139.3","DME30003_OutdoorTemp","三号五楼空调1室外温度","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["97","6.35.139.3","DME30003_OpenTemp","三号五楼空调1开机温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["98","6.35.139.3","DME30003_CloseTemp","三号五楼空调1关机温度","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["99","6.35.139.3","DME30003_TempBias","三号五楼空调1温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["100","6.35.139.3","DME30003_HumidityBias","三号五楼空调1湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["101","6.35.139.3","DME30003_TempSetPoint","三号五楼空调1温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["102","6.35.139.3","DME30003_HumiditySetPoint","三号五楼空调1湿度设定点","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["103","6.35.139.3","DME30003_AirCondition","三号五楼空调1空调状态","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["104","6.35.139.3","DME30003_FanStatus","三号五楼空调1风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["105","6.35.139.3","DME30003_CoolingStatus","三号五楼空调1制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["106","6.35.139.3","DME30003_HeatingStatus","三号五楼空调1加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["107","6.35.139.3","DME30003_WetStatus","三号五楼空调1加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["108","6.35.139.3","DME30003_DehumidificationStatus","三号五楼空调1除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["109","6.35.139.3","DME30003_HighAlarm","三号五楼空调1高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["110","6.35.139.3","DME30003_LowAlarm","三号五楼空调1低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["111","6.35.139.3","DME30003_HighTempAlarm","三号五楼空调1高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["112","6.35.139.3","DME30003_LowTempAlarm","三号五楼空调1低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["113","6.35.139.3","DME30003_HighHumidityAlarm","三号五楼空调1高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["114","6.35.139.3","DME30003_LowHumidityAlarm","三号五楼空调1低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30003_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["115","6.35.139.3","DME30003_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["116","6.35.139.3","DME30003_CommunicationFailureAlarm","三号五楼空调1通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["117","6.35.139.4","DME30004_RoomTemp","三号五楼空调2室内温度","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["118","6.35.139.4","DME30004_RoomHumidity","三号五楼空调2室内湿度","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["119","6.35.139.4","DME30004_OutdoorTemp","三号五楼空调2室外温度","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["120","6.35.139.4","DME30004_OpenTemp","三号五楼空调2开机温度","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["121","6.35.139.4","DME30004_CloseTemp","三号五楼空调2关机温度","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["122","6.35.139.4","DME30004_TempBias","三号五楼空调2温度偏差","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["123","6.35.139.4","DME30004_HumidityBias","三号五楼空调2湿度偏差","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["124","6.35.139.4","DME30004_TempSetPoint","三号五楼空调2温度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["125","6.35.139.4","DME30004_HumiditySetPoint","三号五楼空调2湿度设定点","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","0.1000000015","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["126","6.35.139.4","DME30004_AirCondition","三号五楼空调2空调状态","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["127","6.35.139.4","DME30004_FanStatus","三号五楼空调2风机状态","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["128","6.35.139.4","DME30004_CoolingStatus","三号五楼空调2制冷状态","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["129","6.35.139.4","DME30004_HeatingStatus","三号五楼空调2加热状态","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["130","6.35.139.4","DME30004_WetStatus","三号五楼空调2加湿状态","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["131","6.35.139.4","DME30004_DehumidificationStatus","三号五楼空调2除湿状态","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["132","6.35.139.4","DME30004_HighAlarm","三号五楼空调2高压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["133","6.35.139.4","DME30004_LowAlarm","三号五楼空调2低压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["134","6.35.139.4","DME30004_HighTempAlarm","三号五楼空调2高温","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["135","6.35.139.4","DME30004_LowTempAlarm","三号五楼空调2低温","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomTemp",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["136","6.35.139.4","DME30004_HighHumidityAlarm","三号五楼空调2高湿","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["137","6.35.139.4","DME30004_LowHumidityAlarm","三号五楼空调2低湿","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0","DME30004_RoomHumidity",{"$nulls":9},"0","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["138","6.35.139.4","DME30004_RemoteControl","遥控","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","0","0","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["139","6.35.139.4","DME30004_CommunicationFailureAlarm","三号五楼空调2通讯故障","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["433","6.35.139.1","DME3000_1_ComStatus","六号楼一楼空调1串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["434","6.35.139.2","DME3000_2_ComStatus","六号楼一楼空调2串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["439","6.35.139.3","DME3000_3_ComStatus","三号楼5楼空调1串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["440","6.35.139.4","DME3000_4_ComStatus","三号楼5楼空调2串口状态","1000","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","139","关","开","0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]