{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":20,"n_cols":76,"rows_kept":20,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["35","9.1.114.3","TSDLY_APhase","电量仪A相电压","4","2","1","3","13",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0.0099999998","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","9.1.114.3","TSDLY_BPhase","电量仪B相电压","4","2","1","3","15",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0.0099999998","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["37","9.1.114.3","TSDLY_CPhase","电量仪C相电压","4","2","1","3","17",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0.0099999998","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
[]
["35","9.1.114.3","TSDLY_ABLine","电量仪AB线电压","4","2","1","3","19",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0.0099999998","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["36","9.1.114.3","TSDLY_BCLine","电量仪BC线电压","4","2","1","3","21",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0.0099999998","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["37","9.1.114.3","TSDLY_CALine","电量仪CA线电压","4","2","1","3","23",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0.0099999998","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","1000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
[]
["39","9.1.114.3","TSDLY_ACurr","电量仪A相电流","4","2","1","3","25",null,null,"0","30","60","1",null,null,"5","0","300","0","0","0","0","0","0",null,"900","0.0001000000","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["40","9.1.114.3","TSDLY_BCurr","电量仪B相电流","4","2","1","3","27",null,null,"0","30","60","1",null,null,"5","0","300","0","0","0","0","0","0",null,"900","0.0001000000","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["41","9.1.114.3","TSDLY_CCurr","电量仪C相电流","4","2","1","3","29",null,null,"0","30","60","1",null,null,"5","0","300","0","0","0","0","0","0",null,"900","0.0001000000","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
[]
["44","9.1.114.3","TSDLY_APhasePower","电量仪A相有功功率","4","2","1","3","31",null,null,"0","30","60","1",null,null,"5","0","300","0","0","0","0","0","0",null,"900","0.4000000060","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["45","9.1.114.3","TSDLY_BPhasePower","电量仪B相有功功率","4","2","1","3","33",null,null,"0","30","60","1",null,null,"5","0","300","0","0","0","0","0","0",null,"900","0.4000000060","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["46","9.1.114.3","TSDLY_CPhasePower","电量仪C相有功功率","4","2","1","3","35",null,null,"0","30","60","1",null,null,"5","0","300","0","0","0","0","0","0",null,"900","0.4000000060","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["47","9.1.114.3","TSDLY_TotalPower","电量仪总有功功率","4","2","1","3","37",null,null,"0","30","60","1",null,null,"5","0","300","0","0","0","0","0","0",null,"900","0.4000000060","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","10000","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["43","9.1.114.3","TSDLY_Freq","电量仪频率","3","2","1","3","63",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"900","0.0010681300","3","0","1","1","0","0","0","0","114",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
[]
["51","9.1.114.3","TSDLY_Communications","电量仪串口状态","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","114","关","开","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","通信中断,"]