{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["CMD_Log_2022_09_06","色温仪指令","AutoGamma调试流程"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CMD_Log_2022_09_06","index":0,"n_rows":810,"n_cols":10,"rows_kept":810,"cut":false,"hidden":false,"merged":[]}
["No","FSN","命令名称","命令输入","命令返回","开始时间","结束时间","指令耗时","间隔时间","异常Log"]
[1,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 17:17:06.85"," 17:17:07.24",0.38400000000000001,3600]
[2,null,"老化模式关闭","AA 06 13 00 E2 9D","AB 05 0A DF 4E"," 17:17:07.56"," 17:17:07.58",0.02,0.32300000000000001]
[3,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:17:07.68"," 17:17:07.76",8.3000000000000004E-2,0.10199999999999999]
[4,null,"0xEA00_King_Wide_vine_keyCheck","AA 06 EA 00 4B C4","AB 05 0A DF 4E AB 07 EB 00 01 C6 5B"," 17:17:07.97"," 17:17:08.23",0.26500000000000001,0.20300000000000001]
[5,null,"0xEA07_King_MGK_keyCheck","AA 06 EA 07 3B 23","AB 05 0A DF 4E AB 07 EB 07 01 5F CC"," 17:17:08.29"," 17:17:08.54",0.249,5.5E-2]
[6,null,"0xEA0D_King_Attestation_keyCheck","AA 06 EA 0D 9A 69","AB 05 0A DF 4E AB 07 EB 0D 01 B0 07"," 17:17:08.59"," 17:17:08.71",0.123,5.1999999999999998E-2]
[7,null,"0xEA12_King_Playready_keyCheck","AA 06 EA 12 79 B7","AB 05 0A DF 4E AB 07 EB 12 01 A3 4A"," 17:17:08.79"," 17:17:09.10",0.315,7.8E-2]
[8,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 1E 58 56 38 2D 54 32 32 31 54 30 32 2D 4C 46 31 4D 30 32 34 2E 30 30 30 31 37 38 43 53"," 17:17:09.25"," 17:17:09.33",7.2999999999999995E-2,0.151]
[9,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 1E 58 56 38 2D 54 32 32 31 54 30 32 2D 4C 46 31 4D 30 32 34 2E 30 30 30 31 37 38 43 53"," 17:17:09.33"," 17:17:09.42",9.2999999999999999E-2,2E-3]
[10,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 1E 58 56 38 2D 54 32 32 31 54 30 32 2D 4C 46 31 4D 30 32 34 2E 30 30 30 31 37 38 43 53"," 17:17:09.42"," 17:17:09.55",0.125,1E-3]
[11,null,"内置PATTERN关闭","AA 06 27 00 2B CC","AB 05 0A DF 4E"," 17:17:09.56"," 17:17:09.65",9.1999999999999998E-2,6.0000000000000001E-3]
[1,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 17:17:34.06"," 17:17:34.14",8.1000000000000003E-2,24.408999999999999]
[2,null,"老化模式关闭","AA 06 13 00 E2 9D","AB 05 0A DF 4E"," 17:17:34.14"," 17:17:34.25",0.114,2E-3]
[3,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:17:34.36"," 17:17:34.44",8.2000000000000003E-2,0.10299999999999999]
[4,null,"0xEA00_King_Wide_vine_keyCheck","AA 06 EA 00 4B C4","AB 05 0A DF 4E AB 07 EB 00 01 C6 5B"," 17:17:34.64"," 17:17:34.90",0.26300000000000001,0.20300000000000001]
[5,null,"0xEA07_King_MGK_keyCheck","AA 06 EA 07 3B 23","AB 05 0A DF 4E AB 07 EB 07 01 5F CC"," 17:17:34.95"," 17:17:35.23",0.27500000000000002,5.0999999999999997E-2]
[6,null,"0xEA0D_King_Attestation_keyCheck","AA 06 EA 0D 9A 69","AB 05 0A DF 4E AB 07 EB 0D 01 B0 07"," 17:17:35.28"," 17:17:35.39",0.111,5.1999999999999998E-2]
[7,null,"0xEA12_King_Playready_keyCheck","AA 06 EA 12 79 B7","AB 05 0A DF 4E AB 07 EB 12 01 A3 4A"," 17:17:35.44"," 17:17:35.78",0.33700000000000002,5.0999999999999997E-2]
[8,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 1E 58 56 38 2D 54 32 32 31 54 30 32 2D 4C 46 31 4D 30 32 34 2E 30 30 30 31 37 38 43 53"," 17:17:35.93"," 17:17:36.00",6.2E-2,0.152]
[9,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 17:17:36.00"," 17:17:36.11",0.113,2E-3]
[10,null,"内置PATTERN关闭","AA 06 27 00 2B CC","AB 05 0A DF 4E"," 17:17:36.11"," 17:17:36.22",0.112,1E-3]
[1,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 17:17:52.47"," 17:17:52.54",7.0999999999999994E-2,16.25]
[2,null,"老化模式关闭","AA 06 13 00 E2 9D","AB 05 0A DF 4E"," 17:17:52.55"," 17:17:52.67",0.121,3.0000000000000001E-3]
[3,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:17:52.77"," 17:17:52.86",8.4000000000000005E-2,0.10299999999999999]
[4,null,"0xEA00_King_Wide_vine_keyCheck","AA 06 EA 00 4B C4","AB 05 0A DF 4E AB 07 EB 00 01 C6 5B"," 17:17:53.06"," 17:17:53.32",0.26300000000000001,0.20300000000000001]
[5,null,"0xEA07_King_MGK_keyCheck","AA 06 EA 07 3B 23","AB 05 0A DF 4E AB 07 EB 07 01 5F CC"," 17:17:53.37"," 17:17:53.65",0.27600000000000002,5.1999999999999998E-2]
[6,null,"0xEA0D_King_Attestation_keyCheck","AA 06 EA 0D 9A 69","AB 05 0A DF 4E AB 07 EB 0D 01 B0 07"," 17:17:53.70"," 17:17:53.81",0.111,5.1999999999999998E-2]
[7,null,"0xEA12_King_Playready_keyCheck","AA 06 EA 12 79 B7","AB 05 0A DF 4E AB 07 EB 12 01 A3 4A"," 17:17:53.86"," 17:17:54.20",0.33500000000000002,5.0999999999999997E-2]
[8,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 1E 58 56 38 2D 54 32 32 31 54 30 32 2D 4C 46 31 4D 30 32 34 2E 30 30 30 31 37 38 43 53"," 17:17:54.35"," 17:17:54.41",6.0999999999999999E-2,0.152]
[9,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 17:17:54.41"," 17:17:54.53",0.113,2E-3]
[10,null,"内置PATTERN关闭","AA 06 27 00 2B CC","AB 05 0A DF 4E"," 17:17:54.53"," 17:17:54.64",0.115,2E-3]
[2,null,"老化模式关闭","AA 06 13 00 E2 9D","AB 05 0A DF 4E"," 17:21:37.63"," 17:21:37.72",8.3000000000000004E-2,8.1980000000000004]
[3,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:37.82"," 17:21:37.91",9.5000000000000001E-2,0.10100000000000001]
[4,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:37.91"," 17:21:38.02",0.105,2E-3]
[5,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:38.02"," 17:21:38.12",0.10199999999999999,2E-3]
[6,null,"内置PATTERN关闭","AA 06 27 00 2B CC","AB 05 0A DF 4E"," 17:21:38.13"," 17:21:38.24",0.113,5.0000000000000001E-3]
[1,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 17:21:44.26"," 17:21:44.30",4.1000000000000002E-2,6.0220000000000002]
[2,null,"老化模式关闭","AA 06 13 00 E2 9D","AB 05 0A DF 4E"," 17:21:44.31"," 17:21:44.42",0.115,2E-3]
[3,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:44.52"," 17:21:44.60",8.2000000000000003E-2,0.10100000000000001]
[4,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:44.61"," 17:21:44.72",0.115,1E-3]
[5,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:44.72"," 17:21:44.85",0.125,1E-3]
[6,null,"内置PATTERN关闭","AA 06 27 00 2B CC","AB 05 0A DF 4E"," 17:21:44.85"," 17:21:44.94",9.2999999999999999E-2,6.0000000000000001E-3]
[1,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 17:21:50.93"," 17:21:51.00",7.0999999999999994E-2,5.9889999999999999]
[2,null,"老化模式关闭","AA 06 13 00 E2 9D","AB 05 0A DF 4E"," 17:21:51.01"," 17:21:51.13",0.121,4.0000000000000001E-3]
[3,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:51.23"," 17:21:51.31",8.2000000000000003E-2,0.10199999999999999]
[4,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:51.32"," 17:21:51.42",0.105,2E-3]
[5,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:51.42"," 17:21:51.54",0.113,2E-3]
[6,null,"内置PATTERN关闭","AA 06 27 00 2B CC","AB 05 0A DF 4E"," 17:21:51.54"," 17:21:51.65",0.105,5.0000000000000001E-3]
[1,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 17:21:57.64"," 17:21:57.71",7.2999999999999995E-2,5.9930000000000003]
[2,null,"老化模式关闭","AA 06 13 00 E2 9D","AB 05 0A DF 4E"," 17:21:57.72"," 17:21:57.84",0.127,3.0000000000000001E-3]
[3,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:57.94"," 17:21:58.04",9.4E-2,0.10199999999999999]
[4,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:58.04"," 17:21:58.14",0.10199999999999999,1E-3]
[5,null,"Project ID 查询","AA 06 84 00 63 E1","AB 05 0A DF 4E AB 07 85 16 37 B9 71"," 17:21:58.14"," 17:21:58.26",0.11600000000000001,1E-3]
[6,null,"内置PATTERN关闭","AA 06 27 00 2B CC","AB 05 0A DF 4E"," 17:21:58.26"," 17:21:58.37",0.104,4.0000000000000001E-3]
[1,null,"CA210开启输出","COM，1(+回车)","OK00"," 20:10:54.10"," 20:10:54.14",0.05,3745311054.0999999]
[2,null,"CA210关闭输出","COM，0(+回车)","OK00"," 20:10:54.15"," 20:10:54.20",5.0999999999999997E-2,1E-3]
[3,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:10:56.82"," 20:10:56.87",0.05,2.6230000000000002]
[4,null,"CA410显示模式(x，y，Lv)","MDS，0(+回车)","OK00"," 20:10:56.87"," 20:10:56.92",0.05,0]
[5,null,"CA410同步模式(UNIV)","SCS，3(+回车)","OK00"," 20:10:56.92"," 20:10:56.97",0.05,0]
[6,null,"CA410测量速度(自动)","FSC，2(+回车)","OK00"," 20:10:56.97"," 20:10:57.02",0.05,0]
[7,null,"CA410零校准","ZRC(+回车)","OK00"," 20:10:57.02"," 20:11:00.89",3.871,0]
[8,null,"CA410关闭输出","COM，0(+回车)","OK00"," 20:11:06.91"," 20:11:06.96",0.05,6.0220000000000002]
[9,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:12:27.19"," 20:12:27.24",5.0999999999999997E-2,80.228999999999999]
[10,null,"CA210开启输出","COM，1(+回车)","OK00"," 20:12:28.30"," 20:12:28.35",0.05,1.0609999999999999]
[11,null,"CA210关闭输出","COM，0(+回车)","OK00"," 20:12:28.35"," 20:12:28.40",0.05,0]
[12,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:12:31.32"," 20:12:31.37",5.0999999999999997E-2,2.9140000000000001]
[13,null,"CA410显示模式(x，y，Lv)","MDS，0(+回车)","OK00"," 20:12:31.37"," 20:12:31.42",0.05,0]
[14,null,"CA410同步模式(UNIV)","SCS，3(+回车)","OK00"," 20:12:31.42"," 20:12:31.47",0.05,0]
[15,null,"CA410测量速度(自动)","FSC，2(+回车)","OK00"," 20:12:31.47"," 20:12:31.52",5.0999999999999997E-2,0]
[16,null,"CA410零校准","ZRC(+回车)","OK00"," 20:12:31.52"," 20:12:35.39",3.8719999999999999,2E-3]
[17,null,"CA410关闭输出","COM，0(+回车)","OK00"," 20:12:41.42"," 20:12:41.47",5.0999999999999997E-2,6.0209999999999999]
[1,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:12:47.46"," 20:12:47.51",0.05,5.99]
[2,null,"CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:12:47.56"," 20:12:47.61",0.05,0.05]
[3,null,"CA410关闭输出","COM，0(+回车)",null," 20:12:47.61"," 20:12:47.76",0.15,0]
[4,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:12:48.86"," 20:12:48.88",0.02,1.1000000000000001]
[5,null,"HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:12:49.18"," 20:12:49.22",4.1000000000000002E-2,0.30099999999999999]
[6,null,"白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:12:49.22"," 20:12:49.32",0.1,0]
[7,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:12:49.43"," 20:12:49.48",5.0999999999999997E-2,0.112]
[8,null,"动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:12:49.58"," 20:12:49.61",3.1E-2,0.10100000000000001]
[9,null,"0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:12:49.61"," 20:12:49.65",4.1000000000000002E-2,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[10,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:12:49.65"," 20:12:49.71",5.0999999999999997E-2,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[11,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:12:49.71"," 20:12:49.75",4.1000000000000002E-2,0]
[12,null,"背光设置..1","AA 06 36 50 41 7B","AB 05 0A DF 4E"," 20:12:49.75"," 20:12:49.78",3.1E-2,0]
[13,null,"CA410读取数据","MES(+回车)","OK00，P1 310;330; 307"," 20:12:49.88"," 20:12:50.09",0.215,0.1]
[14,null,"背光设置..1","AA 06 36 39 BC F4","AB 05 0A DF 4E"," 20:12:50.09"," 20:12:50.13",4.2000000000000003E-2,1E-3]
[15,null,"CA410读取数据","MES(+回车)","OK00，P1 311;329; 253"," 20:12:50.24"," 20:12:50.35",0.113,0.1]
[16,null,"背光设置..1","AA 06 36 2A 9E A6","AB 05 0A DF 4E"," 20:12:50.35"," 20:12:50.38",3.3000000000000002E-2,1E-3]
[17,null,"CA410读取数据","MES(+回车)","OK00，P1 312;329; 199"," 20:12:50.48"," 20:12:50.60",0.114,0.1]
[18,null,"背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:12:50.60"," 20:12:50.63",0.03,1E-3]
[19,null,"CA410读取数据","MES(+回车)","OK00，P1 312;329; 221"," 20:12:50.73"," 20:12:50.84",0.113,0.1]
[20,null,"0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:12:50.84"," 20:12:50.96",0.114,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[21,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:12:50.96"," 20:12:51.00",0.05,0]
[22,null,"动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:12:51.11"," 20:12:51.14",3.1E-2,0.1]
[23,null,"普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:12:51.24"," 20:12:51.32",8.3000000000000004E-2,0.1]
[24,null,"CA410读取数据","MES(+回车)","OK00，P1 300;313; 193"," 20:12:51.42"," 20:12:51.53",0.114,0.10100000000000001]
[25,null,"寄存器红驱动赋值..1","AA 06 40 80 28 F9","AB 05 0A DF 4E"," 20:12:51.53"," 20:12:51.58",4.1000000000000002E-2,1E-3]
[26,null,"寄存器绿驱动赋值..1","AA 06 41 80 1B C8","AB 05 0A DF 4E"," 20:12:51.58"," 20:12:51.63",0.05,1E-3]
[27,null,"寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:12:51.63"," 20:12:51.68",5.0999999999999997E-2,0]
[28,null,"CA410读取数据","MES(+回车)","OK00，P1 319;343; 245"," 20:12:51.93"," 20:12:52.04",0.114,0.251]
[29,null,"寄存器绿驱动赋值..1","AA 06 41 79 65 FE","AB 05 0A DF 4E"," 20:12:52.04"," 20:12:52.09",0.05,1E-3]
[30,null,"CA410读取数据","MES(+回车)","OK00，P1 319;329; 225"," 20:12:52.19"," 20:12:52.31",0.113,0.1]
[31,null,"寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:12:52.31"," 20:12:52.34",0.03,1E-3]
[32,null,"CA410读取数据","MES(+回车)","OK00，P1 320;318; 211"," 20:12:52.44"," 20:12:52.55",0.114,0.1]
[33,null,"寄存器红驱动赋值..1","AA 06 40 79 56 CF","AB 05 0A DF 4E"," 20:12:52.55"," 20:12:52.59",4.2000000000000003E-2,1E-3]
[34,null,"CA410读取数据","MES(+回车)","OK00，P1 310;318; 205"," 20:12:52.70"," 20:12:52.81",0.113,0.10100000000000001]
[35,null,"寄存器红驱动赋值..1","AA 06 40 75 97 43","AB 05 0A DF 4E"," 20:12:52.81"," 20:12:52.86",5.2999999999999999E-2,1E-3]
[36,null,"CA410读取数据","MES(+回车)","OK00，P1 303;318; 201"," 20:12:52.96"," 20:12:53.08",0.11600000000000001,0.10100000000000001]
[37,null,"寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:12:53.08"," 20:12:53.12",4.1000000000000002E-2,0]
[38,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:12:53.22"," 20:12:53.33",0.113,0.1]
[39,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:12:53.34"," 20:12:53.54",0.20100000000000001,1E-3]
[40,null,"冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:12:53.57"," 20:12:53.65",8.1000000000000003E-2,0.03]
[41,null,"寄存器红驱动赋值..1","AA 06 40 00 B9 71","AB 05 0A DF 4E"," 20:12:53.65"," 20:12:53.69",0.04,0]
[42,null,"寄存器绿驱动赋值..1","AA 06 41 00 8A 40","AB 05 0A DF 4E"," 20:12:53.69"," 20:12:53.73",4.1000000000000002E-2,0]
[43,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:12:53.73"," 20:12:53.77",4.1000000000000002E-2,0]
[44,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:12:53.92"," 20:12:54.03",0.114,0.15]
[45,null,"寄存器绿驱动赋值..1","AA 06 41 F9 F4 76","AB 05 0A DF 4E"," 20:12:54.03"," 20:12:54.07",0.04,0]
[46,null,"CA410读取数据","MES(+回车)","OK00，P1 300;302; 180"," 20:12:54.17"," 20:12:54.29",0.113,0.10100000000000001]
[47,null,"寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:12:54.29"," 20:12:54.33",0.04,0]
[48,null,"CA410读取数据","MES(+回车)","OK00，P1 301;297; 175"," 20:12:54.43"," 20:12:54.54",0.113,0.1]
[49,null,"寄存器红驱动赋值..1","AA 06 40 FA F7 24","AB 05 0A DF 4E"," 20:12:54.54"," 20:12:54.59",5.1999999999999998E-2,3.0000000000000001E-3]
[50,null,"CA410读取数据","MES(+回车)","OK00，P1 290;296; 170"," 20:12:54.69"," 20:12:54.81",0.114,0.1]
[51,null,"寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:12:54.81"," 20:12:54.84",0.03,0]
[52,null,"CA410读取数据","MES(+回车)","OK00，P1 285;296; 167"," 20:12:54.94"," 20:12:55.05",0.115,0.1]
[53,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:12:55.06"," 20:12:55.25",0.191,1E-3]
[54,null,"暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:12:55.28"," 20:12:55.35",7.0000000000000007E-2,0.03]
[55,null,"寄存器红驱动赋值..1","AA 06 40 00 B9 71","AB 05 0A DF 4E"," 20:12:55.35"," 20:12:55.39",0.04,1E-3]
[56,null,"寄存器绿驱动赋值..1","AA 06 41 00 8A 40","AB 05 0A DF 4E"," 20:12:55.40"," 20:12:55.44",0.04,1.0999999999999999E-2]
[57,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:12:55.44"," 20:12:55.48",4.1000000000000002E-2,0]
[58,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:12:55.63"," 20:12:55.74",0.114,0.15]
[59,null,"寄存器红驱动赋值..1","AA 06 40 05 E9 D4","AB 05 0A DF 4E"," 20:12:55.74"," 20:12:55.79",4.2000000000000003E-2,1E-3]
[60,null,"CA410读取数据","MES(+回车)","OK00，P1 308;318; 203"," 20:12:55.89"," 20:12:56.00",0.115,0.1]
[61,null,"寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:12:56.00"," 20:12:56.04",4.1000000000000002E-2,1E-3]
[62,null,"CA410读取数据","MES(+回车)","OK00，P1 311;318; 205"," 20:12:56.14"," 20:12:56.26",0.11600000000000001,0.1]
[63,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:12:56.26"," 20:12:56.31",5.1999999999999998E-2,1E-3]
[64,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 217"," 20:12:56.41"," 20:12:56.53",0.114,0.1]
[65,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:12:56.53"," 20:12:56.73",0.20399999999999999,0]
[66,null,"Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:12:56.76"," 20:12:56.84",8.2000000000000003E-2,0.03]
[67,null,"寄存器红驱动赋值..1","AA 06 40 00 B9 71","AB 05 0A DF 4E"," 20:12:56.84"," 20:12:56.87",3.2000000000000001E-2,0]
[68,null,"寄存器绿驱动赋值..1","AA 06 41 00 8A 40","AB 05 0A DF 4E"," 20:12:56.87"," 20:12:56.91",3.2000000000000001E-2,0]
[69,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:12:56.91"," 20:12:56.94",3.1E-2,1E-3]
[70,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:12:57.09"," 20:12:57.20",0.113,0.151]
[71,null,"寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:12:57.20"," 20:12:57.24",4.1000000000000002E-2,0]
[72,null,"CA410读取数据","MES(+回车)","OK00，P1 311;318; 205"," 20:12:57.34"," 20:12:57.46",0.112,0.10100000000000001]
[73,null,"寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:12:57.46"," 20:12:57.49",3.2000000000000001E-2,0]
[74,null,"CA410读取数据","MES(+回车)","OK00，P1 321;318; 211"," 20:12:57.59"," 20:12:57.70",0.114,0.1]
[75,null,"寄存器绿驱动赋值..1","AA 06 41 07 FA A7","AB 05 0A DF 4E"," 20:12:57.70"," 20:12:57.74",4.1000000000000002E-2,1E-3]
[76,null,"CA410读取数据","MES(+回车)","OK00，P1 319;333; 231"," 20:12:57.84"," 20:12:57.96",0.113,0.1]
[77,null,"寄存器绿驱动赋值..1","AA 06 41 0C 4B CC","AB 05 0A DF 4E"," 20:12:57.96"," 20:12:57.99",3.2000000000000001E-2,0]
[78,null,"CA410读取数据","MES(+回车)","OK00，P1 319;343; 245"," 20:12:58.09"," 20:12:58.21",0.11600000000000001,0.10100000000000001]
[79,null,"寄存器蓝驱动赋值..1","AA 06 42 F9 A1 25","AB 05 0A DF 4E"," 20:12:58.21"," 20:12:58.24",0.03,0]
[80,null,"CA410读取数据","MES(+回车)","OK00，P1 329;358; 241"," 20:12:58.34"," 20:12:58.45",0.114,0.1]
[81,null,"寄存器蓝驱动赋值..1","AA 06 42 F3 00 6F","AB 05 0A DF 4E"," 20:12:58.45"," 20:12:58.49",4.1000000000000002E-2,1E-3]
[82,null,"CA410读取数据","MES(+回车)","OK00，P1 337;370; 238"," 20:12:58.59"," 20:12:58.71",0.11899999999999999,0.10100000000000001]
[83,null,"寄存器绿驱动赋值..1","AA 06 41 08 0B 48","AB 05 0A DF 4E"," 20:12:58.71"," 20:12:58.75",0.04,2E-3]
[84,null,"CA410读取数据","MES(+回车)","OK00，P1 339;363; 227"," 20:12:58.86"," 20:12:58.97",0.114,0.10100000000000001]
[85,null,"寄存器绿驱动赋值..1","AA 06 41 06 EA 86","AB 05 0A DF 4E"," 20:12:58.97"," 20:12:59.01",0.04,1E-3]
[86,null,"CA410读取数据","MES(+回车)","OK00，P1 339;359; 221"," 20:12:59.11"," 20:12:59.22",0.113,0.10100000000000001]
[87,null,"寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:12:59.22"," 20:12:59.26",3.2000000000000001E-2,1E-3]
[88,null,"CA410读取数据","MES(+回车)","OK00，P1 344;365; 220"," 20:12:59.36"," 20:12:59.47",0.115,0.1]
[89,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:12:59.47"," 20:12:59.50",3.1E-2,0]
[90,null,"CA410读取数据","MES(+回车)","OK00，P1 344;361; 214"," 20:12:59.60"," 20:12:59.72",0.114,0.10100000000000001]
[91,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:12:59.72"," 20:12:59.91",0.19500000000000001,0]
[92,null,"SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:12:59.94"," 20:13:00.02",7.2999999999999995E-2,0.03]
[93,null,"寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:13:00.12"," 20:13:00.16",4.2000000000000003E-2,0.10100000000000001]
[94,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:13:00.16"," 20:13:00.19",0.03,0]
[95,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:13:00.19"," 20:13:00.22",0.03,0]
[96,null,"背光设置..1","AA 06 36 28 BE E4","AB 05 0A DF 4E"," 20:13:00.22"," 20:13:00.25",3.2000000000000001E-2,0]
[97,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 150"," 20:13:00.35"," 20:13:00.47",0.11700000000000001,0.1]
[98,null,"背光设置..1","AA 06 36 1E E8 71","AB 05 0A DF 4E"," 20:13:00.47"," 20:13:00.50",0.03,0]
[99,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 123"," 20:13:00.60"," 20:13:00.71",0.114,0.10100000000000001]
[100,null,"背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:13:00.71"," 20:13:00.74",0.03,1E-3]
[101,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 115"," 20:13:00.84"," 20:13:00.96",0.113,0.1]
[102,null,"背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:13:00.96"," 20:13:00.98",2.1999999999999999E-2,1E-3]
[103,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 112"," 20:13:01.08"," 20:13:01.19",0.113,0.1]
[104,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 112"," 20:13:01.34"," 20:13:01.46",0.113,0.152]
[105,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:13:01.46"," 20:13:01.93",0.47399999999999998,1E-3]
[106,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:01.96"," 20:13:02.02",5.1999999999999998E-2,3.1E-2]
[107,null,"背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:13:02.07"," 20:13:02.10",3.1E-2,5.0999999999999997E-2]
[108,null,"对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:13:02.20"," 20:13:02.29",0.09,0.1]
[109,null,"CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:13:02.49"," 20:13:02.60",0.113,0.2]
[110,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:02.60"," 20:13:02.65",5.1999999999999998E-2,1E-3]
[111,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 217"," 20:13:02.86"," 20:13:02.97",0.115,0.20200000000000001]
[112,null,"CA410关闭输出","COM，0(+回车)","OK00"," 20:13:02.97"," 20:13:03.02",0.05,1E-3]
[1,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:13:05.63"," 20:13:05.68",5.0999999999999997E-2,2.609]
[2,null,"CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:13:05.73"," 20:13:05.78",0.05,0.05]
[3,null,"CA410关闭输出","COM，0(+回车)",null," 20:13:05.78"," 20:13:05.93",0.151,0]
[4,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:13:07.03"," 20:13:07.06",3.1E-2,1.1000000000000001]
[5,null,"HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:13:07.36"," 20:13:07.40",0.04,0.3]
[6,null,"白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:13:07.40"," 20:13:07.50",9.1999999999999998E-2,1E-3]
[7,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:07.60"," 20:13:07.65",0.05,0.1]
[8,null,"动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:13:07.75"," 20:13:07.78",0.03,0.1]
[9,null,"0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:13:07.78"," 20:13:07.82",0.04,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[10,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:13:07.82"," 20:13:07.87",0.05,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[11,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:07.87"," 20:13:07.92",5.0999999999999997E-2,0]
[12,null,"背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:13:07.92"," 20:13:07.95",3.3000000000000002E-2,0]
[13,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 217"," 20:13:08.05"," 20:13:08.17",0.115,0.1]
[14,null,"背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:13:08.17"," 20:13:08.20",3.1E-2,1E-3]
[15,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 220"," 20:13:08.30"," 20:13:08.41",0.113,0.1]
[16,null,"0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:13:08.41"," 20:13:08.51",0.10199999999999999,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[17,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:08.51"," 20:13:08.56",5.0999999999999997E-2,0]
[18,null,"动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:13:08.66"," 20:13:08.70",3.1E-2,0.1]
[19,null,"普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:13:08.80"," 20:13:08.89",9.2999999999999999E-2,0.1]
[20,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 202"," 20:13:08.99"," 20:13:09.10",0.112,0.1]
[21,null,"寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:13:09.10"," 20:13:09.14",4.2000000000000003E-2,1E-3]
[22,null,"寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:13:09.14"," 20:13:09.19",0.05,0]
[23,null,"寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:13:09.19"," 20:13:09.25",5.1999999999999998E-2,0]
[24,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 202"," 20:13:09.50"," 20:13:09.62",0.11700000000000001,0.253]
[25,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:13:09.62"," 20:13:09.75",0.13,1E-3]
[26,null,"冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:13:09.78"," 20:13:09.86",8.1000000000000003E-2,3.2000000000000001E-2]
[27,null,"寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:13:09.86"," 20:13:09.89",0.03,0]
[28,null,"寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:13:09.89"," 20:13:09.92",3.1E-2,3.0000000000000001E-3]
[29,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:13:09.92"," 20:13:09.96",3.1E-2,0]
[30,null,"CA410读取数据","MES(+回车)","OK00，P1 285;296; 170"," 20:13:10.11"," 20:13:10.22",0.114,0.151]
[31,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:13:10.22"," 20:13:10.35",0.13300000000000001,1E-3]
[32,null,"暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:13:10.38"," 20:13:10.47",8.3000000000000004E-2,0.03]
[33,null,"寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:13:10.47"," 20:13:10.51",4.2000000000000003E-2,1E-3]
[34,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:13:10.51"," 20:13:10.56",5.0999999999999997E-2,0]
[35,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:13:10.56"," 20:13:10.61",5.1999999999999998E-2,0]
[36,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 220"," 20:13:10.76"," 20:13:10.88",0.11700000000000001,0.151]
[37,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:13:10.88"," 20:13:11.01",0.13200000000000001,1E-3]
[38,null,"Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:13:11.05"," 20:13:11.13",8.3000000000000004E-2,3.3000000000000002E-2]
[39,null,"寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:13:11.13"," 20:13:11.17",4.2000000000000003E-2,0]
[40,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:13:11.17"," 20:13:11.21",0.04,0]
[41,null,"寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:13:11.21"," 20:13:11.26",4.3999999999999997E-2,0]
[42,null,"CA410读取数据","MES(+回车)","OK00，P1 344;361; 218"," 20:13:11.41"," 20:13:11.52",0.115,0.151]
[43,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:13:11.52"," 20:13:11.66",0.14199999999999999,1E-3]
[44,null,"SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:13:11.70"," 20:13:11.78",8.1000000000000003E-2,3.1E-2]
[45,null,"寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:13:11.88"," 20:13:11.92",4.1000000000000002E-2,0.10199999999999999]
[46,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:13:11.92"," 20:13:11.95",3.3000000000000002E-2,0]
[47,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:13:11.96"," 20:13:11.99",3.2000000000000001E-2,3.0000000000000001E-3]
[48,null,"背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:13:11.99"," 20:13:12.01",2.1999999999999999E-2,1E-3]
[49,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 113"," 20:13:12.11"," 20:13:12.23",0.115,0.10100000000000001]
[50,null,"背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:13:12.23"," 20:13:12.27",0.04,0]
[51,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 116"," 20:13:12.37"," 20:13:12.48",0.113,0.1]
[52,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 116"," 20:13:12.63"," 20:13:12.75",0.114,0.153]
[53,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:13:12.75"," 20:13:13.08",0.33600000000000002,1E-3]
[54,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:13.11"," 20:13:13.16",5.0999999999999997E-2,0.03]
[55,null,"背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:13:13.21"," 20:13:13.25",0.03,0.05]
[56,null,"对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:13:13.34"," 20:13:13.44",9.1999999999999998E-2,0.1]
[57,null,"CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:13:13.64"," 20:13:13.75",0.113,0.2]
[58,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:13.75"," 20:13:13.80",5.2999999999999999E-2,1E-3]
[59,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 220"," 20:13:14.01"," 20:13:14.12",0.115,0.20300000000000001]
[60,null,"CA410关闭输出","COM，0(+回车)","OK00"," 20:13:14.12"," 20:13:14.17",0.05,1E-3]
[1,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:13:15.75"," 20:13:15.80",0.05,1.5740000000000001]
[2,null,"CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:13:15.85"," 20:13:15.90",5.0999999999999997E-2,5.0999999999999997E-2]
[3,null,"CA410关闭输出","COM，0(+回车)",null," 20:13:15.90"," 20:13:16.05",0.152,1E-3]
[4,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:13:17.15"," 20:13:17.18",0.03,1.1000000000000001]
[5,null,"HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:13:17.48"," 20:13:17.51",0.03,0.30199999999999999]
[6,null,"HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:13:17.52"," 20:13:17.56",4.1000000000000002E-2,2E-3]
[7,null,"白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:13:17.56"," 20:13:17.65",9.0999999999999998E-2,0]
[8,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:17.75"," 20:13:17.80",5.0999999999999997E-2,0.1]
[9,null,"动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:13:17.90"," 20:13:17.93",0.03,0.105]
[10,null,"0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:13:17.93"," 20:13:17.97",3.3000000000000002E-2,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[11,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:13:17.97"," 20:13:18.02",0.05,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[12,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:18.02"," 20:13:18.06",4.2999999999999997E-2,4.0000000000000001E-3]
[13,null,"背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:13:18.07"," 20:13:18.10",3.1E-2,2E-3]
[14,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 220"," 20:13:18.20"," 20:13:18.31",0.113,0.1]
[15,null,"背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:13:18.31"," 20:13:18.34",3.2000000000000001E-2,1E-3]
[16,null,"CA410读取数据","MES(+回车)","OK00，P1 311;327; 216"," 20:13:18.44"," 20:13:18.56",0.114,0.1]
[17,null,"0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:13:18.56"," 20:13:18.67",0.112,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[18,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:18.67"," 20:13:18.72",5.0999999999999997E-2,0]
[19,null,"动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:13:18.82"," 20:13:18.84",2.1000000000000001E-2,0.1]
[20,null,"普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:13:18.94"," 20:13:19.02",8.1000000000000003E-2,0.10100000000000001]
[21,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:13:19.12"," 20:13:19.24",0.114,0.1]
[22,null,"寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:13:19.24"," 20:13:19.27",3.2000000000000001E-2,2E-3]
[23,null,"寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:13:19.27"," 20:13:19.30",3.1E-2,0]
[24,null,"寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:13:19.30"," 20:13:19.34",4.2000000000000003E-2,0]
[25,null,"CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:13:19.59"," 20:13:19.71",0.114,0.25]
[26,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:13:19.71"," 20:13:19.85",0.14299999999999999,1E-3]
[27,null,"冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:13:19.88"," 20:13:19.97",8.3000000000000004E-2,3.1E-2]
[28,null,"寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:13:19.97"," 20:13:20.01",4.2000000000000003E-2,0]
[29,null,"寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:13:20.01"," 20:13:20.06",5.1999999999999998E-2,0]
[30,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:13:20.06"," 20:13:20.11",0.05,1E-3]
[31,null,"CA410读取数据","MES(+回车)","OK00，P1 285;296; 167"," 20:13:20.26"," 20:13:20.38",0.11600000000000001,0.15]
[32,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:13:20.38"," 20:13:20.52",0.14000000000000001,1E-3]
[33,null,"暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:13:20.55"," 20:13:20.63",8.2000000000000003E-2,0.03]
[34,null,"寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:13:20.63"," 20:13:20.67",4.1000000000000002E-2,1E-3]
[35,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:13:20.67"," 20:13:20.70",3.1E-2,0]
[36,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:13:20.70"," 20:13:20.75",4.2000000000000003E-2,0]
[37,null,"CA410读取数据","MES(+回车)","OK00，P1 310;327; 216"," 20:13:20.90"," 20:13:21.01",0.113,0.151]
[38,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:13:21.01"," 20:13:21.15",0.14199999999999999,2E-3]
[39,null,"Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:13:21.18"," 20:13:21.27",8.1000000000000003E-2,3.1E-2]
[40,null,"寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:13:21.27"," 20:13:21.31",4.2000000000000003E-2,0]
[41,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:13:21.31"," 20:13:21.34",3.1E-2,0]
[42,null,"寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:13:21.34"," 20:13:21.37",3.1E-2,0]
[43,null,"CA410读取数据","MES(+回车)","OK00，P1 345;361; 214"," 20:13:21.52"," 20:13:21.63",0.112,0.15]
[44,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:13:21.63"," 20:13:21.76",0.13200000000000001,0]
[45,null,"SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:13:21.80"," 20:13:21.88",8.2000000000000003E-2,3.2000000000000001E-2]
[46,null,"寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:13:21.98"," 20:13:22.03",0.05,0.1]
[47,null,"寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:13:22.03"," 20:13:22.08",5.0999999999999997E-2,0]
[48,null,"寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:13:22.08"," 20:13:22.12",4.2000000000000003E-2,1E-3]
[49,null,"背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:13:22.12"," 20:13:22.14",0.02,0]
[50,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 114"," 20:13:22.25"," 20:13:22.36",0.115,0.10299999999999999]
[51,null,"背光设置..1","AA 06 36 1C C8 33","AB 05 0A DF 4E"," 20:13:22.36"," 20:13:22.39",3.2000000000000001E-2,2E-3]
[52,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 117"," 20:13:22.50"," 20:13:22.61",0.115,0.10100000000000001]
[53,null,"CA410读取数据","MES(+回车)","OK00，P1 312;327; 117"," 20:13:22.76"," 20:13:22.88",0.11700000000000001,0.153]
[54,null,"RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:13:22.88"," 20:13:23.22",0.34399999999999997,1E-3]
[55,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:23.25"," 20:13:23.30",4.2000000000000003E-2,0.03]
[56,null,"背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:13:23.35"," 20:13:23.38",3.1E-2,5.0999999999999997E-2]
[57,null,"对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:13:23.48"," 20:13:23.57",9.1999999999999998E-2,0.1]
[58,null,"CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:13:23.77"," 20:13:23.89",0.114,0.20300000000000001]
[59,null,"标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:13:23.89"," 20:13:23.94",0.05,1E-3]
[60,null,"CA410读取数据","MES(+回车)","OK00，P1 311;327; 216"," 20:13:24.14"," 20:13:24.25",0.113,0.20200000000000001]
[61,null,"CA410关闭输出","COM，0(+回车)","OK00"," 20:13:24.25"," 20:13:24.30",0.05,0]
[1,null,"CA410开启输出","COM，1(+回车)","OK00"," 20:14:09.59"," 20:14:09.64",0.05,45.286000000000001]
[2,null,"CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:14:09.69"," 20:14:09.74",5.0999999999999997E-2,0.05]
[3,null,"CA410关闭输出","COM，0(+回车)",null," 20:14:09.74"," 20:14:09.89",0.151,0]
[4,null,"进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:14:10.99"," 20:14:11.01",0.02,1.1000000000000001]
[5,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:14:11.31"," 20:14:11.37",0.06,0.3]
[6,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:14:11.37"," 20:14:11.42",5.0999999999999997E-2,0]
[7,null,"电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:14:11.42"," 20:14:11.47",5.1999999999999998E-2,0]
[8,null,"CA410关闭输出","COM，0(+回车)","OK00"," 20:14:11.49"," 20:14:11.54",5.0999999999999997E-2,1.4E-2]
[1,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:14:27.59"," 20:14:27.64",0.05,16.047999999999998]
[2,"CMIGMCFXEU214600018","CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:14:27.69"," 20:14:27.74",0.05,0.05]
[3,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)",null," 20:14:27.74"," 20:14:27.89",0.15,0]
[4,"CMIGMCFXEU214600018","进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:14:28.99"," 20:14:29.01",0.02,1.101]
[5,"CMIGMCFXEU214600018","电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:14:29.31"," 20:14:29.36",0.05,0.3]
[6,"CMIGMCFXEU214600018","条形码写入_22","AA 18 71 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 32 77","AB 05 0A DF 4E"," 20:14:29.36"," 20:14:31.91",2.5529999999999999,0]
[7,"CMIGMCFXEU214600018","HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:14:31.91"," 20:14:31.96",4.4999999999999998E-2,0]
[8,"CMIGMCFXEU214600018","HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:14:31.96"," 20:14:31.99",0.03,0]
[9,"CMIGMCFXEU214600018","白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:14:31.99"," 20:14:32.08",9.0999999999999998E-2,0]
[10,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:32.18"," 20:14:32.24",0.06,0.1]
[11,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:14:32.34"," 20:14:32.37",0.03,0.1]
[12,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:14:32.37"," 20:14:32.40",3.2000000000000001E-2,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[13,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:14:32.40"," 20:14:32.45",5.0999999999999997E-2,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[14,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:32.45"," 20:14:32.50",0.05,1E-3]
[15,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:14:32.50"," 20:14:32.53",0.03,0]
[16,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 216"," 20:14:32.63"," 20:14:32.75",0.112,0.10299999999999999]
[17,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:14:32.75"," 20:14:32.78",3.1E-2,0]
[18,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 220"," 20:14:32.88"," 20:14:32.99",0.114,0.1]
[19,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:14:32.99"," 20:14:33.11",0.113,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[20,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:33.11"," 20:14:33.15",4.2000000000000003E-2,0]
[21,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:14:33.25"," 20:14:33.28",3.1E-2,0.10100000000000001]
[22,"CMIGMCFXEU214600018","普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:14:33.38"," 20:14:33.47",0.09,0.1]
[23,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;318; 202"," 20:14:33.57"," 20:14:33.68",0.113,0.1]
[24,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:14:33.68"," 20:14:33.72",4.1000000000000002E-2,1E-3]
[25,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:14:33.75"," 20:14:33.79",4.2000000000000003E-2,0.02]
[26,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:14:33.79"," 20:14:33.82",3.1E-2,2E-3]
[27,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;318; 202"," 20:14:34.07"," 20:14:34.18",0.115,0.25]
[28,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:14:34.18"," 20:14:34.31",0.13,0]
[29,"CMIGMCFXEU214600018","冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:14:34.34"," 20:14:34.43",8.1000000000000003E-2,0.03]
[30,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:14:34.43"," 20:14:34.46",0.03,0]
[31,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:14:34.46"," 20:14:34.49",3.2000000000000001E-2,2E-3]
[32,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:14:34.49"," 20:14:34.53",0.04,0]
[33,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 286;296; 170"," 20:14:34.68"," 20:14:34.79",0.112,0.152]
[34,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:14:34.80"," 20:14:34.94",0.14099999999999999,1E-3]
[35,"CMIGMCFXEU214600018","暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:14:34.97"," 20:14:35.05",8.1000000000000003E-2,3.1E-2]
[36,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:14:35.05"," 20:14:35.09",0.04,0]
[37,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:14:35.09"," 20:14:35.13",4.2000000000000003E-2,0]
[38,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:14:35.13"," 20:14:35.17",4.1000000000000002E-2,0]
[39,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 220"," 20:14:35.32"," 20:14:35.44",0.115,0.151]
[40,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:14:35.44"," 20:14:35.57",0.13,0]
[41,"CMIGMCFXEU214600018","Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:14:35.60"," 20:14:35.68",8.1000000000000003E-2,0.03]
[42,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:14:35.68"," 20:14:35.73",0.05,0]
[43,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:14:35.73"," 20:14:35.78",5.0999999999999997E-2,0]
[44,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:14:35.78"," 20:14:35.82",4.1000000000000002E-2,0]
[45,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 345;361; 218"," 20:14:35.97"," 20:14:36.09",0.114,0.151]
[46,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:14:36.09"," 20:14:36.22",0.13200000000000001,0]
[47,"CMIGMCFXEU214600018","SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:14:36.25"," 20:14:36.33",8.1000000000000003E-2,0.03]
[48,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:14:36.43"," 20:14:36.48",0.05,0.1]
[49,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:14:36.48"," 20:14:36.53",5.1999999999999998E-2,0]
[50,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:14:36.53"," 20:14:36.57",4.2000000000000003E-2,0]
[51,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1C C8 33","AB 05 0A DF 4E"," 20:14:36.57"," 20:14:36.59",2.1000000000000001E-2,0]
[52,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 312;326; 119"," 20:14:36.69"," 20:14:36.81",0.115,0.1]
[53,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:14:36.81"," 20:14:36.83",2.1000000000000001E-2,1E-3]
[54,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 312;326; 116"," 20:14:36.93"," 20:14:37.05",0.115,0.1]
[55,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:14:37.05"," 20:14:37.08",0.03,1E-3]
[56,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 312;327; 113"," 20:14:37.18"," 20:14:37.29",0.115,0.1]
[57,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 312;327; 113"," 20:14:37.44"," 20:14:37.56",0.115,0.151]
[58,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:14:37.56"," 20:14:37.92",0.36599999999999999,1E-3]
[59,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:37.95"," 20:14:38.00",5.0999999999999997E-2,0.03]
[60,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:14:38.06"," 20:14:38.09",0.03,0.05]
[61,"CMIGMCFXEU214600018","对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:14:38.18"," 20:14:38.28",9.2999999999999999E-2,0.1]
[62,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:14:38.48"," 20:14:38.59",0.115,0.20200000000000001]
[63,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:38.60"," 20:14:38.65",5.3999999999999999E-2,1E-3]
[64,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 220"," 20:14:38.85"," 20:14:38.97",0.115,0.20200000000000001]
[65,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)","OK00"," 20:14:38.97"," 20:14:39.02",0.05,1E-3]
[66,"CMIGMCFXEU214600018","网络参数查询..1","AA 06 BE 03 B9 DC","AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0"," 20:14:39.02"," 20:14:39.07",5.0999999999999997E-2,0,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[1,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:14:44.56"," 20:14:44.61",5.0999999999999997E-2,5.4909999999999997,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[2,"CMIGMCFXEU214600018","CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:14:44.66"," 20:14:44.71",0.05,5.0999999999999997E-2,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[3,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)",null," 20:14:44.71"," 20:14:44.86",0.15,0]
[4,"CMIGMCFXEU214600018","进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:14:45.96"," 20:14:45.99",3.1E-2,1.1000000000000001]
[5,"CMIGMCFXEU214600018","电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:14:46.29"," 20:14:46.34",4.1000000000000002E-2,0.30099999999999999]
[6,"CMIGMCFXEU214600018","条形码写入_22","AA 18 71 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 32 77","AB 05 0A DF 4E"," 20:14:46.34"," 20:14:48.75",2.4129999999999998,0]
[7,"CMIGMCFXEU214600018","HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:14:48.75"," 20:14:48.79",0.04,0]
[8,"CMIGMCFXEU214600018","HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:14:48.79"," 20:14:48.82",0.03,0]
[9,"CMIGMCFXEU214600018","白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:14:48.82"," 20:14:48.92",0.1,0]
[10,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:49.02"," 20:14:49.07",5.0999999999999997E-2,0.1]
[11,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:14:49.17"," 20:14:49.20",0.03,0.1]
[12,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:14:49.20"," 20:14:49.24",0.04,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[13,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:14:49.24"," 20:14:49.29",5.0999999999999997E-2,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[14,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:49.29"," 20:14:49.33",4.2000000000000003E-2,1E-3]
[15,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:14:49.33"," 20:14:49.37",3.3000000000000002E-2,0]
[16,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 220"," 20:14:49.47"," 20:14:49.58",0.114,0.10299999999999999]
[17,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:14:49.58"," 20:14:49.62",3.3000000000000002E-2,0]
[18,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 217"," 20:14:49.72"," 20:14:49.83",0.114,0.10100000000000001]
[19,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:14:49.83"," 20:14:49.94",0.107,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[20,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:49.94"," 20:14:49.98",4.2000000000000003E-2,1E-3]
[21,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:14:50.08"," 20:14:50.11",0.03,0.10199999999999999]
[22,"CMIGMCFXEU214600018","普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:14:50.22"," 20:14:50.31",9.2999999999999999E-2,0.10100000000000001]
[23,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:14:50.41"," 20:14:50.52",0.112,0.1]
[24,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:14:50.52"," 20:14:50.56",4.1000000000000002E-2,1E-3]
[25,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:14:50.56"," 20:14:50.61",5.0999999999999997E-2,0]
[26,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:14:50.61"," 20:14:50.66",4.2000000000000003E-2,0]
[27,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;318; 199"," 20:14:50.91"," 20:14:51.02",0.113,0.251]
[28,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:14:51.02"," 20:14:51.15",0.13,1E-3]
[29,"CMIGMCFXEU214600018","冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:14:51.18"," 20:14:51.27",8.5000000000000006E-2,3.1E-2]
[30,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:14:51.27"," 20:14:51.31",4.2000000000000003E-2,0]
[31,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:14:51.31"," 20:14:51.34",0.03,0]
[32,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:14:51.34"," 20:14:51.37",3.3000000000000002E-2,2E-3]
[33,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 286;296; 167"," 20:14:51.52"," 20:14:51.64",0.113,0.151]
[34,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:14:51.64"," 20:14:51.77",0.13,1E-3]
[35,"CMIGMCFXEU214600018","暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:14:51.80"," 20:14:51.88",0.08,0.03]
[36,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:14:51.88"," 20:14:51.93",5.0999999999999997E-2,0]
[37,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:14:51.93"," 20:14:51.97",4.1000000000000002E-2,0]
[38,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:14:51.97"," 20:14:52.01",4.2000000000000003E-2,0]
[39,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 217"," 20:14:52.16"," 20:14:52.28",0.114,0.152]
[40,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:14:52.28"," 20:14:52.42",0.14000000000000001,0]
[41,"CMIGMCFXEU214600018","Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:14:52.45"," 20:14:52.53",0.08,3.1E-2]
[42,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:14:52.53"," 20:14:52.57",4.1000000000000002E-2,0]
[43,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:14:52.57"," 20:14:52.61",0.04,0]
[44,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:14:52.62"," 20:14:52.66",4.2000000000000003E-2,1.0999999999999999E-2]
[45,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 345;361; 214"," 20:14:52.81"," 20:14:52.93",0.114,0.15]
[46,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:14:52.93"," 20:14:53.07",0.14000000000000001,0]
[47,"CMIGMCFXEU214600018","SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:14:53.10"," 20:14:53.18",8.2000000000000003E-2,3.2000000000000001E-2]
[48,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:14:53.28"," 20:14:53.32",4.2000000000000003E-2,0.1]
[49,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:14:53.33"," 20:14:53.37",0.04,1.2E-2]
[50,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:14:53.37"," 20:14:53.41",0.03,0]
[51,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:14:53.41"," 20:14:53.43",2.1000000000000001E-2,0]
[52,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 112"," 20:14:53.53"," 20:14:53.64",0.114,0.10100000000000001]
[53,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:14:53.64"," 20:14:53.66",2.3E-2,0]
[54,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 312;326; 115"," 20:14:53.76"," 20:14:53.88",0.11700000000000001,0.1]
[55,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 312;326; 115"," 20:14:54.03"," 20:14:54.15",0.114,0.152]
[56,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:14:54.15"," 20:14:54.51",0.36699999999999999,1E-3]
[57,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:54.55"," 20:14:54.60",5.0999999999999997E-2,3.2000000000000001E-2]
[58,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:14:54.65"," 20:14:54.68",0.03,0.05]
[59,"CMIGMCFXEU214600018","对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:14:54.78"," 20:14:54.87",9.1999999999999998E-2,0.1]
[60,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:14:55.07"," 20:14:55.18",0.112,0.2]
[61,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:14:55.18"," 20:14:55.23",0.05,1E-3]
[62,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:14:55.44"," 20:14:55.55",0.115,0.20300000000000001]
[63,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)","OK00"," 20:14:55.55"," 20:14:55.60",0.05,1E-3]
[64,"CMIGMCFXEU214600018","网络参数查询..1","AA 06 BE 03 B9 DC","AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0"," 20:14:55.60"," 20:14:55.65",5.0999999999999997E-2,0,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[1,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:01.13"," 20:15:01.18",0.05,5.476,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[2,"CMIGMCFXEU214600018","CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:15:01.23"," 20:15:01.28",0.05,5.0999999999999997E-2,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[3,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)",null," 20:15:01.28"," 20:15:01.43",0.15,3.0000000000000001E-3]
[4,"CMIGMCFXEU214600018","进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:15:02.54"," 20:15:02.57",3.1E-2,1.1020000000000001]
[5,"CMIGMCFXEU214600018","电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:15:02.87"," 20:15:02.92",0.05,0.30099999999999999]
[6,"CMIGMCFXEU214600018","条形码写入_22","AA 18 71 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 32 77","AB 05 0A DF 4E"," 20:15:02.92"," 20:15:05.33",2.415,0]
[7,"CMIGMCFXEU214600018","HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:15:05.33"," 20:15:05.37",4.1000000000000002E-2,1E-3]
[8,"CMIGMCFXEU214600018","HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:15:05.37"," 20:15:05.41",3.2000000000000001E-2,1E-3]
[9,"CMIGMCFXEU214600018","白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:15:05.41"," 20:15:05.50",9.0999999999999998E-2,0]
[10,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:05.60"," 20:15:05.65",0.05,0.1]
[11,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:05.75"," 20:15:05.78",3.1E-2,0.1]
[12,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:15:05.78"," 20:15:05.82",0.04,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[13,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:05.82"," 20:15:05.87",0.05,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[14,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:05.87"," 20:15:05.92",0.05,0]
[15,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:15:05.92"," 20:15:05.95",0.03,1E-3]
[16,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:15:06.05"," 20:15:06.17",0.114,0.10100000000000001]
[17,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:15:06.17"," 20:15:06.20",3.1E-2,1E-3]
[18,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 220"," 20:15:06.30"," 20:15:06.41",0.113,0.10100000000000001]
[19,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:15:06.41"," 20:15:06.51",0.10299999999999999,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[20,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:06.52"," 20:15:06.57",0.05,1E-3]
[21,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:06.67"," 20:15:06.70",0.03,0.1]
[22,"CMIGMCFXEU214600018","普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:15:06.80"," 20:15:06.89",9.1999999999999998E-2,0.1]
[23,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;318; 202"," 20:15:06.99"," 20:15:07.10",0.112,0.1]
[24,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:15:07.10"," 20:15:07.14",4.2000000000000003E-2,2E-3]
[25,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:15:07.14"," 20:15:07.19",0.05,0]
[26,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:15:07.19"," 20:15:07.25",5.2999999999999999E-2,0]
[27,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;318; 202"," 20:15:07.50"," 20:15:07.61",0.113,0.25]
[28,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:15:07.61"," 20:15:07.75",0.14099999999999999,1E-3]
[29,"CMIGMCFXEU214600018","冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:15:07.78"," 20:15:07.86",8.2000000000000003E-2,0.03]
[30,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:15:07.87"," 20:15:07.91",4.1000000000000002E-2,1E-3]
[31,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:15:07.91"," 20:15:07.94",3.2000000000000001E-2,0]
[32,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:07.94"," 20:15:07.98",0.04,0]
[33,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 286;296; 170"," 20:15:08.13"," 20:15:08.24",0.112,0.15]
[34,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:15:08.24"," 20:15:08.38",0.14199999999999999,1E-3]
[35,"CMIGMCFXEU214600018","暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:15:08.41"," 20:15:08.50",8.4000000000000005E-2,3.1E-2]
[36,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:08.50"," 20:15:08.54",0.04,0]
[37,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:08.54"," 20:15:08.58",0.04,1E-3]
[38,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:08.58"," 20:15:08.62",4.1000000000000002E-2,0]
[39,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 220"," 20:15:08.77"," 20:15:08.89",0.11600000000000001,0.151]
[40,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:15:08.89"," 20:15:09.02",0.13,1E-3]
[41,"CMIGMCFXEU214600018","Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:15:09.05"," 20:15:09.13",8.2000000000000003E-2,0.03]
[42,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:15:09.13"," 20:15:09.17",4.3999999999999997E-2,0]
[43,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:09.17"," 20:15:09.21",3.2000000000000001E-2,0]
[44,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:15:09.21"," 20:15:09.25",0.04,0]
[45,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 345;361; 218"," 20:15:09.40"," 20:15:09.51",0.114,0.15]
[46,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:15:09.51"," 20:15:09.65",0.14299999999999999,0]
[47,"CMIGMCFXEU214600018","SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:15:09.68"," 20:15:09.76",8.1000000000000003E-2,3.1E-2]
[48,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:09.87"," 20:15:09.91",0.04,0.1]
[49,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:09.91"," 20:15:09.95",4.1000000000000002E-2,0]
[50,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:09.95"," 20:15:09.99",4.1000000000000002E-2,0]
[51,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:15:09.99"," 20:15:10.01",2.1000000000000001E-2,1E-3]
[52,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 116"," 20:15:10.11"," 20:15:10.22",0.113,0.1]
[53,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:15:10.22"," 20:15:10.24",0.02,1E-3]
[54,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 113"," 20:15:10.34"," 20:15:10.46",0.115,0.1]
[55,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 113"," 20:15:10.61"," 20:15:10.73",0.113,0.154]
[56,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:15:10.73"," 20:15:11.11",0.38500000000000001,0]
[57,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:11.14"," 20:15:11.18",0.04,0.03]
[58,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:15:11.23"," 20:15:11.26",3.1E-2,0.05]
[59,"CMIGMCFXEU214600018","对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:15:11.36"," 20:15:11.45",9.2999999999999999E-2,0.10100000000000001]
[60,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:15:11.66"," 20:15:11.77",0.113,0.2]
[61,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:11.77"," 20:15:11.82",5.3999999999999999E-2,1E-3]
[62,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:15:12.02"," 20:15:12.14",0.11600000000000001,0.20200000000000001]
[63,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)","OK00"," 20:15:12.14"," 20:15:12.19",0.05,1E-3]
[64,"CMIGMCFXEU214600018","网络参数查询..1","AA 06 BE 03 B9 DC","AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0"," 20:15:12.19"," 20:15:12.25",5.2999999999999999E-2,0,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[1,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:17.73"," 20:15:17.78",0.05,5.4859999999999998,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[2,"CMIGMCFXEU214600018","CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:15:17.83"," 20:15:17.88",0.05,5.0999999999999997E-2,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[3,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)",null," 20:15:17.88"," 20:15:18.03",0.15,0]
[4,"CMIGMCFXEU214600018","进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:15:18.23"," 20:15:18.26",3.1E-2,0.20100000000000001]
[5,"CMIGMCFXEU214600018","电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:15:18.56"," 20:15:18.62",5.0999999999999997E-2,0.30099999999999999]
[6,"CMIGMCFXEU214600018","条形码写入_22","AA 18 71 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 32 77","AB 05 0A DF 4E"," 20:15:18.62"," 20:15:21.02",2.4039999999999999,0]
[7,"CMIGMCFXEU214600018","HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:15:21.02"," 20:15:21.05",3.1E-2,1E-3]
[8,"CMIGMCFXEU214600018","HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:15:21.05"," 20:15:21.08",3.1E-2,1E-3]
[9,"CMIGMCFXEU214600018","白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:15:21.08"," 20:15:21.18",9.0999999999999998E-2,0]
[10,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:21.27"," 20:15:21.32",4.2999999999999997E-2,0.1]
[11,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:21.42"," 20:15:21.45",3.1E-2,0.10199999999999999]
[12,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:15:21.45"," 20:15:21.49",0.04,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[13,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:21.49"," 20:15:21.54",0.05,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[14,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:21.54"," 20:15:21.58",4.3999999999999997E-2,0]
[15,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:15:21.59"," 20:15:21.62",3.1E-2,1E-3]
[16,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:15:21.72"," 20:15:21.83",0.115,0.1]
[17,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:15:21.83"," 20:15:21.86",3.1E-2,1E-3]
[18,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:15:21.97"," 20:15:22.08",0.114,0.10299999999999999]
[19,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:15:22.08"," 20:15:22.18",0.10100000000000001,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[20,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:22.18"," 20:15:22.24",5.1999999999999998E-2,0]
[21,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:22.34"," 20:15:22.37",3.1E-2,0.10100000000000001]
[22,"CMIGMCFXEU214600018","普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:15:22.47"," 20:15:22.56",0.09,0.10100000000000001]
[23,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 199"," 20:15:22.66"," 20:15:22.77",0.11600000000000001,0.1]
[24,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:15:22.77"," 20:15:22.81",0.03,1E-3]
[25,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:15:22.81"," 20:15:22.85",0.04,0]
[26,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:15:22.85"," 20:15:22.89",0.05,0]
[27,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 199"," 20:15:23.15"," 20:15:23.26",0.113,0.252]
[28,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:15:23.26"," 20:15:23.40",0.14199999999999999,1E-3]
[29,"CMIGMCFXEU214600018","冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:15:23.43"," 20:15:23.51",8.1000000000000003E-2,3.1E-2]
[30,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:15:23.51"," 20:15:23.56",4.2000000000000003E-2,0]
[31,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:15:23.56"," 20:15:23.59",0.03,0]
[32,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:23.59"," 20:15:23.63",0.04,0]
[33,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 286;296; 167"," 20:15:23.78"," 20:15:23.89",0.115,0.151]
[34,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:15:23.89"," 20:15:24.04",0.14199999999999999,1E-3]
[35,"CMIGMCFXEU214600018","暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:15:24.07"," 20:15:24.15",8.1000000000000003E-2,0.03]
[36,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:24.15"," 20:15:24.19",4.2000000000000003E-2,0]
[37,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:24.19"," 20:15:24.23",0.04,0]
[38,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:24.23"," 20:15:24.27",4.2000000000000003E-2,0]
[39,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;327; 217"," 20:15:24.42"," 20:15:24.54",0.113,0.152]
[40,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:15:24.54"," 20:15:24.67",0.13100000000000001,1E-3]
[41,"CMIGMCFXEU214600018","Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:15:24.70"," 20:15:24.78",8.1000000000000003E-2,3.1E-2]
[42,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:15:24.78"," 20:15:24.82",0.04,0]
[43,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:24.82"," 20:15:24.86",4.1000000000000002E-2,0]
[44,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:15:24.86"," 20:15:24.91",5.0999999999999997E-2,0]
[45,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 345;361; 214"," 20:15:25.06"," 20:15:25.18",0.11600000000000001,0.152]
[46,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:15:25.18"," 20:15:25.32",0.14199999999999999,0]
[47,"CMIGMCFXEU214600018","SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:15:25.35"," 20:15:25.43",0.08,3.1E-2]
[48,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:25.53"," 20:15:25.57",4.1000000000000002E-2,0.1]
[49,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:25.57"," 20:15:25.61",3.2000000000000001E-2,0]
[50,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:25.61"," 20:15:25.65",0.04,0]
[51,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:15:25.65"," 20:15:25.68",3.1E-2,2E-3]
[52,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 112"," 20:15:25.79"," 20:15:25.91",0.115,0.112]
[53,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:15:25.91"," 20:15:25.94",0.03,0]
[54,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 115"," 20:15:26.04"," 20:15:26.15",0.114,0.1]
[55,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 115"," 20:15:26.30"," 20:15:26.42",0.114,0.152]
[56,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:15:26.42"," 20:15:26.80",0.38500000000000001,1E-3]
[57,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:26.83"," 20:15:26.88",5.0999999999999997E-2,0.03]
[58,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:15:26.93"," 20:15:26.97",3.1E-2,5.1999999999999998E-2]
[59,"CMIGMCFXEU214600018","对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:15:27.07"," 20:15:27.16",9.0999999999999998E-2,0.1]
[60,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:15:27.36"," 20:15:27.47",0.113,0.2]
[61,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:27.47"," 20:15:27.52",5.2999999999999999E-2,1E-3]
[62,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:15:27.73"," 20:15:27.84",0.114,0.20100000000000001]
[63,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)","OK00"," 20:15:27.84"," 20:15:27.89",0.05,3.0000000000000001E-3]
[64,"CMIGMCFXEU214600018","网络参数查询..1","AA 06 BE 03 B9 DC","AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0"," 20:15:27.89"," 20:15:27.94",5.2999999999999999E-2,0,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[1,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:33.43"," 20:15:33.48",0.05,5.4870000000000001,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[2,"CMIGMCFXEU214600018","CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:15:33.53"," 20:15:33.58",0.05,0.05,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[3,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)",null," 20:15:33.58"," 20:15:33.73",0.15,0]
[4,"CMIGMCFXEU214600018","进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:15:33.93"," 20:15:33.97",3.2000000000000001E-2,0.20100000000000001]
[5,"CMIGMCFXEU214600018","电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:15:34.27"," 20:15:34.32",5.0999999999999997E-2,0.30099999999999999]
[6,"CMIGMCFXEU214600018","条形码写入_22","AA 18 71 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 32 77","AB 05 0A DF 4E"," 20:15:34.32"," 20:15:36.72",2.4039999999999999,0]
[7,"CMIGMCFXEU214600018","HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:15:36.72"," 20:15:36.75",3.2000000000000001E-2,0]
[8,"CMIGMCFXEU214600018","HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:15:36.75"," 20:15:36.79",3.3000000000000002E-2,0]
[9,"CMIGMCFXEU214600018","白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:15:36.79"," 20:15:36.88",9.2999999999999999E-2,0]
[10,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:36.98"," 20:15:37.03",5.3999999999999999E-2,0.10100000000000001]
[11,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:37.13"," 20:15:37.17",3.1E-2,0.1]
[12,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:15:37.17"," 20:15:37.21",4.2000000000000003E-2,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[13,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:37.21"," 20:15:37.26",0.05,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[14,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:37.26"," 20:15:37.30",4.2999999999999997E-2,1E-3]
[15,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:15:37.30"," 20:15:37.33",3.2000000000000001E-2,0]
[16,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:15:37.43"," 20:15:37.55",0.113,0.10100000000000001]
[17,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:15:37.55"," 20:15:37.58",0.03,0]
[18,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:15:37.68"," 20:15:37.79",0.115,0.1]
[19,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:15:37.79"," 20:15:37.90",0.104,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[20,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:37.90"," 20:15:37.95",5.0999999999999997E-2,0]
[21,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:38.05"," 20:15:38.08",0.03,0.1]
[22,"CMIGMCFXEU214600018","普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:15:38.18"," 20:15:38.27",9.0999999999999998E-2,0.104]
[23,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 202"," 20:15:38.37"," 20:15:38.49",0.114,0.1]
[24,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:15:38.49"," 20:15:38.53",4.1000000000000002E-2,1E-3]
[25,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:15:38.53"," 20:15:38.58",0.05,0]
[26,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:15:38.58"," 20:15:38.63",0.05,0]
[27,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 202"," 20:15:38.88"," 20:15:39.00",0.113,0.252]
[28,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:15:39.00"," 20:15:39.14",0.14099999999999999,0]
[29,"CMIGMCFXEU214600018","冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:15:39.17"," 20:15:39.25",8.2000000000000003E-2,0.03]
[30,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:15:39.25"," 20:15:39.29",4.1000000000000002E-2,0]
[31,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:15:39.29"," 20:15:39.33",0.04,0]
[32,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:39.33"," 20:15:39.38",5.1999999999999998E-2,0]
[33,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 286;296; 170"," 20:15:39.53"," 20:15:39.65",0.115,0.152]
[34,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:15:39.65"," 20:15:39.78",0.13200000000000001,1E-3]
[35,"CMIGMCFXEU214600018","暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:15:39.81"," 20:15:39.89",8.3000000000000004E-2,3.1E-2]
[36,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:39.89"," 20:15:39.94",0.05,0]
[37,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:39.94"," 20:15:40.00",5.0999999999999997E-2,0]
[38,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:40.00"," 20:15:40.05",0.05,0]
[39,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:15:40.20"," 20:15:40.31",0.113,0.151]
[40,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:15:40.31"," 20:15:40.45",0.14099999999999999,1E-3]
[41,"CMIGMCFXEU214600018","Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:15:40.48"," 20:15:40.56",8.2000000000000003E-2,3.1E-2]
[42,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:15:40.56"," 20:15:40.61",4.2000000000000003E-2,0]
[43,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:40.61"," 20:15:40.64",0.03,0]
[44,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:15:40.64"," 20:15:40.68",0.04,0]
[45,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 345;360; 218"," 20:15:40.83"," 20:15:40.94",0.113,0.151]
[46,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:15:40.94"," 20:15:41.08",0.14299999999999999,0]
[47,"CMIGMCFXEU214600018","SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:15:41.12"," 20:15:41.20",8.1000000000000003E-2,3.1E-2]
[48,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:41.30"," 20:15:41.34",4.2000000000000003E-2,0.10100000000000001]
[49,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:41.34"," 20:15:41.38",0.04,0]
[50,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:41.38"," 20:15:41.43",0.05,0]
[51,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:15:41.43"," 20:15:41.47",0.04,0]
[52,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 116"," 20:15:41.57"," 20:15:41.68",0.113,0.10100000000000001]
[53,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:15:41.68"," 20:15:41.72",3.2000000000000001E-2,1E-3]
[54,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 113"," 20:15:41.82"," 20:15:41.93",0.114,0.1]
[55,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 113"," 20:15:42.08"," 20:15:42.20",0.115,0.151]
[56,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:15:42.20"," 20:15:42.59",0.39700000000000002,1E-3]
[57,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:42.62"," 20:15:42.67",4.1000000000000002E-2,0.03]
[58,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:15:42.72"," 20:15:42.75",3.1E-2,0.05]
[59,"CMIGMCFXEU214600018","对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:15:42.85"," 20:15:42.94",9.1999999999999998E-2,0.1]
[60,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:15:43.14"," 20:15:43.25",0.11600000000000001,0.2]
[61,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:43.25"," 20:15:43.31",5.1999999999999998E-2,1E-3]
[62,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:15:43.51"," 20:15:43.62",0.114,0.20100000000000001]
[63,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)","OK00"," 20:15:43.62"," 20:15:43.67",5.0999999999999997E-2,1E-3]
[64,"CMIGMCFXEU214600018","网络参数查询..1","AA 06 BE 03 B9 DC","AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0"," 20:15:43.67"," 20:15:43.73",5.1999999999999998E-2,0,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[1,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:49.21"," 20:15:49.26",0.05,5.4820000000000002,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[2,"CMIGMCFXEU214600018","CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:15:49.31"," 20:15:49.36",0.05,5.0999999999999997E-2,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[3,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)",null," 20:15:49.36"," 20:15:49.51",0.151,4.0000000000000001E-3]
[4,"CMIGMCFXEU214600018","进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:15:49.71"," 20:15:49.75",3.1E-2,0.2]
[5,"CMIGMCFXEU214600018","电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:15:50.06"," 20:15:50.11",0.05,0.311]
[6,"CMIGMCFXEU214600018","条形码写入_22","AA 18 71 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 32 77","AB 05 0A DF 4E"," 20:15:50.11"," 20:15:52.50",2.3919999999999999,0]
[7,"CMIGMCFXEU214600018","HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:15:52.50"," 20:15:52.54",0.04,0]
[8,"CMIGMCFXEU214600018","HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:15:52.54"," 20:15:52.57",3.1E-2,0]
[9,"CMIGMCFXEU214600018","白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:15:52.57"," 20:15:52.66",9.5000000000000001E-2,0]
[10,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:52.77"," 20:15:52.82",5.0999999999999997E-2,0.10199999999999999]
[11,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:52.92"," 20:15:52.95",0.03,0.1]
[12,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:15:52.95"," 20:15:52.99",4.1000000000000002E-2,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[13,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:15:52.99"," 20:15:53.04",0.05,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[14,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:53.04"," 20:15:53.09",0.05,0]
[15,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:15:53.09"," 20:15:53.12",0.03,0]
[16,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:15:53.22"," 20:15:53.33",0.113,0.10100000000000001]
[17,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:15:53.33"," 20:15:53.37",3.2000000000000001E-2,1E-3]
[18,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:15:53.47"," 20:15:53.58",0.114,0.1]
[19,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:15:53.58"," 20:15:53.68",0.104,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[20,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:53.68"," 20:15:53.74",5.0999999999999997E-2,0]
[21,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:15:53.83"," 20:15:53.87",3.2000000000000001E-2,0.1]
[22,"CMIGMCFXEU214600018","普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:15:53.97"," 20:15:54.06",9.1999999999999998E-2,0.10100000000000001]
[23,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 199"," 20:15:54.16"," 20:15:54.27",0.115,0.1]
[24,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:15:54.28"," 20:15:54.31",3.1E-2,1E-3]
[25,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:15:54.31"," 20:15:54.34",0.03,0]
[26,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:15:54.34"," 20:15:54.38",4.2000000000000003E-2,1E-3]
[27,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 199"," 20:15:54.63"," 20:15:54.75",0.115,0.25]
[28,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:15:54.75"," 20:15:54.89",0.14099999999999999,1E-3]
[29,"CMIGMCFXEU214600018","冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:15:54.92"," 20:15:55.00",8.1000000000000003E-2,0.03]
[30,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:15:55.00"," 20:15:55.04",0.04,0]
[31,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:15:55.04"," 20:15:55.08",0.04,0]
[32,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:55.08"," 20:15:55.12",4.2000000000000003E-2,0]
[33,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 286;296; 167"," 20:15:55.27"," 20:15:55.39",0.114,0.153]
[34,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:15:55.39"," 20:15:55.52",0.13200000000000001,1E-3]
[35,"CMIGMCFXEU214600018","暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:15:55.55"," 20:15:55.63",8.3000000000000004E-2,0.03]
[36,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:55.63"," 20:15:55.68",4.2000000000000003E-2,0]
[37,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:55.68"," 20:15:55.70",0.03,0]
[38,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:55.71"," 20:15:55.74",3.2000000000000001E-2,1E-3]
[39,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:15:55.89"," 20:15:56.00",0.113,0.151]
[40,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:15:56.00"," 20:15:56.13",0.13100000000000001,1E-3]
[41,"CMIGMCFXEU214600018","Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:15:56.17"," 20:15:56.25",8.1000000000000003E-2,3.2000000000000001E-2]
[42,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:15:56.25"," 20:15:56.30",0.05,0]
[43,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:56.30"," 20:15:56.34",0.04,1E-3]
[44,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:15:56.34"," 20:15:56.37",3.4000000000000002E-2,0]
[45,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 345;360; 214"," 20:15:56.52"," 20:15:56.63",0.113,0.15]
[46,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:15:56.64"," 20:15:56.77",0.13300000000000001,1E-3]
[47,"CMIGMCFXEU214600018","SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:15:56.80"," 20:15:56.88",8.2000000000000003E-2,3.2000000000000001E-2]
[48,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:15:56.98"," 20:15:57.02",0.04,0.10100000000000001]
[49,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:15:57.02"," 20:15:57.06",3.1E-2,0]
[50,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:15:57.06"," 20:15:57.10",4.1000000000000002E-2,0]
[51,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:15:57.10"," 20:15:57.13",3.2000000000000001E-2,0]
[52,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 112"," 20:15:57.23"," 20:15:57.34",0.114,0.1]
[53,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:15:57.34"," 20:15:57.36",2.1000000000000001E-2,1E-3]
[54,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 115"," 20:15:57.47"," 20:15:57.58",0.113,0.10100000000000001]
[55,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 115"," 20:15:57.73"," 20:15:57.84",0.114,0.151]
[56,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:15:57.84"," 20:15:58.25",0.40600000000000003,1E-3]
[57,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:58.28"," 20:15:58.34",6.0999999999999999E-2,0.03]
[58,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:15:58.39"," 20:15:58.41",0.02,5.1999999999999998E-2]
[59,"CMIGMCFXEU214600018","对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:15:58.52"," 20:15:58.61",9.8000000000000004E-2,0.10299999999999999]
[60,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:15:58.81"," 20:15:58.93",0.114,0.20100000000000001]
[61,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:15:58.93"," 20:15:58.99",6.0999999999999999E-2,0]
[62,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:15:59.19"," 20:15:59.31",0.114,0.20200000000000001]
[63,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)","OK00"," 20:15:59.31"," 20:15:59.36",0.05,0]
[64,"CMIGMCFXEU214600018","网络参数查询..1","AA 06 BE 03 B9 DC","AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0"," 20:15:59.36"," 20:15:59.41",0.05,0,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[1,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:16:04.91"," 20:16:04.96",0.05,5.5010000000000003,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[2,"CMIGMCFXEU214600018","CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:16:05.01"," 20:16:05.06",0.05,0.05,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]
[]
[3,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)",null," 20:16:05.06"," 20:16:05.21",0.15,0]
[4,"CMIGMCFXEU214600018","进工厂模式","AA 06 10 01 A7 EF","AB 05 0A DF 4E"," 20:16:05.41"," 20:16:05.43",2.1000000000000001E-2,0.2]
[5,"CMIGMCFXEU214600018","电视版本信息查询","AA 06 57 00 23 95","AB 05 0A DF 4E AB 17 58 56 38 2D 52 54 37 39 35 43 4D 2D 54 30 31 56 30 30 31 12 85"," 20:16:05.73"," 20:16:05.79",6.2E-2,0.3]
[6,"CMIGMCFXEU214600018","HDCP KEY检测","AA 06 87 00 36 B2","AB 05 0A DF 4E AB 06 88 01 40 19"," 20:16:05.79"," 20:16:05.82",3.1E-2,0]
[7,"CMIGMCFXEU214600018","HDCPKEY2.0检测","AA 06 E5 00 5B FA","AB 05 0A DF 4E AB 06 E6 01 68 3C"," 20:16:05.82"," 20:16:05.85",0.03,0]
[8,"CMIGMCFXEU214600018","白平衡调试条件设置","AA 06 16 01 0D 49","AB 05 0A DF 4E"," 20:16:05.85"," 20:16:05.94",9.0999999999999998E-2,0]
[9,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:16:06.04"," 20:16:06.08",4.1000000000000002E-2,0.1]
[10,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:16:06.18"," 20:16:06.21",0.03,0.10100000000000001]
[11,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 02 4B E9","AB 05 0A DF 4E"," 20:16:06.22"," 20:16:06.26",4.2000000000000003E-2,1E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[12,"CMIGMCFXEU214600018","CA410开启输出","COM，1(+回车)","OK00"," 20:16:06.26"," 20:16:06.31",0.05,0,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[13,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:16:06.31"," 20:16:06.36",0.05,0]
[14,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 30 2D DD","AB 05 0A DF 4E"," 20:16:06.36"," 20:16:06.38",0.02,0]
[15,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 217"," 20:16:06.48"," 20:16:06.59",0.113,0.1]
[16,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 31 3D FC","AB 05 0A DF 4E"," 20:16:06.59"," 20:16:06.61",2.1000000000000001E-2,1E-3]
[17,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:16:06.71"," 20:16:06.82",0.112,0.1]
[18,"CMIGMCFXEU214600018","0xFC07_背光保存","AA 08 FC 07 03 00 6B AB","AB 05 0A DF 4E"," 20:16:06.83"," 20:16:06.92",9.0999999999999998E-2,2E-3,"异常Log：单ACK读取OK，但有干扰字符。AB 05 0A DF 4E AB 05 0E 9F CA "]
[]
[19,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:16:06.92"," 20:16:06.97",5.0999999999999997E-2,0]
[20,"CMIGMCFXEU214600018","动态背光关闭","AA 06 39 00 0B B0","AB 05 0A DF 4E"," 20:16:07.07"," 20:16:07.10",3.2000000000000001E-2,0.10100000000000001]
[21,"CMIGMCFXEU214600018","普通色温状态","AA 06 31 01 92 38","AB 05 0A DF 4E"," 20:16:07.20"," 20:16:07.30",9.4E-2,0.1]
[22,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 202"," 20:16:07.39"," 20:16:07.51",0.113,0.1]
[23,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 73 F7 85","AB 05 0A DF 4E"," 20:16:07.51"," 20:16:07.54",3.1E-2,1E-3]
[24,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 74 B4 53","AB 05 0A DF 4E"," 20:16:07.54"," 20:16:07.57",3.1E-2,3.0000000000000001E-3]
[25,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 80 4E 9B","AB 05 0A DF 4E"," 20:16:07.57"," 20:16:07.60",0.03,0]
[26,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 300;317; 202"," 20:16:07.85"," 20:16:07.97",0.113,0.25]
[27,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 01 01 73 74 80 00 E4","AB 05 0A DF 4E"," 20:16:07.97"," 20:16:08.10",0.13100000000000001,1E-3]
[28,"CMIGMCFXEU214600018","冷色温状态","AA 06 31 02 A2 5B","AB 05 0A DF 4E"," 20:16:08.13"," 20:16:08.21",0.08,0.03]
[29,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 F7 26 89","AB 05 0A DF 4E"," 20:16:08.21"," 20:16:08.24",3.1E-2,0]
[30,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 F7 15 B8","AB 05 0A DF 4E"," 20:16:08.24"," 20:16:08.27",3.2000000000000001E-2,0]
[31,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:16:08.27"," 20:16:08.31",4.1000000000000002E-2,0]
[32,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 286;295; 170"," 20:16:08.46"," 20:16:08.58",0.114,0.15]
[33,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 02 01 F7 F7 00 D6 EF","AB 05 0A DF 4E"," 20:16:08.58"," 20:16:08.72",0.14299999999999999,1E-3]
[34,"CMIGMCFXEU214600018","暖色温状态","AA 06 31 03 B2 7A","AB 05 0A DF 4E"," 20:16:08.75"," 20:16:08.83",8.3000000000000004E-2,0.03]
[35,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:16:08.83"," 20:16:08.88",4.2000000000000003E-2,0]
[36,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:16:08.88"," 20:16:08.93",5.1999999999999998E-2,1E-3]
[37,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:16:08.93"," 20:16:08.98",5.0999999999999997E-2,0]
[38,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:16:09.13"," 20:16:09.24",0.112,0.15]
[39,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 03 01 07 04 00 D9 7E","AB 05 0A DF 4E"," 20:16:09.25"," 20:16:09.39",0.13200000000000001,1.2E-2]
[40,"CMIGMCFXEU214600018","Warm 5000k","AA 06 31 04 C2 9D","AB 05 0A DF 4E"," 20:16:09.42"," 20:16:09.49",7.3999999999999996E-2,3.2000000000000001E-2]
[41,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 0D 68 DC","AB 05 0A DF 4E"," 20:16:09.49"," 20:16:09.52",3.1E-2,0]
[42,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:16:09.52"," 20:16:09.55",3.1E-2,0]
[43,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 F0 30 0C","AB 05 0A DF 4E"," 20:16:09.55"," 20:16:09.60",4.1000000000000002E-2,0]
[44,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 345;360; 218"," 20:16:09.75"," 20:16:09.86",0.113,0.153]
[45,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 04 01 0D 04 F0 96 74","AB 05 0A DF 4E"," 20:16:09.86"," 20:16:10.00",0.14099999999999999,1E-3]
[46,"CMIGMCFXEU214600018","SRGB状态","AA 06 31 05 D2 BC","AB 05 0A DF 4E"," 20:16:10.03"," 20:16:10.12",8.2000000000000003E-2,0.03]
[47,"CMIGMCFXEU214600018","寄存器红驱动赋值..1","AA 06 40 07 C9 96","AB 05 0A DF 4E"," 20:16:10.22"," 20:16:10.26",4.2999999999999997E-2,0.1]
[48,"CMIGMCFXEU214600018","寄存器绿驱动赋值..1","AA 06 41 04 CA C4","AB 05 0A DF 4E"," 20:16:10.26"," 20:16:10.29",3.1E-2,0]
[49,"CMIGMCFXEU214600018","寄存器蓝驱动赋值..1","AA 06 42 00 DF 13","AB 05 0A DF 4E"," 20:16:10.29"," 20:16:10.32",3.3000000000000002E-2,0]
[50,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1B B8 D4","AB 05 0A DF 4E"," 20:16:10.32"," 20:16:10.34",2.1000000000000001E-2,1E-3]
[51,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 116"," 20:16:10.44"," 20:16:10.56",0.113,0.1]
[52,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 1A A8 F5","AB 05 0A DF 4E"," 20:16:10.56"," 20:16:10.58",2.1000000000000001E-2,1E-3]
[53,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 113"," 20:16:10.68"," 20:16:10.79",0.113,0.1]
[54,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 313;326; 114"," 20:16:10.94"," 20:16:11.06",0.114,0.151]
[55,"CMIGMCFXEU214600018","RGBgain或offset单独保存到NVM..6","AA 0B 4D 04 05 01 07 04 00 14 FB","AB 05 0A DF 4E"," 20:16:11.06"," 20:16:11.48",0.41699999999999998,1E-3]
[56,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:16:11.51"," 20:16:11.55",4.1000000000000002E-2,3.1E-2]
[57,"CMIGMCFXEU214600018","背光设置..1","AA 06 36 64 37 AC","AB 05 0A DF 4E"," 20:16:11.60"," 20:16:11.63",0.03,0.05]
[58,"CMIGMCFXEU214600018","对比度..1","AA 06 33 64 C8 59","AB 05 0A DF 4E"," 20:16:11.73"," 20:16:11.82",9.1999999999999998E-2,0.106]
[59,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 317;343; 376"," 20:16:12.02"," 20:16:12.14",0.114,0.2]
[60,"CMIGMCFXEU214600018","标准图像状态(STANDARD)","AA 06 30 01 A1 09","AB 05 0A DF 4E"," 20:16:12.14"," 20:16:12.18",4.2000000000000003E-2,1E-3]
[61,"CMIGMCFXEU214600018","CA410读取数据","MES(+回车)","OK00，P1 311;326; 220"," 20:16:12.38"," 20:16:12.50",0.113,0.20200000000000001]
[62,"CMIGMCFXEU214600018","CA410关闭输出","COM，0(+回车)","OK00"," 20:16:12.50"," 20:16:12.55",5.0999999999999997E-2,1E-3]
[63,"CMIGMCFXEU214600018","网络参数查询..1","AA 06 BE 03 B9 DC","AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0"," 20:16:12.55"," 20:16:12.61",6.0999999999999999E-2,0,"异常Log：两帧数据读取长度检验PASS。有干扰字符。AB 05 0A DF 4E AB 18 BF 03 43 4D 49 47 4D 43 46 58 45 55 32 31 34 36 30 30 30 31 38 C0 29 "]

{"sheet":"色温仪指令","index":1,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,0,2,0],[3,0,8,0],[9,0,11,0],[12,0,17,0]]}
["项目","命令名称","命令输入","命令返回","开始时间","结束时间","指令耗时","间隔时间"]
["色温仪通讯检测","CA210开启输出","COM，1(+回车)","OK00"," 20:12:28.30"," 20:12:28.35",0.05,1.0609999999999999,"43 4F 4D 2C 31 0D"]
[null,"CA210关闭输出","COM，0(+回车)","OK00"," 20:12:28.35"," 20:12:28.40",0.05,0,"43 4F 4D 2C 30 0D"]
["CA410调零","CA410开启输出","COM，1(+回车)","OK00"," 20:12:31.32"," 20:12:31.37",5.0999999999999997E-2,2.9140000000000001,"43 4F 4D 2C 31 0D"]
[null,"CA410显示模式(x，y，Lv)","MDS，0(+回车)","OK00"," 20:12:31.37"," 20:12:31.42",0.05,0,"4D 44 53 2C 30 0D"]
[null,"CA410同步模式(UNIV)","SCS，3(+回车)","OK00"," 20:12:31.42"," 20:12:31.47",0.05,0,"53 43 53 2C 33 0D"]
[null,"CA410测量速度(自动)","FSC，2(+回车)","OK00"," 20:12:31.47"," 20:12:31.52",5.0999999999999997E-2,0,"46 53 43 2C 32 0D"]
[null,"CA410零校准","ZRC(+回车)","OK00"," 20:12:31.52"," 20:12:35.39",3.8719999999999999,2E-3,"5A 52 43 0D"]
[null,"CA410关闭输出","COM，0(+回车)","OK00"," 20:12:41.42"," 20:12:41.47",5.0999999999999997E-2,6.0209999999999999,"43 4F 4D 2C 30 0D"]
["设定校准通道01","CA410开启输出","COM，1(+回车)","OK00"," 20:12:47.46"," 20:12:47.51",0.05,5.99,"43 4F 4D 2C 31 0D"]
[null,"CA410开启输出并锁定键控","MCH，01(+回车)","OK00"," 20:12:47.56"," 20:12:47.61",0.05,0.05,"4D 43 48 2C 30 31 0D"]
[null,"CA410关闭输出","COM，0(+回车)",null," 20:12:47.61"," 20:12:47.76",0.15,0,"43 4F 4D 2C 30 0D"]
["色温仪读数","CA410开启输出","COM，1(+回车)","OK00",null,null,0.05,5.99,"43 4F 4D 2C 31 0D"]
[null,"CA410开启输出并锁定键控","MCH，01(+回车)","OK00",null,null,0.05,0.05,"4D 43 48 2C 30 31 0D"]
[null,"CA410读取数据","MES(+回车)","OK00，P1 312;329; 221",null,null,0.113,0.1,"4D 45 53 0D"]
[null,"CA410读取数据","MES(+回车)","OK00，P1 312;329; 221",null,null,0.113,0.1]
[null,"......",null,"结果，P1 x,y,Lm"]
[null,"CA410关闭输出","COM，0(+回车)",null,null,null,0.15,0,"43 4F 4D 2C 30 0D"]

{"sheet":"AutoGamma调试流程","index":2,"n_rows":86,"n_cols":5,"rows_kept":86,"cut":false,"hidden":false,"merged":[[71,0,71,4],[76,0,76,4],[81,0,81,4],[1,0,1,4],[10,0,10,4],[50,0,50,4],[54,0,54,4],[58,0,58,4],[66,0,66,4]]}
["顺序","命令描述","命令","返回","说明"]
["调试gamma前期准备"]
[null,"进工厂 "]
[null,"读取条形码 "]
[null,"开启210 "]
[null,"白平衡初始化 ","AA 06 16 01 0D 49  ",null,"关闭动态背光，动态对比度，以及设置图像模式为电脑桌面 "]
[null,"关闭localdimming ","AA 07 9F 07 00 E1 74 "]
[null,"打开内置pattern ","AA 06 27 02 0B 8E  "]
[null,"切换到标准色温 ","AA 06 31 01 92 38 ",null,"打开内置pattern后，C1机器色温不在normal下 "]
[null,"gamma初始化 ","AA 07 9F 09 01 D2 5A ",null,"Gamma初始化：load linear gamma to bypass gamma affection，set RGB gain & offset to 128 "]
["切换13张pattern获取xyY"]
[null,"内置pattern灰度选择…3 ","AA 08 28 1A 1A 1A 02 FB ",null,"RGB分别为：0x1A 0x1A 0x1A "]
[null,"延时500ms "]
[null,"210读取数据 "]
[null,"内置pattern灰度选择…3 ","AA 08 28 33 33 33 13 99 "]
[]
[]
[null,null,"AA 08 28 4D 4D 4D 64 9F "]
[]
[]
[null,null,"AA 08 28 66 66 66 5D BD "]
[]
[]
[null,null,"AA 08 28 80 80 80 68 D0 "]
[]
[]
[null,null,"AA 08 28 99 99 99 8F D1 "]
[]
[]
[null,null,"AA 08 28 B3 B3 B3 A2 D3 "]
[]
[]
[null,null,"AA 08 28 CC CC CC C1 F5  "]
[]
[]
[null,null,"AA 08 28 E6 E6 E6 EC F7  "]
[]
[]
[null,null,"AA 08 28 FF FF FF 0B F6 "]
[]
[]
[null,null,"AA 08 28 0 FF 0 DA 65 "]
[]
[]
[null,null,"AA 08 28 0 0 FF C7 6A  "]
[]
[]
[null,null,"AA 08 28 FF 0 0 16 F9  "]
[]
[]
["采集数据结束，处理并生成gamm.ini文件"]
[null,"处理210采集到的数据 "]
[null,"根据dll生成gamma文件 "]
[null,"压缩gamma.ini文件为zip压缩包，并生成两位CRC16校验码 "]
["串口写gamma数据到TV"]
[null,"串口写zip压缩包文件至TV端 ","AA XX XX XX E9 02 XX XX… ",null,"XX表示数据取决于gamma.ini文件 "]
[null,"gamma文件抄写状态位检测 ","AA 06 EA 2 6B 86 "]
[null,"gamma文件 CRC16校验 ","AA 08 99 06 CRC1 CRC2 XX XX ",null,"检测TV和PC端的CRC校验是否一致，并立即生效gamma数据 "]
["gamma文件生效后，检验gamma数据是否符合要求"]
[null,"内置pattern灰度选择…3 ","AA 08 28 FF FF FF 0B F6  ",null,"RGB分别为：0xFF 0xFF 0xFF "]
[null,"延时500ms "]
[null,"210读取数据 ","Y255",null,"从210获取到的亮度Y255 "]
[null,"内置pattern灰度选择…3 ","AA 08 28 CC CC CC C1 F5  ",null,"RGB分别为：0xCC 0xCC 0xCC "]
[null,"延时500ms "]
[null,"210读取数据 ","Y204"]
[null,"计算gamma值 ","log(Y204/Y255)/log(204/255) ",null,"Y204：RGB为0xCC下的亮度；Y255：RGB为0xFF下的亮度 "]
["对比计算到的gamma是否在要求范围内 "]
[null,"内置pattern灰度选择…3 ","AA 08 28 99 99 99 8F D1 ",null,"RGB分别为：0x99 0x99 0x99 "]
[null,"延时500ms "]
[null,"210读取数据 ","Y153",null,"从210获取到的亮度Y153 "]
[null,"计算gamma值 ","log(Y153/Y255)/log(153/255) "]
["对比计算到的gamma是否在要求范围内 "]
[null,"内置pattern灰度选择…3 ","AA 08 28 66 66 66 5D BD  ",null,"RGB分别为：0x99 0x99 0x99 "]
[null,"延时500ms "]
[null,"210读取数据 ","Y102",null,"从210获取到的亮度Y102"]
[null,"计算gamma值 ","log(Y102/Y255)/log(102/255) "]
["对比计算到的gamma是否在要求范围内 "]
[null,"内置pattern灰度选择…3 ","AA 08 28 4D 4D 4D 64 9F ",null,"RGB分别为：0x4D 0x4D 0x4D "]
[null,"延时500ms "]
[null,"210读取数据 ","Y77",null,"从210获取到的亮度Y77"]
[null,"计算gamma值 ","log(Y102/Y255)/log(102/255) "]
["对比计算到的gamma是否在要求范围内 "]
[null,"关闭内置pattern ","AA 06 27 00 2B CC ",null,"RGB分别为：0x4D 0x4D 0x4D "]
[null,"关闭210 "]
[null,"保存gamma调试数据 "]
[null,"调试结束 "]