{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["变量结构详细列表","设备结构详细列表","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量结构详细列表","index":0,"n_rows":97,"n_cols":6,"rows_kept":97,"flags":["formulas_cached_only"]}
[null,"段名","客户端","是否序列化","数据库使用否","备注"]
[1,"变量ID","m_nVarID",1]
[2,"设备Uid","m_strVarUID",1]
[3,"变量名称","m_strName",1]
[4,"变量描述","m_strDesc",1]
[5,"变量类型ID","m_nVarTypeID",1]
[6,"变量数据长度","m_nDataLen",1]
[7,"请求寄存器个数","m_nRegNum",1]
[8,"功能码id","m_nFuncCode",1]
[9,"寄存器起始地址","m_nRegStartAddr",1]
[10,"命令","m_strRs232Cmd",1]
[11,"类型","m_strRs232Type",1]
[12,"索引","m_nRs232Index",1]
[13,"辨识时间","m_nIdentifyTime",1]
[14,"重新检测等待时间","m_nRedetectTime",1]
[15,"恢复正常是否触发远程报警","m_bIsNormalAlarm",1]
[16,"snmp对象oid","m_strSnmpOid",1]
[17,"SNMP域","m_strFields",1]
[18,"最大值","m_nMaxValues",1]
[19,"最小值","m_nMinValues",1]
[20,"最大转换比率","m_nMaxConvtRate",1]
[21,"最小转换比率","m_nMinConvtRate",1]
[22,"下限","m_nLowerLimit",1]
[23,"上限","m_nUpperLimit",1]
[24,"正常状态","m_nNormalState",1]
[25,"校正值","m_nRearm",1]
[26,"偏移值","m_nOffset",1]
[27,"单位","m_strUnit",1]
[28,"采集频率","m_nCollectFreq",1]
[29,"转换系数","m_fCoef",1]
[30,"告警级别","m_nWaringLevel",1]
[31,"读写权限","m_nPurview",1]
[32,"是否保存数值","m_bIsSave",1]
[33,"是否实时采集数据","m_bRealtimeFlag",1]
[34,"是否记录实时曲线","m_bRecCurve",1]
[35,"是否允许DDE访问","m_bIsDDE",1]
[36,"寄存器子ID","m_nVarChildID",1,null,"UnKnow"]
[37,"位信息ID","m_nVarItemID",1]
[38,"设备类型ID","m_nDevID",1]
[39,"开的描述","m_strOnDesc",1]
[40,"关的描述","m_strOffDesc",1]
[41,"设定值","m_strSetValue",1]
[42,"变量起始BIT位","m_nStartBit",1]
[43,"变量终止BIT位","m_nEndBit",1]
[44,"预留1_Str","m_strReserved1",1]
[45,"预留2_Str","m_strReserved2",1]
[46,"预留3_Str","m_strReserved3",1]
[47,"预留4_Str","m_strReserved4",1]
[48,"预留5_Str","m_strReserved5",1]
[49,"预留6_Str","m_strReserved6",1]
[50,"预留7_Str","m_strReserved7",1]
[51,"预留8_Str","m_strReserved8",1]
[52,"预留9_Str","m_strReserved9",1]
[53,"预留10_Str","m_strReserved10",1]
[54,"预留1_Int","m_nReserved1",1]
[55,"预留2_Int","m_nReserved2",1]
[56,"预留3_Int","m_nReserved3",1]
[57,"预留4_Int","m_nReserved4",1]
[58,"预留5_Int","m_nReserved5",1]
[59,"预留6_Int","m_nReserved6",1]
[60,"预留7_Int","m_nReserved7",1]
[61,"预留8_Int","m_nReserved8",1]
[62,"预留9_Int","m_nReserved9",1]
[63,"预留10_Int","m_nReserved10",1]
[64,"预留1_Bool","m_bReserved1",1]
[65,"预留2_Bool","m_bReserved2",1]
[66,"预留3_Bool","m_bReserved3",1]
[67,"预留4_Bool","m_bReserved4",1]
[68,"预留5_Bool","m_bReserved5",1]
[69,"预留6_Bool","m_bReserved6",1]
[70,"预留7_Bool","m_bReserved7",1]
[71,"预留8_Bool","m_bReserved8",1]
[72,"预留9_Bool","m_bReserved9",1]
[73,"预留10_Bool","m_bReserved10",1]
[74,"变量状态个数","m_nStatusListNum",1]
[75,"变量状态ID","m_listStatusID",1]
[76,"变量状态描述","m_listStatusDesc",1]
[]
[77,"关联Web页面","m_strRelatePage",1,null,"UnKnow"]
[null,"报警内容","m_strContent",0]
[null,"状态维持次数","m_nReadNum",0]
[null,"是否有时间计划","m_bExistDatePlan",0]
[null,"辨识Tick","m_dwIdentityTick",0,null,"UnKnow"]
[null,"回复正常辨识Tick","m_dwReturnNormalIdentityTick",0,null,"UnKnow"]
[]
[null,"存盘否(用于变量修改或创建?)","m_bSave",1,null,"UnKnow"]
[null,"当前运行值","m_fData",1,null,"变量当前采集到的值"]
[null,"月","m_nMonth",1,null,"UnKnow"]
[null,"日","m_nDay",1,null,"UnKnow"]
[null,"最小和?","m_nMinCount",1,null,"UnKnow"]
[null,"日最大","m_fDayMax",1,null,"UnKnow"]
[null,"日平均","m_fDayAvg",1,null,"UnKnow"]
[null,"日最小","m_fDayMin",1,null,"UnKnow"]
[]
[null,"设备地址?寄存器地址?","addr",0,null,"UnKnow"]
[null,"确认操作??","bConfirm",0,null,"UnKnow"]
[null,"分钟","m_nMinutes",0,null,"UnKnow"]

{"sheet":"设备结构详细列表","index":1,"n_rows":79,"n_cols":6,"rows_kept":79,"flags":["formulas_cached_only"]}
[null," 段名 ","客户端"," 是否序列化 "," 数据库使用否 ","   备注   "]
[1,"设备UID","m_strUID",1]
[2,"该设备类型","m_strType",1]
[3,"该设备名称","m_strName",1]
[4,"驱动Dll名称","m_strProtocolName",1]
[5,"是否投入使用标志","m_bUsed",1]
[6,"站号","m_Address",1,null,"UnKnow"]
[7,"协议类型","m_nProtocolType",1]
[8,"是否为采集模块","m_nIsCollectDev",1]
[9,"通讯超时","m_nTimeout",1]
[10,"设备驱动名称","m_strDevDriveName",1]
[11,"设备厂家名称","m_strDevFactoryName",1]
[12,"设备IP","m_strDevIP",1]
[13,"网络通信端口","m_nNetPort",1]
[14,"配置文件名称","m_strIniName",1]
[15,"预留1_Str","m_strReserved1",1]
[16,"预留2_Str","m_strReserved2",1]
[17,"预留3_Str","m_strReserved3",1]
[18,"预留4_Str","m_strReserved4",1]
[19,"预留5_Str","m_strReserved5",1]
[20,"预留6_Str","m_strReserved6",1]
[21,"预留7_Str","m_strReserved7",1]
[22,"预留8_Str","m_strReserved8",1]
[23,"预留9_Str","m_strReserved9",1]
[24,"预留10_Str","m_strReserved10",1]
[25,"预留1_Int","m_nReserved1",1]
[26,"预留2_Int","m_nReserved2",1]
[27,"预留3_Int","m_nReserved3",1]
[28,"预留4_Int","m_nReserved4",1]
[29,"预留5_Int","m_nReserved5",1]
[30,"预留6_Int","m_nReserved6",1]
[31,"预留7_Int","m_nReserved7",1]
[32,"预留8_Int","m_nReserved8",1]
[33,"预留9_Int","m_nReserved9",1]
[34,"预留10_Int","m_nReserved10",1]
[35,"预留1_Bool","m_bReserved1",1]
[36,"预留2_Bool","m_bReserved2",1]
[37,"预留3_Bool","m_bReserved3",1]
[38,"预留4_Bool","m_bReserved4",1]
[39,"预留5_Bool","m_bReserved5",1]
[40,"预留6_Bool","m_bReserved6",1]
[41,"预留7_Bool","m_bReserved7",1]
[42,"预留8_Bool","m_bReserved8",1]
[43,"预留9_Bool","m_bReserved9",1]
[44,"预留10_Bool","m_bReserved10",1]
[45]
[46,"是否有控制命令","m_bHasAction",0,null,"UnKnow"]
[47]
[48]
[49]
[50,"通信类型 0:串口  1:网络","m_nCommunicateType",1]
[51,"通信口名称","m_strName",1]
[52,"当前工作的设备号","m_nCurDeviceNo",0,null,"一个串口下有多个地址设备"]
[53,"串口或端口名","m_strPort",0]
[54,"串口地址","m_nAddr",0]
[55,"串口波特率","m_nBaudRate",0]
[56,"串口数据位","m_nByteSize",0]
[57,"串口校验位","m_nParity",0]
[58,"串口停止位","m_nStopBits",0]
[59,"?","m_bDTRDSR",0,null,"UnKnow"]
[60,"?","m_bRTSCTS",0,null,"UnKnow"]
[61,"?","m_bXONXOFF",0,null,"UnKnow"]
[62]
[63]
[64]
[65]
[66]
[67]
[68]
[69]
[70]
[71]
[72]
[73]
[74]
[75]
[76]
[]
[77]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}