{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":58,"n_cols":76,"rows_kept":58,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","4.17.33.1","CMS_1_UInRphaseV","市电输入R相电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","4.17.33.1","CMS_1_UInSphaseV","市电输入S相电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","4.17.33.1","CMS_1_UInTphaseV","市电输入T相电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","4.17.33.1","CMS_1_IOutRphaseV","逆变输出R相电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","4.17.33.1","CMS_1_IOutSphaseV","逆变输出S相电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","4.17.33.1","CMS_1_IOutTphaseV","逆变输出T相电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","4.17.33.1","CMS_1_BInRphaseV","旁路输入R相电压","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","4.17.33.1","CMS_1_BInSphaseV","旁路输入S相电压","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","4.17.33.1","CMS_1_BInTphaseV","旁路输入T相电压","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["10","4.17.33.1","CMS_1_SOutRCurr","系统R相输出电流","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["11","4.17.33.1","CMS_1_SOutSCurr","系统S相输出电流","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["12","4.17.33.1","CMS_1_SOutTCurr","系统T相输出电流","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["13","4.17.33.1","CMS_1_SOutRPower","系统输出R相视在功率","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","W","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["14","4.17.33.1","CMS_1_SOutSPower","系统输出S相视在功率","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","W","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["15","4.17.33.1","CMS_1_SOutTPower","系统输出T相视在功率","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","W","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["16","4.17.33.1","CMS_1_Bat1Vol","1号电池组电压值","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["17","4.17.33.1","CMS_1_Bat2Vol","2号电池组电压值","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["18","4.17.33.1","CMS_1_Bat1Curr","1号电池组电流值","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["19","4.17.33.1","CMS_1_Bat2Curr","2号电池组电流值","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["20","4.17.33.1","CMS_1_IOutFrequency","逆变输出频率","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["21","4.17.33.1","CMS_1_CurOnLineModule","当前在线模块数量","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","9","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["22","4.17.33.1","CMS_1_SysMaxModule","系统设置最大模块数量","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","9","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["23","4.17.33.1","CMS_1_PhaseAOwePre","A相欠压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["24","4.17.33.1","CMS_1_PhaseAOverPre","A相过压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["25","4.17.33.1","CMS_1_PhaseBOwePre","B相欠压","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["26","4.17.33.1","CMS_1_PhaseBOverPre","B相过压","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["27","4.17.33.1","CMS_1_PhaseCOwePre","C相欠压","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["28","4.17.33.1","CMS_1_PhaseCOverPre","C相过压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["29","4.17.33.1","CMS_1_ByInAlarm","旁路输入异常报警状态","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["30","4.17.33.1","CMS_1_InOutAlarm","逆变输出异常报警状态","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["31","4.17.33.1","CMS_1_PositiveV","正极欠压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["32","4.17.33.1","CMS_1_PositiveVShutD","正极欠压关机","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["33","4.17.33.1","CMS_1_PositivePres","正极过压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["34","4.17.33.1","CMS_1_NegativeOwePres","负极欠压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["35","4.17.33.1","CMS_1_NegativeOwePresShutD","负极欠压关机","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["36","4.17.33.1","CMS_1_NegativePres","负极过压","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["37","4.17.33.1","CMS_1_PhNShutD","正极高于负极关机","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["38","4.17.33.1","CMS_1_NhPShutD","负极高于正极关机","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["39","4.17.33.1","CMS_1_PhaseAOver","A相过载","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["40","4.17.33.1","CMS_1_PhaseBOver","B相过载","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["41","4.17.33.1","CMS_1_PhaseCOver","C相过载","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["42","4.17.33.1","CMS_1_PhaseAVoltCutByp","A相欠压切旁路","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["43","4.17.33.1","CMS_1_PhaseBVoltCutByp","B相欠压切旁路","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["44","4.17.33.1","CMS_1_PhaseCVoltCutByp","C相欠压切旁路","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["45","4.17.33.1","CMS_1_PhaseAOverVoltCutByp","A相过压切旁路","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["46","4.17.33.1","CMS_1_PhaseBOverVoltCutByp","B相过压切旁路","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["47","4.17.33.1","CMS_1_PhaseCOverVoltCutByp","C相过压切旁路","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["48","4.17.33.1","CMS_1_ManualByp","手动旁路","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["49","4.17.33.1","CMS_1_DcPosiOwePreShutD","直流正极欠压关机","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["50","4.17.33.1","CMS_1_DcPosiPreShutD","直流正极过压关机","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["51","4.17.33.1","CMS_1_DcNegOwePreShutD","直流负极欠压关机","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["52","4.17.33.1","CMS_1_DcNegPreShutD","直流负极过压关机","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["53","4.17.33.1","CMS_1_DcPhNShutD","直流正极大于负极关机","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["54","4.17.33.1","CMS_1_DcNhPShutD","直流负极大于正极关机","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["55","4.17.33.1","CMS_1_EPOShutD","EPO关机","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["56","4.17.33.1","CMS_1_ManualShutD","手动关机","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","1","1,","报警,"]
["34","4.17.33.1","CMS_1_Communications","先控UPS通信状态","1000","0","0","1","0",null,null,"0","60","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","Alarm,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":57,"n_cols":76,"rows_kept":57,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","5.32.131.1","CMS_1_UInRphaseV","市电输入R相电压","1","0","0","1","0","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["2","5.32.131.1","CMS_1_UInSphaseV","市电输入S相电压","1","0","0","1","0","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["3","5.32.131.1","CMS_1_UInTphaseV","市电输入T相电压","1","0","0","1","0","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["4","5.32.131.1","CMS_1_IOutRphaseV","逆变输出R相电压","1","0","0","1","0","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["5","5.32.131.1","CMS_1_IOutSphaseV","逆变输出S相电压","1","0","0","1","0","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["6","5.32.131.1","CMS_1_IOutTphaseV","逆变输出T相电压","1","0","0","1","0","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["7","5.32.131.1","CMS_1_BInRphaseV","旁路输入R相电压","1","0","0","1","0","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["8","5.32.131.1","CMS_1_BInSphaseV","旁路输入S相电压","1","0","0","1","0","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["9","5.32.131.1","CMS_1_BInTphaseV","旁路输入T相电压","1","0","0","1","0","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["10","5.32.131.1","CMS_1_SOutRCurr","系统R相输出电流","1","0","0","1","0","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["11","5.32.131.1","CMS_1_SOutSCurr","系统S相输出电流","1","0","0","1","0","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["12","5.32.131.1","CMS_1_SOutTCurr","系统T相输出电流","1","0","0","1","0","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["13","5.32.131.1","CMS_1_SOutRPower","系统输出R相视在功率","1","0","0","1","0","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","W","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["14","5.32.131.1","CMS_1_SOutSPower","系统输出S相视在功率","1","0","0","1","0","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","W","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["15","5.32.131.1","CMS_1_SOutTPower","系统输出T相视在功率","1","0","0","1","0","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","W","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["16","5.32.131.1","CMS_1_Bat1Vol","1号电池组电压值","1","0","0","1","0","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["17","5.32.131.1","CMS_1_Bat2Vol","2号电池组电压值","1","0","0","1","0","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","V","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["18","5.32.131.1","CMS_1_Bat1Curr","1号电池组电流值","1","0","0","1","0","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["19","5.32.131.1","CMS_1_Bat2Curr","2号电池组电流值","1","0","0","1","0","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","A","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["20","5.32.131.1","CMS_1_IOutFrequency","逆变输出频率","1","0","0","1","0","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","Hz","300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","999","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["21","5.32.131.1","CMS_1_CurOnLineModule","当前在线模块数量","1","0","0","1","0","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","9","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["22","5.32.131.1","CMS_1_SysMaxModule","系统设置最大模块数量","1","0","0","1","0","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","9","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["23","5.32.131.1","CMS_1_PhaseAOwePre","A相欠压","1","0","0","1","0","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["24","5.32.131.1","CMS_1_PhaseAOverPre","A相过压","1","0","0","1","0","cmd-24","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["25","5.32.131.1","CMS_1_PhaseBOwePre","B相欠压","1","0","0","1","0","cmd-25","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["26","5.32.131.1","CMS_1_PhaseBOverPre","B相过压","1","0","0","1","0","cmd-26","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["27","5.32.131.1","CMS_1_PhaseCOwePre","C相欠压","1","0","0","1","0","cmd-27","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["28","5.32.131.1","CMS_1_PhaseCOverPre","C相过压","1","0","0","1","0","cmd-28","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["29","5.32.131.1","CMS_1_ByInAlarm","旁路输入异常报警状态","1","0","0","1","0","cmd-29","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["30","5.32.131.1","CMS_1_InOutAlarm","逆变输出异常报警状态","1","0","0","1","0","cmd-30","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["31","5.32.131.1","CMS_1_PositiveV","正极欠压","1","0","0","1","0","cmd-31","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["32","5.32.131.1","CMS_1_PositiveVShutD","正极欠压关机","1","0","0","1","0","cmd-32","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["33","5.32.131.1","CMS_1_PositivePres","正极过压","1","0","0","1","0","cmd-33","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["34","5.32.131.1","CMS_1_NegativeOwePres","负极欠压","1","0","0","1","0","cmd-34","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["35","5.32.131.1","CMS_1_NegativeOwePresShutD","负极欠压关机","1","0","0","1","0","cmd-35","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["36","5.32.131.1","CMS_1_NegativePres","负极过压","1","0","0","1","0","cmd-36","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["37","5.32.131.1","CMS_1_PhNShutD","正极高于负极关机","1","0","0","1","0","cmd-37","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["38","5.32.131.1","CMS_1_NhPShutD","负极高于正极关机","1","0","0","1","0","cmd-38","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["39","5.32.131.1","CMS_1_PhaseAOver","A相过载","1","0","0","1","0","cmd-39","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["40","5.32.131.1","CMS_1_PhaseBOver","B相过载","1","0","0","1","0","cmd-40","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["41","5.32.131.1","CMS_1_PhaseCOver","C相过载","1","0","0","1","0","cmd-41","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["42","5.32.131.1","CMS_1_PhaseAVoltCutByp","A相欠压切旁路","1","0","0","1","0","cmd-42","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["43","5.32.131.1","CMS_1_PhaseBVoltCutByp","B相欠压切旁路","1","0","0","1","0","cmd-43","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["44","5.32.131.1","CMS_1_PhaseCVoltCutByp","C相欠压切旁路","1","0","0","1","0","cmd-44","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["45","5.32.131.1","CMS_1_PhaseAOverVoltCutByp","A相过压切旁路","1","0","0","1","0","cmd-45","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["46","5.32.131.1","CMS_1_PhaseBOverVoltCutByp","B相过压切旁路","1","0","0","1","0","cmd-46","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["47","5.32.131.1","CMS_1_PhaseCOverVoltCutByp","C相过压切旁路","1","0","0","1","0","cmd-47","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["48","5.32.131.1","CMS_1_ManualByp","手动旁路","1","0","0","1","0","cmd-48","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["49","5.32.131.1","CMS_1_DcPosiOwePreShutD","直流正极欠压关机","1","0","0","1","0","cmd-49","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["50","5.32.131.1","CMS_1_DcPosiPreShutD","直流正极过压关机","1","0","0","1","0","cmd-50","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["51","5.32.131.1","CMS_1_DcNegOwePreShutD","直流负极欠压关机","1","0","0","1","0","cmd-51","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["52","5.32.131.1","CMS_1_DcNegPreShutD","直流负极过压关机","1","0","0","1","0","cmd-52","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["53","5.32.131.1","CMS_1_DcPhNShutD","直流正极大于负极关机","1","0","0","1","0","cmd-53","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["54","5.32.131.1","CMS_1_DcNhPShutD","直流负极大于正极关机","1","0","0","1","0","cmd-54","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["55","5.32.131.1","CMS_1_EPOShutD","EPO关机","1","0","0","1","0","cmd-55","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]
["56","5.32.131.1","CMS_1_ManualShutD","手动关机","1","0","0","1","0","cmd-56","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","131",null,null,"0","0","0",{"$nulls":10},"30","1","2","0","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0"]