{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["变量dat文件","CSpreadSheetBackup"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":5,"n_cols":76,"rows_kept":5,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["11","7.33.154.1","FG_ALS_1_Line_Leak","漏水","4","2","1","3","2",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","154",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["12","7.33.154.1","FG_ALS_1_Line_CableCut","断线","4","2","1","3","4",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","154",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["13","7.33.154.1","FG_ALS_1_Line_LeakPos","漏水位置","4","2","1","3","6",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","154",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["1","7.33.154.1","FG_ALS_Communications","漏水设备通信状态","1000","0","0","1","0","","","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","154",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断开,"]

{"sheet":"CSpreadSheetBackup","index":1,"n_rows":26,"n_cols":76,"rows_kept":26,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","5.29.128.1","AKCP_1_Temp","端口1温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","5.29.128.1","AKCP_1_Humidity","端口1湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","5.29.128.1","AKCP_2_Temp","端口2温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.1","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","5.29.128.1","AKCP_2_Humidity","端口2湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.1","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["1","5.29.128.1","AKCP_3_Temp","端口3温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.2","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","5.29.128.1","AKCP_3_Humidity","端口3湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.2","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","5.29.128.1","AKCP_4_Temp","端口4温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.3","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","5.29.128.1","AKCP_4_Humidity","端口4湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.3","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["1","5.29.128.1","AKCP_5_Temp","端口5温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.4","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","5.29.128.1","AKCP_5_Humidity","端口5湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.4","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","5.29.128.1","AKCP_6_Temp","端口6温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.5","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","5.29.128.1","AKCP_6_Humidity","端口6湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.5","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["1","5.29.128.1","AKCP_7_Temp","端口7温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.6","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","5.29.128.1","AKCP_7_Humidity","端口7湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.6","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","5.29.128.1","AKCP_8_Temp","端口8温度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.16.1.3.7","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","5.29.128.1","AKCP_8_Humidity","端口8湿度","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.7","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","5.29.128.1","AKCP_1_3_Smoke1","烟感1","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.18.1.3.2","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["6","5.29.128.1","AKCP_1_4_Smoke2","烟感2","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.18.1.3.3","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["7","5.29.128.1","AKCP_1_5_Infrared1","红外1","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.18.1.3.4","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["8","5.29.128.1","AKCP_1_6_Infrared2","红外2","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.18.1.3.5","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["9","5.29.128.1","AKCP_1_7_Current","电流","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.17.1.3.6","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","5.29.128.1","AKCP_1_8_Reserre","保留","1","0","0","1","0",null,null,"0","30","60","1","1.3.6.1.4.1.3854.1.2.2.1.18.1.3.7","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","128",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","7.33.154.1","FG_ALS_1_Line_Leak","漏水","4","2","1","3","2",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","154",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["12","7.33.154.1","FG_ALS_1_Line_CableCut","断线","4","2","1","3","4",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","154",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","1","1,","报警,"]
["13","7.33.154.1","FG_ALS_1_Line_LeakPos","漏水位置","4","2","1","3","6",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","154",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]