{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":12,"n_cols":76,"rows_kept":12,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","5.34.134.1","IMS1002_1_1_Temp","IMS1002* 温度","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.3.0","public","0","0","0","0","10","30","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"20","0","100","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0","0","0","0"]
["2","5.34.134.1","IMS1002_1_2_Humidity","IMS1002* 湿度","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.4.0","public","0","0","0","0","10","90","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"60","0","100","0","0","0","0","0","0","0","1","1","0","0","0","0","0","0","0","0","0","0","0"]
["3","5.34.134.1","IMS1002_1_3_Leap","IMS1002* 漏水","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.5.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["4","5.34.134.1","IMS1002_1_4_Voltage","IMS1002* 电压","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.6.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["5","5.34.134.1","IMS1002_1_5_Current","IMS1002* 电流","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.7.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["6","5.34.134.1","IMS1002_1_6_Infrared","IMS1002* 空调房红外","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.8.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["7","5.34.134.1","IMS1002_1_7_Smoke","IMS1002* 空调房烟感","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.9.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["8","5.34.134.1","IMS1002_1_8_DryContact","IMS1002* 干接点","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.10.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["9","5.34.134.1","IMS1002_1_9_Built-inPower","IMS1002* 内置断电","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.39.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["10","5.34.134.1","IMS1002_1_10_Built-inBattery","IMS1002* 内置电池","1","0","0","0","0",null,null,"0","30","60","1","1.3.6.1.4.1.8338.1.1.3.1.6.1.1.42.40.0","public","0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","0","0","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","255","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["11","5.34.134.1","IMS1002_1_Netstutes","IMS1002* 通信","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","134",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]