{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":50,"n_cols":76,"rows_kept":50,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","6.7.88.1","stulz1ReturnTemp","1号空调回风温度","1","1","1","1","1","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"20","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","6.7.88.1","stulz1ReturnHumidity","1号空调回风湿度","1","1","1","1","1","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","0.1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"60","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","6.7.88.1","stulz1ReturnAirTempTooHigh","1号空调室内温度太高","1","1","1","1","1","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["4","6.7.88.1","stulz1ReturnAirHumidityTooHigh","1号空调室内湿度太高","1","1","1","1","1","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["5","6.7.88.1","stulz1ReturnAirTempTooLow","1号空调室内温度太低","1","1","1","1","1","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["6","6.7.88.1","stulz1ReturnAirHumidityTooLow","1号空调室内湿度太低","1","1","1","1","1","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["7","6.7.88.1","stulz1Mod1Reheat3","1号空调模块1加热器1","1","1","1","1","1","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","6.7.88.1","stulz1Mod1Compressor","1号空调模块1压缩机","1","1","1","1","1","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","6.7.88.1","stulz1Mod1Humidification","1号空调模块1加湿器","1","1","1","1","1","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","6.7.88.1","stulz1Mod1DeHumidification","1号空调模块1除湿器","1","1","1","1","1","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","6.7.88.1","stulz1Mod1Fan","1号空调模块1风机","1","1","1","1","1","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","6.7.88.1","stulz1Mod1DryCooler","1号空调模块1干冷机","1","1","1","1","1","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","6.7.88.1","stulz1Mod1Reheat3","1号空调模块1热风加热器/加热器3","1","1","1","1","1","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","6.7.88.1","stulz1Mod1Reheat2","1号空调模块1加热器2","1","1","1","1","1","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","6.7.88.1","stulz1Mod2Reheat1","1号空调模块2加热器1","1","1","1","1","1","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","6.7.88.1","stulz1Mod2Compressor","1号空调模块2压缩机","1","1","1","1","1","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","6.7.88.1","stulz1Mod2Humidification","1号空调模块2加湿器","1","1","1","1","1","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","6.7.88.1","stulz1Mod2DeHumidification","1号空调模块2除湿器","1","1","1","1","1","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","6.7.88.1","stulz1Mod2Fan","1号空调模块2风机","1","1","1","1","1","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","6.7.88.1","stulz1Mod2DryCooler","1号空调模块2干冷机","1","1","1","1","1","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","6.7.88.1","stulz1Mod2Reheat3","1号空调模块2热风加热器/加热器3","1","1","1","1","1","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","6.7.88.1","stulz1Mod2Reheat2","1号空调模块2加热器2","1","1","1","1","1","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","6.7.88.1","stulz1OnOff","1号空调开关机","1","1","1","1","1","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","1","0","0","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","6.7.88.1","stulz1_Netstatus","1号空调通信","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]
[]
["1","6.7.88.2","stulz2ReturnTemp","2号空调回风温度","1","1","1","1","1","cmd-1","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","℃","300","0.1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"20","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","6.7.88.2","stulz2ReturnHumidity","2号空调回风湿度","1","1","1","1","1","cmd-2","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0","%","300","0.1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"60","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","6.7.88.2","stulz2ReturnAirTempTooHigh","2号空调室内温度太高","1","1","1","1","1","cmd-3","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["4","6.7.88.2","stulz2ReturnAirHumidityTooHigh","2号空调室内湿度太高","1","1","1","1","1","cmd-4","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["5","6.7.88.2","stulz2ReturnAirTempTooLow","2号空调室内温度太低","1","1","1","1","1","cmd-5","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["6","6.7.88.2","stulz2ReturnAirHumidityTooLow","2号空调室内湿度太低","1","1","1","1","1","cmd-6","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","报警,"]
["7","6.7.88.2","stulz2Mod1Reheat3","2号空调模块1加热器1","1","1","1","1","1","cmd-7","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","6.7.88.2","stulz2Mod1Compressor","2号空调模块1压缩机","1","1","1","1","1","cmd-8","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","6.7.88.2","stulz2Mod1Humidification","2号空调模块1加湿器","1","1","1","1","1","cmd-9","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","6.7.88.2","stulz2Mod1DeHumidification","2号空调模块1除湿器","1","1","1","1","1","cmd-10","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","6.7.88.2","stulz2Mod1Fan","2号空调模块1风机","1","1","1","1","1","cmd-11","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","6.7.88.2","stulz2Mod1DryCooler","2号空调模块1干冷机","1","1","1","1","1","cmd-12","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","6.7.88.2","stulz2Mod1Reheat3","2号空调模块1热风加热器/加热器3","1","1","1","1","1","cmd-13","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","6.7.88.2","stulz2Mod1Reheat2","2号空调模块1加热器2","1","1","1","1","1","cmd-14","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","6.7.88.2","stulz2Mod2Reheat1","2号空调模块2加热器1","1","1","1","1","1","cmd-15","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","6.7.88.2","stulz2Mod2Compressor","2号空调模块2压缩机","1","1","1","1","1","cmd-16","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["17","6.7.88.2","stulz2Mod2Humidification","2号空调模块2加湿器","1","1","1","1","1","cmd-17","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["18","6.7.88.2","stulz2Mod2DeHumidification","2号空调模块2除湿器","1","1","1","1","1","cmd-18","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["19","6.7.88.2","stulz2Mod2Fan","2号空调模块2风机","1","1","1","1","1","cmd-19","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["20","6.7.88.2","stulz2Mod2DryCooler","2号空调模块2干冷机","1","1","1","1","1","cmd-20","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["21","6.7.88.2","stulz2Mod2Reheat3","2号空调模块2热风加热器/加热器3","1","1","1","1","1","cmd-21","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["22","6.7.88.2","stulz2Mod2Reheat2","2号空调模块2加热器2","1","1","1","1","1","cmd-22","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["23","6.7.88.2","stulz2OnOff","2号空调开关机","1","1","1","1","1","cmd-23","type-1","0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","1","0","0","0","0","0","0","88","关","开","0","0","0",{"$nulls":10},"0","0","100","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["24","6.7.88.2","stulz2_Netstatus","2号空调通信","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1","3","0","1","1","0","0","0","0","88",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]