{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["变量dat文件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"变量dat文件","index":0,"n_rows":34,"n_cols":76,"rows_kept":34,"flags":["formulas_cached_only"]}
["变量ID","设备Uid","变量名称","变量描述","变量类型ID","变量数据长度","请求寄存器个数","功能码id","寄存器起始地址","命令","类型","索引","辨识时间","重新检测等待时间","恢复正常是否触发远程报警","snmp对象oid","SNMP域","最大值","最小值","最大转换比率","最小转换比率","下限","上限","正常状态","校正值","偏移值","单位","采集频率","转换系数","告警级别","读写权限","是否保存数值","是否实时采集数据","是否记录实时曲线","是否允许DDE访问","寄存器子ID","位信息ID","设备类型ID","开的描述","关的描述","设定值","变量起始BIT位","变量终止BIT位","预留1_Str","预留2_Str","预留3_Str","预留4_Str","预留5_Str","预留6_Str","预留7_Str","预留8_Str","预留9_Str","预留10_Str","预留1_Int","预留2_Int","预留3_Int","预留4_Int","预留5_Int","预留6_Int","预留7_Int","预留8_Int","预留9_Int","预留10_Int","预留1_Bool","预留2_Bool","预留3_Bool","预留4_Bool","预留5_Bool","预留6_Bool","预留7_Bool","预留8_Bool","预留9_Bool","预留10_Bool","变量状态个数","变量状态ID","变量状态描述"]
["1","14.1.127.1","YMKK16_1_DO0_status","开关1状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","25","165","开","关","0","7","7",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","14.1.127.1","YMKK16_1_DO1_status","开关2状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","26","165","开","关","0","6","6",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","14.1.127.1","YMKK16_1_DO2_status","开关3状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","27","165","开","关","0","5","5",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","14.1.127.1","YMKK16_1_DO3_status","开关4状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","28","165","开","关","0","4","4",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","14.1.127.1","YMKK16_1_DO4_status","开关5状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","29","165","开","关","0","3","3",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","14.1.127.1","YMKK16_1_DO5_status","开关6状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","30","165","开","关","0","2","2",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","14.1.127.1","YMKK16_1_DO6_status","开关7状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","31","165","开","关","0","1","1",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","14.1.127.1","YMKK16_1_DO7_status","开关8状态","2","1","1","2","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","32","165","开","关","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","14.1.127.1","YMKK16_1_DO8_status","开关9状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","25","165","开","关","0","7","7",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","14.1.127.1","YMKK16_1_DO9_status","开关10状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","26","165","开","关","0","6","6",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","14.1.127.1","YMKK16_1_DOA_status","开关11状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","27","165","开","关","0","5","5",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","14.1.127.1","YMKK16_1_DOB_status","开关12状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","28","165","开","关","0","4","4",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","14.1.127.1","YMKK16_1_DOC_status","开关13状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","29","165","开","关","0","3","3",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","14.1.127.1","YMKK16_1_DOD_status","开关14状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","30","165","开","关","0","2","2",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","14.1.127.1","YMKK16_1_DOE_status","开关15状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","31","165","开","关","0","1","1",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","14.1.127.1","YMKK16_1_DOF_status","开关16状态","2","1","1","2","8",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","32","165","开","关","0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["1","14.1.127.1","YMKK16_1_SetDO0","设置开关1状态","2","1","1","5","0",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","17","165",null,null,"0","15","15",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["2","14.1.127.1","YMKK16_1_SetDO1","设置开关2状态","2","1","1","5","1",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","18","165",null,null,"0","14","14",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["3","14.1.127.1","YMKK16_1_SetDO2","设置开关3状态","2","1","1","5","2",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","19","165",null,null,"0","13","13",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["4","14.1.127.1","YMKK16_1_SetDO3","设置开关4状态","2","1","1","5","3",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","20","165",null,null,"0","12","12",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["5","14.1.127.1","YMKK16_1_SetDO4","设置开关5状态","2","1","1","5","4",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","21","165",null,null,"0","11","11",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["6","14.1.127.1","YMKK16_1_SetDO5","设置开关6状态","2","1","1","5","5",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","22","165",null,null,"0","10","10",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["7","14.1.127.1","YMKK16_1_SetDO6","设置开关7状态","2","1","1","5","6",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","23","165",null,null,"0","9","9",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["8","14.1.127.1","YMKK16_1_SetDO7","设置开关8状态","2","1","1","5","7",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","24","165",null,null,"0","8","8",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["9","14.1.127.1","YMKK16_1_SetDO8","设置开关9状态","2","1","1","5","8",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","25","165",null,null,"0","7","7",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["10","14.1.127.1","YMKK16_1_SetDO9","设置开关10状态","2","1","1","5","9",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","26","165",null,null,"0","6","6",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["11","14.1.127.1","YMKK16_1_SetDOA","设置开关11状态","2","1","1","5","10",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","27","165",null,null,"0","5","5",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["12","14.1.127.1","YMKK16_1_SetDOB","设置开关12状态","2","1","1","5","11",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","28","165",null,null,"0","4","4",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["13","14.1.127.1","YMKK16_1_SetDOC","设置开关13状态","2","1","1","5","12",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","29","165",null,null,"0","3","3",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["14","14.1.127.1","YMKK16_1_SetDOD","设置开关14状态","2","1","1","5","13",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","30","165",null,null,"0","2","2",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["15","14.1.127.1","YMKK16_1_SetDOE","设置开关15状态","2","1","1","5","14",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","31","165",null,null,"0","1","1",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["16","14.1.127.1","YMKK16_1_SetDOF","设置开关16状态","2","1","1","5","15",null,null,"0","30","60","0",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","1","1","1","0","0","0","32","165",null,null,"0","0","0",{"$nulls":10},"0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["33","14.1.127.1","YMKK16_1_status","配电开关状态检测通信","1000","0","0","1","0",null,null,"0","30","60","1",null,null,"0","0","0","0","0","0","0","0","0",null,"300","1.0000000000","3","0","1","1","0","0","0","0","165",null,null,"0","0","0",{"$nulls":10},"0","0","2","0","0","0","0","0","0","0","0","1","0","0","0","0","0","0","0","0","1","1,","断线报警,"]